# Vulkan® 1.4.304 - A Specification (with all registered extensions)

The Khronos® Vulkan Working Group
version 1.4.304, 2025-01-13 20:32:51Z
from git branch: Git branch not available commit: Git commit not available

Loading… please wait.

Search:

## 8. Render Pass

Draw commands must be recorded within a render pass instance. Each render pass instance defines a set of image resources, referred to as attachments, used during rendering.

To begin a render pass instance, call:

    // Provided by VK_VERSION_1_3
    void vkCmdBeginRendering(
        VkCommandBuffer                             commandBuffer,
        const VkRenderingInfo*                      pRenderingInfo);

or the equivalent command

    // Provided by VK_KHR_dynamic_rendering
    void vkCmdBeginRenderingKHR(
        VkCommandBuffer                             commandBuffer,
        const VkRenderingInfo*                      pRenderingInfo);

- `commandBuffer` is the command buffer in which to record the command.

- `pRenderingInfo` is a pointer to a VkRenderingInfo structure specifying details of the render pass instance to begin.

After beginning a render pass instance, the command buffer is ready to record draw commands.

If `pRenderingInfo->flags` includes `VK_RENDERING_RESUMING_BIT` then this render pass is resumed from a render pass instance that has been suspended earlier in submission order.

Valid Usage

- VUID-vkCmdBeginRendering-dynamicRendering-06446
  The `dynamicRendering` feature must be enabled

- VUID-vkCmdBeginRendering-commandBuffer-06068
  If `commandBuffer` is a secondary command buffer, and the `nestedCommandBuffer` feature is not enabled, `pRenderingInfo->flags` must not include `VK_RENDERING_CONTENTS_SECONDARY_COMMAND_BUFFERS_BIT`

- VUID-vkCmdBeginRendering-pRenderingInfo-09588
  If `pRenderingInfo->pDepthAttachment` is not `NULL` and `pRenderingInfo->pDepthAttachment->imageView` is not VK_NULL_HANDLE, `pRenderingInfo->pDepthAttachment->imageView` must be in the layout specified by `pRenderingInfo->pDepthAttachment->imageLayout`

- VUID-vkCmdBeginRendering-pRenderingInfo-09589
  If `pRenderingInfo->pDepthAttachment` is not `NULL`, `pRenderingInfo->pDepthAttachment->imageView` is not VK_NULL_HANDLE, `pRenderingInfo->pDepthAttachment->imageResolveMode` is not `VK_RESOLVE_MODE_NONE`, and `pRenderingInfo->pDepthAttachment->resolveImageView` is not VK_NULL_HANDLE, `pRenderingInfo->pDepthAttachment->resolveImageView` must be in the layout specified by `pRenderingInfo->pDepthAttachment->resolveImageLayout`

- VUID-vkCmdBeginRendering-pRenderingInfo-09590
  If `pRenderingInfo->pStencilAttachment` is not `NULL` and `pRenderingInfo->pStencilAttachment->imageView` is not VK_NULL_HANDLE, `pRenderingInfo->pStencilAttachment->imageView` must be in the layout specified by `pRenderingInfo->pStencilAttachment->imageLayout`

- VUID-vkCmdBeginRendering-pRenderingInfo-09591
  If `pRenderingInfo->pStencilAttachment` is not `NULL`, `pRenderingInfo->pStencilAttachment->imageView` is not VK_NULL_HANDLE, `pRenderingInfo->pStencilAttachment->imageResolveMode` is not `VK_RESOLVE_MODE_NONE`, and `pRenderingInfo->pStencilAttachment->resolveImageView` is not VK_NULL_HANDLE, `pRenderingInfo->pStencilAttachment->resolveImageView` must be in the layout specified by `pRenderingInfo->pStencilAttachment->resolveImageLayout`

- VUID-vkCmdBeginRendering-pRenderingInfo-09592
  For any element of `pRenderingInfo->pColorAttachments`, if `imageView` is not VK_NULL_HANDLE, that image view must be in the layout specified by `imageLayout`

- VUID-vkCmdBeginRendering-pRenderingInfo-09593
  For any element of `pRenderingInfo->pColorAttachments`, if either `imageResolveMode` is `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, or `imageView` is not VK_NULL_HANDLE and `resolveMode` is not `VK_RESOLVE_MODE_NONE`, and `resolveImageView` is not VK_NULL_HANDLE, `resolveImageView` must be in the layout specified by `resolveImageLayout`

Valid Usage (Implicit)

- VUID-vkCmdBeginRendering-commandBuffer-parameter
  `commandBuffer` must be a valid VkCommandBuffer handle

- VUID-vkCmdBeginRendering-pRenderingInfo-parameter
  `pRenderingInfo` must be a valid pointer to a valid VkRenderingInfo structure

- VUID-vkCmdBeginRendering-commandBuffer-recording
  `commandBuffer` must be in the recording state

- VUID-vkCmdBeginRendering-commandBuffer-cmdpool
  The `VkCommandPool` that `commandBuffer` was allocated from must support graphics operations

- VUID-vkCmdBeginRendering-renderpass
  This command must only be called outside of a render pass instance

- VUID-vkCmdBeginRendering-videocoding
  This command must only be called outside of a video coding scope

Host Synchronization

- Host access to `commandBuffer` must be externally synchronized

- Host access to the `VkCommandPool` that `commandBuffer` was allocated from must be externally synchronized

Command Properties

Command Buffer Levels | Render Pass Scope | Video Coding Scope | Supported Queue Types | Command Type
--- | --- | --- | --- | ---
Primary Secondary | Outside | Outside | Graphics | Action State

The `VkRenderingInfo` structure is defined as:

    // Provided by VK_VERSION_1_3
    typedef struct VkRenderingInfo {
        VkStructureType                     sType;
        const void*                         pNext;
        VkRenderingFlags                    flags;
        VkRect2D                            renderArea;
        uint32_t                            layerCount;
        uint32_t                            viewMask;
        uint32_t                            colorAttachmentCount;
        const VkRenderingAttachmentInfo*    pColorAttachments;
        const VkRenderingAttachmentInfo*    pDepthAttachment;
        const VkRenderingAttachmentInfo*    pStencilAttachment;
    } VkRenderingInfo;

or the equivalent

    // Provided by VK_KHR_dynamic_rendering, VK_QCOM_tile_properties with VK_KHR_dynamic_rendering or VK_VERSION_1_3
    typedef VkRenderingInfo VkRenderingInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `flags` is a bitmask of VkRenderingFlagBits.

- `renderArea` is the render area that is affected by the render pass instance.

- `layerCount` is the number of layers rendered to in each attachment when `viewMask` is `0`.

- `viewMask` is the view mask indicating the indices of attachment layers that will be rendered when it is not `0`.

- `colorAttachmentCount` is the number of elements in `pColorAttachments`.

- `pColorAttachments` is a pointer to an array of `colorAttachmentCount` VkRenderingAttachmentInfo structures describing any color attachments used.

- `pDepthAttachment` is a pointer to a VkRenderingAttachmentInfo structure describing a depth attachment.

- `pStencilAttachment` is a pointer to a VkRenderingAttachmentInfo structure describing a stencil attachment.

If `viewMask` is not `0`, multiview is enabled.

If there is an instance of VkDeviceGroupRenderPassBeginInfo included in the `pNext` chain and its `deviceRenderAreaCount` member is not `0`, then `renderArea` is ignored, and the render area is defined per-device by that structure.

If multiview is enabled, and the `multiviewPerViewRenderAreas` feature is enabled, and there is an instance of VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM included in the `pNext` chain with `perViewRenderAreaCount` not equal to `0`, then the elements of VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM::`pPerViewRenderAreas` override `renderArea` and define a render area for each view. In this case, `renderArea` must be an area at least as large as the union of all the per-view render areas.

Each element of the `pColorAttachments` array corresponds to an output location in the shader, i.e. if the shader declares an output variable decorated with a `Location` value of X, then it uses the attachment provided in `pColorAttachments`[X]. If the `imageView` member of any element of `pColorAttachments` is VK_NULL_HANDLE, and `resolveMode` is not `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, writes to the corresponding location by a fragment are discarded.

Valid Usage

- VUID-VkRenderingInfo-viewMask-06069
  If `viewMask` is `0`, `layerCount` must not be `0`

- VUID-VkRenderingInfo-multisampledRenderToSingleSampled-06857
  `imageView` members of `pDepthAttachment`, `pStencilAttachment`, and elements of `pColorAttachments` that are not VK_NULL_HANDLE must have been created with the same `sampleCount` , if none of the following are enabled:

  - The `VK_AMD_mixed_attachment_samples` extension

  - The `VK_NV_framebuffer_mixed_samples` extension

  - The `multisampledRenderToSingleSampled` feature,

- VUID-VkRenderingInfo-imageView-09429
  `imageView` members of elements of `pColorAttachments` that are not VK_NULL_HANDLE must have been created with the same `sampleCount` , if the `multisampledRenderToSingleSampled` feature is not enabled

- VUID-VkRenderingInfo-None-08994
  If VkDeviceGroupRenderPassBeginInfo::`deviceRenderAreaCount` is 0, `renderArea.extent.width` must be greater than 0

- VUID-VkRenderingInfo-None-08995
  If VkDeviceGroupRenderPassBeginInfo::`deviceRenderAreaCount` is 0, `renderArea.extent.height` must be greater than 0

- VUID-VkRenderingInfo-imageView-06858
  If multisampled-render-to-single-sampled is enabled, then all attachments referenced by `imageView` members of `pDepthAttachment`, `pStencilAttachment`, and elements of `pColorAttachments` that are not VK_NULL_HANDLE must have a sample count that is either `VK_SAMPLE_COUNT_1_BIT` or equal to VkMultisampledRenderToSingleSampledInfoEXT::`rasterizationSamples`

- VUID-VkRenderingInfo-imageView-06859
  If multisampled-render-to-single-sampled is enabled, then all attachments referenced by `imageView` members of `pDepthAttachment`, `pStencilAttachment`, and elements of `pColorAttachments` that are not VK_NULL_HANDLE and have a sample count of `VK_SAMPLE_COUNT_1_BIT` must have been created with `VK_IMAGE_CREATE_MULTISAMPLED_RENDER_TO_SINGLE_SAMPLED_BIT_EXT` in their VkImageCreateInfo::`flags`

- VUID-VkRenderingInfo-pNext-06077
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, `renderArea.offset.x` must be greater than or equal to 0

- VUID-VkRenderingInfo-pNext-06078
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, `renderArea.offset.y` must be greater than or equal to 0

- VUID-VkRenderingInfo-pNext-07815
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, the sum of `renderArea.extent.width` and `renderArea.offset.x` must be less than or equal to `maxFramebufferWidth`

- VUID-VkRenderingInfo-pNext-07816
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, the sum of `renderArea.extent.height` and `renderArea.offset.y` must be less than or equal to `maxFramebufferHeight`

- VUID-VkRenderingInfo-pNext-06079
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, the width of the `imageView` member of any element of `pColorAttachments`, `pDepthAttachment`, or `pStencilAttachment` that is not VK_NULL_HANDLE must be greater than or equal to `renderArea.offset.x` + `renderArea.extent.width`

- VUID-VkRenderingInfo-pNext-06080
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, the height of the `imageView` member of any element of `pColorAttachments`, `pDepthAttachment`, or `pStencilAttachment` that is not VK_NULL_HANDLE must be greater than or equal to `renderArea.offset.y` + `renderArea.extent.height`

- VUID-VkRenderingInfo-pNext-06083
  If the `pNext` chain contains VkDeviceGroupRenderPassBeginInfo, the width of the `imageView` member of any element of `pColorAttachments`, `pDepthAttachment`, or `pStencilAttachment` that is not VK_NULL_HANDLE must be greater than or equal to the sum of the `offset.x` and `extent.width` members of each element of `pDeviceRenderAreas`

- VUID-VkRenderingInfo-pNext-06084
  If the `pNext` chain contains VkDeviceGroupRenderPassBeginInfo, the height of the `imageView` member of any element of `pColorAttachments`, `pDepthAttachment`, or `pStencilAttachment` that is not VK_NULL_HANDLE must be greater than or equal to the sum of the `offset.y` and `extent.height` members of each element of `pDeviceRenderAreas`

- VUID-VkRenderingInfo-pDepthAttachment-06085
  If neither `pDepthAttachment` or `pStencilAttachment` are `NULL` and the `imageView` member of either structure is not VK_NULL_HANDLE, the `imageView` member of each structure must be the same

- VUID-VkRenderingInfo-pDepthAttachment-06086
  If neither `pDepthAttachment` or `pStencilAttachment` are `NULL`, and the `resolveMode` member of each is not `VK_RESOLVE_MODE_NONE`, the `resolveImageView` member of each structure must be the same

- VUID-VkRenderingInfo-colorAttachmentCount-06087
  If `colorAttachmentCount` is not `0` and the `imageView` member of an element of `pColorAttachments` is not VK_NULL_HANDLE, that `imageView` must have been created with `VK_IMAGE_USAGE_COLOR_ATTACHMENT_BIT`

- VUID-VkRenderingInfo-colorAttachmentCount-09476
  If `colorAttachmentCount` is not `0` and there is an element of `pColorAttachments` with either its `resolveMode` member set to `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, or its `imageView` member not VK_NULL_HANDLE, and its `resolveMode` member not set to `VK_RESOLVE_MODE_NONE`, the `resolveImageView` member of that element of `pColorAttachments` must have been created with `VK_IMAGE_USAGE_COLOR_ATTACHMENT_BIT`

- VUID-VkRenderingInfo-pDepthAttachment-06547
  If `pDepthAttachment` is not `NULL` and `pDepthAttachment->imageView` is not VK_NULL_HANDLE, `pDepthAttachment->imageView` must have been created with a format that includes a depth component

- VUID-VkRenderingInfo-pDepthAttachment-06088
  If `pDepthAttachment` is not `NULL` and `pDepthAttachment->imageView` is not VK_NULL_HANDLE, `pDepthAttachment->imageView` must have been created with `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkRenderingInfo-pDepthAttachment-09477
  If `pDepthAttachment` is not `NULL` and `pDepthAttachment->resolveMode` is not `VK_RESOLVE_MODE_NONE`, `pDepthAttachment->resolveImageView` must have been created with `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkRenderingInfo-pStencilAttachment-06548
  If `pStencilAttachment` is not `NULL` and `pStencilAttachment->imageView` is not VK_NULL_HANDLE, `pStencilAttachment->imageView` must have been created with a format that includes a stencil aspect

- VUID-VkRenderingInfo-pStencilAttachment-06089
  If `pStencilAttachment` is not `NULL` and `pStencilAttachment->imageView` is not VK_NULL_HANDLE, `pStencilAttachment->imageView` must have been created with a stencil usage including `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkRenderingInfo-pStencilAttachment-09478
  If `pStencilAttachment` is not `NULL` and `pStencilAttachment->resolveMode` is not `VK_RESOLVE_MODE_NONE`, `pStencilAttachment->resolveImageView` must have been created with `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkRenderingInfo-colorAttachmentCount-06090
  If `colorAttachmentCount` is not `0` and the `imageView` member of an element of `pColorAttachments` is not VK_NULL_HANDLE, the `layout` member of that element of `pColorAttachments` must not be `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderingInfo-colorAttachmentCount-06091
  If `colorAttachmentCount` is not `0` and the `imageView` member of an element of `pColorAttachments` is not VK_NULL_HANDLE, if the `resolveMode` member of that element of `pColorAttachments` is not `VK_RESOLVE_MODE_NONE`, its `resolveImageLayout` member must not be `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderingInfo-pDepthAttachment-06092
  If `pDepthAttachment` is not `NULL` and `pDepthAttachment->imageView` is not VK_NULL_HANDLE, `pDepthAttachment->layout` must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL`

- VUID-VkRenderingInfo-pDepthAttachment-06093
  If `pDepthAttachment` is not `NULL`, `pDepthAttachment->imageView` is not VK_NULL_HANDLE, and `pDepthAttachment->resolveMode` is not `VK_RESOLVE_MODE_NONE`, `pDepthAttachment->resolveImageLayout` must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL`

- VUID-VkRenderingInfo-pStencilAttachment-06094
  If `pStencilAttachment` is not `NULL` and `pStencilAttachment->imageView` is not VK_NULL_HANDLE, `pStencilAttachment->layout` must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL`

- VUID-VkRenderingInfo-pStencilAttachment-06095
  If `pStencilAttachment` is not `NULL`, `pStencilAttachment->imageView` is not VK_NULL_HANDLE, and `pStencilAttachment->resolveMode` is not `VK_RESOLVE_MODE_NONE`, `pStencilAttachment->resolveImageLayout` must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL`

- VUID-VkRenderingInfo-colorAttachmentCount-06096
  If `colorAttachmentCount` is not `0` and the `imageView` member of an element of `pColorAttachments` is not VK_NULL_HANDLE, the `layout` member of that element of `pColorAttachments` must not be `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderingInfo-colorAttachmentCount-06097
  If `colorAttachmentCount` is not `0` and the `imageView` member of an element of `pColorAttachments` is not VK_NULL_HANDLE, if the `resolveMode` member of that element of `pColorAttachments` is not `VK_RESOLVE_MODE_NONE`, its `resolveImageLayout` member must not be `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderingInfo-pDepthAttachment-06098
  If `pDepthAttachment` is not `NULL`, `pDepthAttachment->imageView` is not VK_NULL_HANDLE, and `pDepthAttachment->resolveMode` is not `VK_RESOLVE_MODE_NONE`, `pDepthAttachment->resolveImageLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkRenderingInfo-pStencilAttachment-06099
  If `pStencilAttachment` is not `NULL`, `pStencilAttachment->imageView` is not VK_NULL_HANDLE, and `pStencilAttachment->resolveMode` is not `VK_RESOLVE_MODE_NONE`, `pStencilAttachment->resolveImageLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderingInfo-colorAttachmentCount-06100
  If `colorAttachmentCount` is not `0` and the `imageView` member of an element of `pColorAttachments` is not VK_NULL_HANDLE, the `layout` member of that element of `pColorAttachments` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderingInfo-colorAttachmentCount-06101
  If `colorAttachmentCount` is not `0` and the `imageView` member of an element of `pColorAttachments` is not VK_NULL_HANDLE, if the `resolveMode` member of that element of `pColorAttachments` is not `VK_RESOLVE_MODE_NONE`, its `resolveImageLayout` member must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderingInfo-pDepthAttachment-07732
  If `pDepthAttachment` is not `NULL` and `pDepthAttachment->imageView` is not VK_NULL_HANDLE, `pDepthAttachment->layout` must not be `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderingInfo-pDepthAttachment-07733
  If `pDepthAttachment` is not `NULL`, `pDepthAttachment->imageView` is not VK_NULL_HANDLE, and `pDepthAttachment->resolveMode` is not `VK_RESOLVE_MODE_NONE`, `pDepthAttachment->resolveImageLayout` must not be `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderingInfo-pStencilAttachment-07734
  If `pStencilAttachment` is not `NULL` and `pStencilAttachment->imageView` is not VK_NULL_HANDLE, `pStencilAttachment->layout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`

- VUID-VkRenderingInfo-pStencilAttachment-07735
  If `pStencilAttachment` is not `NULL`, `pStencilAttachment->imageView` is not VK_NULL_HANDLE, and `pStencilAttachment->resolveMode` is not `VK_RESOLVE_MODE_NONE`, `pStencilAttachment->resolveImageLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`

- VUID-VkRenderingInfo-pDepthAttachment-06102
  If `pDepthAttachment` is not `NULL` and `pDepthAttachment->imageView` is not VK_NULL_HANDLE, `pDepthAttachment->resolveMode` must be one of the bits set in VkPhysicalDeviceDepthStencilResolveProperties::`supportedDepthResolveModes`

- VUID-VkRenderingInfo-pStencilAttachment-06103
  If `pStencilAttachment` is not `NULL` and `pStencilAttachment->imageView` is not VK_NULL_HANDLE, `pStencilAttachment->resolveMode` must be one of the bits set in VkPhysicalDeviceDepthStencilResolveProperties::`supportedStencilResolveModes`

- VUID-VkRenderingInfo-pDepthAttachment-06104
  If `pDepthAttachment` or `pStencilAttachment` are both not `NULL`, `pDepthAttachment->imageView` and `pStencilAttachment->imageView` are both not VK_NULL_HANDLE, and VkPhysicalDeviceDepthStencilResolveProperties::`independentResolveNone` is `VK_FALSE`, the `resolveMode` of both structures must be the same value

- VUID-VkRenderingInfo-pDepthAttachment-06105
  If `pDepthAttachment` or `pStencilAttachment` are both not `NULL`, `pDepthAttachment->imageView` and `pStencilAttachment->imageView` are both not VK_NULL_HANDLE, VkPhysicalDeviceDepthStencilResolveProperties::`independentResolve` is `VK_FALSE`, and the `resolveMode` of neither structure is `VK_RESOLVE_MODE_NONE`, the `resolveMode` of both structures must be the same value

- VUID-VkRenderingInfo-colorAttachmentCount-06106
  `colorAttachmentCount` must be less than or equal to VkPhysicalDeviceLimits::`maxColorAttachments`

- VUID-VkRenderingInfo-imageView-06107
  If the `imageView` member of a VkRenderingFragmentDensityMapAttachmentInfoEXT structure included in the `pNext` chain is not VK_NULL_HANDLE, and the `fragmentDensityMapNonSubsampledImages` feature is not enabled, valid `imageView` and `resolveImageView` members of `pDepthAttachment`, `pStencilAttachment`, and each element of `pColorAttachments` must be a VkImageView created with `VK_IMAGE_CREATE_SUBSAMPLED_BIT_EXT`

- VUID-VkRenderingInfo-imageView-06108
  If the `imageView` member of a VkRenderingFragmentDensityMapAttachmentInfoEXT structure included in the `pNext` chain is not VK_NULL_HANDLE, and `viewMask` is not `0`, `imageView` must have a `layerCount` greater than or equal to the index of the most significant bit in `viewMask`

- VUID-VkRenderingInfo-imageView-06109
  If the `imageView` member of a VkRenderingFragmentDensityMapAttachmentInfoEXT structure included in the `pNext` chain is not VK_NULL_HANDLE, and `viewMask` is `0`, `imageView` must have a `layerCount` equal to `1`

- VUID-VkRenderingInfo-pNext-06112
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0 and the `imageView` member of a VkRenderingFragmentDensityMapAttachmentInfoEXT structure included in the `pNext` chain is not VK_NULL_HANDLE, `imageView` must have a width greater than or equal to ⌈ma x F r a g m e n t De n s i t y T e x e lS i z e w i d t h​re n d er A re a x​+re n d er A re a w i d t h​​⌉

- VUID-VkRenderingInfo-pNext-06114
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0 and the `imageView` member of a VkRenderingFragmentDensityMapAttachmentInfoEXT structure included in the `pNext` chain is not VK_NULL_HANDLE, `imageView` must have a height greater than or equal to ⌈ma x F r a g m e n t De n s i t y T e x e lS i z e h e i g h t​re n d er A re a y​+re n d er A re a h e i g h t​​⌉

- VUID-VkRenderingInfo-pNext-06113
  If the `pNext` chain contains a VkDeviceGroupRenderPassBeginInfo structure, its `deviceRenderAreaCount` member is not 0, and the `imageView` member of a VkRenderingFragmentDensityMapAttachmentInfoEXT structure included in the `pNext` chain is not VK_NULL_HANDLE, `imageView` must have a width greater than or equal to ⌈ma x F r a g m e n t De n s i t y T e x e lS i z e w i d t h​p De v i ce R e n d er A re a s x​+p De v i ce R e n d er A re a s w i d t h​​⌉ for each element of `pDeviceRenderAreas`

- VUID-VkRenderingInfo-pNext-06115
  If the `pNext` chain contains a VkDeviceGroupRenderPassBeginInfo structure, its `deviceRenderAreaCount` member is not 0, and the `imageView` member of a VkRenderingFragmentDensityMapAttachmentInfoEXT structure included in the `pNext` chain is not VK_NULL_HANDLE, `imageView` must have a height greater than or equal to ⌈ma x F r a g m e n t De n s i t y T e x e lS i z e h e i g h t​p De v i ce R e n d er A re a s y​+p De v i ce R e n d er A re a s h e i g h t​​⌉ for each element of `pDeviceRenderAreas`

- VUID-VkRenderingInfo-imageView-06116
  If the `imageView` member of a VkRenderingFragmentDensityMapAttachmentInfoEXT structure included in the `pNext` chain is not VK_NULL_HANDLE, it must not be equal to the `imageView` or `resolveImageView` member of `pDepthAttachment`, `pStencilAttachment`, or any element of `pColorAttachments`

- VUID-VkRenderingInfo-pNext-06119
  If the `maintenance7` feature is not enabled or the `robustFragmentShadingRateAttachmentAccess` limit is `VK_FALSE` or the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure was created with VkImageSubresourceRange::`baseMipLevel` greater than 0, the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, and the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure included in the `pNext` chain is not VK_NULL_HANDLE, `imageView` must have a width greater than or equal to ⌈s ha d in g R a t e A tt a c hm e n tT e x e lS i z e w i d t h​re n d er A re a x​+re n d er A re a w i d t h​​⌉

- VUID-VkRenderingInfo-pNext-06121
  If the `maintenance7` feature is not enabled or the `robustFragmentShadingRateAttachmentAccess` limit is `VK_FALSE` or the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure was created with VkImageSubresourceRange::`baseMipLevel` greater than 0, the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0 and the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure included in the `pNext` chain is not VK_NULL_HANDLE, `imageView` must have a height greater than or equal to ⌈s ha d in g R a t e A tt a c hm e n tT e x e lS i z e h e i g h t​re n d er A re a y​+re n d er A re a h e i g h t​​⌉

- VUID-VkRenderingInfo-pNext-06120
  If the `maintenance7` feature is not enabled or the `robustFragmentShadingRateAttachmentAccess` limit is `VK_FALSE` or the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure was created with VkImageSubresourceRange::`baseMipLevel` greater than 0, the `pNext` chain contains a VkDeviceGroupRenderPassBeginInfo structure, its `deviceRenderAreaCount` member is not 0, and the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure included in the `pNext` chain is not VK_NULL_HANDLE, `imageView` must have a width greater than or equal to ⌈s ha d in g R a t e A tt a c hm e n tT e x e lS i z e w i d t h​p De v i ce R e n d er A re a s x​+p De v i ce R e n d er A re a s w i d t h​​⌉ for each element of `pDeviceRenderAreas`

- VUID-VkRenderingInfo-pNext-06122
  If the `maintenance7` feature is not enabled or the `robustFragmentShadingRateAttachmentAccess` limit is `VK_FALSE` or the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure was created with VkImageSubresourceRange::`baseMipLevel` greater than 0, the `pNext` chain contains a VkDeviceGroupRenderPassBeginInfo structure, its `deviceRenderAreaCount` member is not 0, and the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure included in the `pNext` chain is not VK_NULL_HANDLE, `imageView` must have a height greater than or equal to ⌈s ha d in g R a t e A tt a c hm e n tT e x e lS i z e h e i g h t​p De v i ce R e n d er A re a s y​+p De v i ce R e n d er A re a s h e i g h t​​⌉ for each element of `pDeviceRenderAreas`

- VUID-VkRenderingInfo-layerCount-07817
  `layerCount` must be less than or equal to `maxFramebufferLayers`

- VUID-VkRenderingInfo-imageView-06123
  If the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure included in the `pNext` chain is not VK_NULL_HANDLE, and `viewMask` is `0`, `imageView` must have a `layerCount` that is either equal to `1` or greater than or equal to `layerCount`

- VUID-VkRenderingInfo-imageView-06124
  If the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure included in the `pNext` chain is not VK_NULL_HANDLE, and `viewMask` is not `0`, `imageView` must have a `layerCount` that either equal to `1` or greater than or equal to the index of the most significant bit in `viewMask`

- VUID-VkRenderingInfo-imageView-06125
  If the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure included in the `pNext` chain is not VK_NULL_HANDLE, it must not be equal to the `imageView` or `resolveImageView` member of `pDepthAttachment`, `pStencilAttachment`, or any element of `pColorAttachments`

- VUID-VkRenderingInfo-imageView-06126
  If the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure included in the `pNext` chain is not VK_NULL_HANDLE, it must not be equal to the `imageView` member of a VkRenderingFragmentDensityMapAttachmentInfoEXT structure included in the `pNext` chain

- VUID-VkRenderingInfo-multiview-06127
  If the `multiview` feature is not enabled, `viewMask` must be `0`

- VUID-VkRenderingInfo-viewMask-06128
  The index of the most significant bit in `viewMask` must be less than `maxMultiviewViewCount`

- VUID-VkRenderingInfo-perViewRenderAreaCount-07857
  If the `perViewRenderAreaCount` member of a VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM structure included in the `pNext` chain is not `0`, then the `multiviewPerViewRenderAreas` feature must be enabled

- VUID-VkRenderingInfo-perViewRenderAreaCount-07858
  If the `perViewRenderAreaCount` member of a VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM structure included in the `pNext` chain is not `0`, then `renderArea` must specify a render area that includes the union of all per view render areas

- VUID-VkRenderingInfo-None-09044
  Valid attachments specified by this structure must not be bound to memory locations that are bound to any other valid attachments specified by this structure

- VUID-VkRenderingInfo-flags-10012
  If `flags` includes `VK_RENDERING_CONTENTS_INLINE_BIT_KHR` then at least one of the following features must be enabled

  - `maintenance7`

  - `nestedCommandBuffer`

- VUID-VkRenderingInfo-pDepthAttachment-09318
  `pDepthAttachment->resolveMode` must not be `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`

- VUID-VkRenderingInfo-pStencilAttachment-09319
  `pStencilAttachment->resolveMode` must not be `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`

- VUID-VkRenderingInfo-colorAttachmentCount-09320
  If `colorAttachmentCount` is not `1`, the `resolveMode` member of any element of `pColorAttachments` must not be `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`

- VUID-VkRenderingInfo-resolveMode-09321
  If the `resolveMode` of any element of `pColorAttachments` is `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, VkRenderingFragmentDensityMapAttachmentInfoEXT::`imageView` must be VK_NULL_HANDLE

- VUID-VkRenderingInfo-resolveMode-09322
  If the `resolveMode` of any element of `pColorAttachments` is `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, VkRenderingFragmentShadingRateAttachmentInfoKHR::`imageView` must be VK_NULL_HANDLE

- VUID-VkRenderingInfo-pNext-09535
  If the `pNext` chain contains a VkRenderPassStripeBeginInfoARM structure, the union of stripe areas defined by the elements of VkRenderPassStripeInfoARM::`pStripeInfos` must cover the `renderArea`

- VUID-VkRenderingInfo-colorAttachmentCount-09479
  If `colorAttachmentCount` is not `0` and the `imageView` member of an element of `pColorAttachments` is not VK_NULL_HANDLE, that `imageView` must have been created with the identity swizzle

- VUID-VkRenderingInfo-colorAttachmentCount-09480
  If `colorAttachmentCount` is not `0`, and there is an element of `pColorAttachments` with either its `resolveMode` member set to `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, or its `imageView` member not set to VK_NULL_HANDLE and its `resolveMode` member not set to `VK_RESOLVE_MODE_NONE`, the `resolveImageView` member of that element of `pColorAttachments` must have been created with the identity swizzle

- VUID-VkRenderingInfo-pDepthAttachment-09481
  If `pDepthAttachment` is not `NULL` and `pDepthAttachment->imageView` is not VK_NULL_HANDLE, `pDepthAttachment->imageView` must have been created with the identity swizzle

- VUID-VkRenderingInfo-pDepthAttachment-09482
  If `pDepthAttachment` is not `NULL`, `pDepthAttachment->imageView` is not VK_NULL_HANDLE, and `pDepthAttachment->resolveMode` is not `VK_RESOLVE_MODE_NONE`, `pDepthAttachment->resolveImageView` must have been created with the identity swizzle

- VUID-VkRenderingInfo-pStencilAttachment-09483
  If `pStencilAttachment` is not `NULL` and `pStencilAttachment->imageView` is not VK_NULL_HANDLE, `pStencilAttachment->imageView` must have been created with the identity swizzle

- VUID-VkRenderingInfo-pStencilAttachment-09484
  If `pStencilAttachment` is not `NULL`, `pStencilAttachment->imageView` is not VK_NULL_HANDLE, and `pStencilAttachment->resolveMode` is not `VK_RESOLVE_MODE_NONE`, `pStencilAttachment->resolveImageView` must have been created with the identity swizzle

- VUID-VkRenderingInfo-imageView-09485
  If the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure included in the `pNext` chain is not VK_NULL_HANDLE, it must have been created with the identity swizzle

- VUID-VkRenderingInfo-imageView-09486
  If the `imageView` member of a VkRenderingFragmentDensityMapAttachmentInfoEXT structure included in the `pNext` chain is not VK_NULL_HANDLE, it must have been created with the identity swizzle

Valid Usage (Implicit)

- VUID-VkRenderingInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDERING_INFO`

- VUID-VkRenderingInfo-pNext-pNext
  Each `pNext` member of any structure (including this one) in the `pNext` chain must be either `NULL` or a pointer to a valid instance of VkDeviceGroupRenderPassBeginInfo, VkMultisampledRenderToSingleSampledInfoEXT, VkMultiviewPerViewAttributesInfoNVX, VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM, VkRenderPassStripeBeginInfoARM, VkRenderingFragmentDensityMapAttachmentInfoEXT, or VkRenderingFragmentShadingRateAttachmentInfoKHR

- VUID-VkRenderingInfo-sType-unique
  The `sType` value of each struct in the `pNext` chain must be unique

- VUID-VkRenderingInfo-flags-parameter
  `flags` must be a valid combination of VkRenderingFlagBits values

- VUID-VkRenderingInfo-pColorAttachments-parameter
  If `colorAttachmentCount` is not `0`, `pColorAttachments` must be a valid pointer to an array of `colorAttachmentCount` valid VkRenderingAttachmentInfo structures

- VUID-VkRenderingInfo-pDepthAttachment-parameter
  If `pDepthAttachment` is not `NULL`, `pDepthAttachment` must be a valid pointer to a valid VkRenderingAttachmentInfo structure

- VUID-VkRenderingInfo-pStencilAttachment-parameter
  If `pStencilAttachment` is not `NULL`, `pStencilAttachment` must be a valid pointer to a valid VkRenderingAttachmentInfo structure

Bits which can be set in VkRenderingInfo::`flags` describing additional properties of the render pass are:

    // Provided by VK_VERSION_1_3
    typedef enum VkRenderingFlagBits {
        VK_RENDERING_CONTENTS_SECONDARY_COMMAND_BUFFERS_BIT = 0x00000001,
        VK_RENDERING_SUSPENDING_BIT = 0x00000002,
        VK_RENDERING_RESUMING_BIT = 0x00000004,
      // Provided by VK_EXT_legacy_dithering with (VK_KHR_dynamic_rendering or VK_VERSION_1_3) and (VK_KHR_maintenance5 or VK_VERSION_1_4)
        VK_RENDERING_ENABLE_LEGACY_DITHERING_BIT_EXT = 0x00000008,
      // Provided by VK_KHR_maintenance7
        VK_RENDERING_CONTENTS_INLINE_BIT_KHR = 0x00000010,
      // Provided by VK_KHR_dynamic_rendering
        VK_RENDERING_CONTENTS_SECONDARY_COMMAND_BUFFERS_BIT_KHR = VK_RENDERING_CONTENTS_SECONDARY_COMMAND_BUFFERS_BIT,
      // Provided by VK_KHR_dynamic_rendering
        VK_RENDERING_SUSPENDING_BIT_KHR = VK_RENDERING_SUSPENDING_BIT,
      // Provided by VK_KHR_dynamic_rendering
        VK_RENDERING_RESUMING_BIT_KHR = VK_RENDERING_RESUMING_BIT,
      // Provided by VK_EXT_nested_command_buffer
        VK_RENDERING_CONTENTS_INLINE_BIT_EXT = VK_RENDERING_CONTENTS_INLINE_BIT_KHR,
    } VkRenderingFlagBits;

or the equivalent

    // Provided by VK_KHR_dynamic_rendering
    typedef VkRenderingFlagBits VkRenderingFlagBitsKHR;

- `VK_RENDERING_CONTENTS_SECONDARY_COMMAND_BUFFERS_BIT` specifies that draw calls for the render pass instance will be recorded in secondary command buffers. If the `nestedCommandBuffer` feature is enabled, the draw calls can come from both inline and vkCmdExecuteCommands.

- `VK_RENDERING_RESUMING_BIT` specifies that the render pass instance is resuming an earlier suspended render pass instance.

- `VK_RENDERING_SUSPENDING_BIT` specifies that the render pass instance will be suspended.

- `VK_RENDERING_ENABLE_LEGACY_DITHERING_BIT_EXT` specifies that Legacy Dithering is enabled for the render pass instance.

- `VK_RENDERING_CONTENTS_INLINE_BIT_KHR` specifies that draw calls for the render pass instance can be recorded inline within the current command buffer. This can be combined with the `VK_RENDERING_CONTENTS_SECONDARY_COMMAND_BUFFERS_BIT` bit to allow draw calls to be recorded both inline and in secondary command buffers.

The contents of `pRenderingInfo` must match between suspended render pass instances and the render pass instances that resume them, other than the presence or absence of the `VK_RENDERING_RESUMING_BIT`, `VK_RENDERING_SUSPENDING_BIT`, and `VK_RENDERING_CONTENTS_SECONDARY_COMMAND_BUFFERS_BIT` flags. No action or synchronization commands, or other render pass instances, are allowed between suspending and resuming render pass instances.

    // Provided by VK_VERSION_1_3
    typedef VkFlags VkRenderingFlags;

or the equivalent

    // Provided by VK_KHR_dynamic_rendering
    typedef VkRenderingFlags VkRenderingFlagsKHR;

`VkRenderingFlags` is a bitmask type for setting a mask of zero or more VkRenderingFlagBits.

The `VkRenderingAttachmentInfo` structure is defined as:

    // Provided by VK_VERSION_1_3
    typedef struct VkRenderingAttachmentInfo {
        VkStructureType          sType;
        const void*              pNext;
        VkImageView              imageView;
        VkImageLayout            imageLayout;
        VkResolveModeFlagBits    resolveMode;
        VkImageView              resolveImageView;
        VkImageLayout            resolveImageLayout;
        VkAttachmentLoadOp       loadOp;
        VkAttachmentStoreOp      storeOp;
        VkClearValue             clearValue;
    } VkRenderingAttachmentInfo;

or the equivalent

    // Provided by VK_KHR_dynamic_rendering
    typedef VkRenderingAttachmentInfo VkRenderingAttachmentInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `imageView` is the image view that will be used for rendering.

- `imageLayout` is the layout that `imageView` will be in during rendering.

- `resolveMode` is a VkResolveModeFlagBits value defining how data written to `imageView` will be resolved into `resolveImageView`.

- `resolveImageView` is an image view used to write resolved data at the end of rendering.

- `resolveImageLayout` is the layout that `resolveImageView` will be in during rendering.

- `loadOp` is a VkAttachmentLoadOp value defining the load operation for the attachment.

- `storeOp` is a VkAttachmentStoreOp value defining the store operation for the attachment.

- `clearValue` is a VkClearValue structure defining values used to clear `imageView` when `loadOp` is `VK_ATTACHMENT_LOAD_OP_CLEAR`.

Values in `imageView` are loaded and stored according to the values of `loadOp` and `storeOp`, within the render area for each device specified in VkRenderingInfo. If `imageView` is VK_NULL_HANDLE, and `resolveMode` is not `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, other members of this structure are ignored; writes to this attachment will be discarded, and no load, store, or multisample resolve operations will be performed.

If `resolveMode` is `VK_RESOLVE_MODE_NONE`, then `resolveImageView` is ignored. If `resolveMode` is not `VK_RESOLVE_MODE_NONE`, and `resolveImageView` is not VK_NULL_HANDLE, a render pass multisample resolve operation is defined for the attachment subresource. If `resolveMode` is `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, and the `nullColorAttachmentWithExternalFormatResolve` limit is `VK_TRUE`, values are only undefined once load operations have completed.

Note | The resolve mode and store operation are independent; it is valid to write both resolved and unresolved values, and equally valid to discard the unresolved values while writing the resolved ones.

Store and resolve operations are only performed at the end of a render pass instance that does not specify the `VK_RENDERING_SUSPENDING_BIT_KHR` flag.

Load operations are only performed at the beginning of a render pass instance that does not specify the `VK_RENDERING_RESUMING_BIT_KHR` flag.

Image contents at the end of a suspended render pass instance remain defined for access by a resuming render pass instance.

If the `nullColorAttachmentWithExternalFormatResolve` limit is `VK_TRUE`, and `resolveMode` is `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, values in the color attachment will be loaded from the resolve attachment at the start of rendering, and may also be reloaded any time after a resolve occurs or the resolve attachment is written to; if this occurs it must happen-before any writes to the color attachment are performed which happen-after the resolve that triggers this. If any color component in the external format is subsampled, values will be read from the nearest sample in the image when they are loaded.

Valid Usage

- VUID-VkRenderingAttachmentInfo-imageView-06129
  If `imageView` is not VK_NULL_HANDLE and has a non-integer color format, `resolveMode` must be `VK_RESOLVE_MODE_NONE` or `VK_RESOLVE_MODE_AVERAGE_BIT`

- VUID-VkRenderingAttachmentInfo-imageView-06130
  If `imageView` is not VK_NULL_HANDLE and has an integer color format, `resolveMode` must be `VK_RESOLVE_MODE_NONE` or `VK_RESOLVE_MODE_SAMPLE_ZERO_BIT`

- VUID-VkRenderingAttachmentInfo-imageView-06861
  `imageView` must not have a sample count of `VK_SAMPLE_COUNT_1_BIT` if all of the following hold:

  - `imageView` is not VK_NULL_HANDLE

  - `resolveMode` is not `VK_RESOLVE_MODE_NONE`

  - the `pNext` chain of VkRenderingInfo does not include a VkMultisampledRenderToSingleSampledInfoEXT structure with the `multisampledRenderToSingleSampledEnable` field equal to `VK_TRUE`

- VUID-VkRenderingAttachmentInfo-imageView-06862
  `resolveImageView` must not be VK_NULL_HANDLE if all of the following hold:

  - `imageView` is not VK_NULL_HANDLE

  - `resolveMode` is not `VK_RESOLVE_MODE_NONE`

  - the `pNext` chain of VkRenderingInfo does not include a VkMultisampledRenderToSingleSampledInfoEXT structure with the `multisampledRenderToSingleSampledEnable` field equal to `VK_TRUE`

- VUID-VkRenderingAttachmentInfo-imageView-06863
  If `imageView` is not VK_NULL_HANDLE, `resolveMode` is not `VK_RESOLVE_MODE_NONE`, the `pNext` chain of VkRenderingInfo includes a VkMultisampledRenderToSingleSampledInfoEXT structure with the `multisampledRenderToSingleSampledEnable` field equal to `VK_TRUE`, and `imageView` has a sample count of `VK_SAMPLE_COUNT_1_BIT`, `resolveImageView` must be VK_NULL_HANDLE

- VUID-VkRenderingAttachmentInfo-imageView-06864
  If `imageView` is not VK_NULL_HANDLE, `resolveImageView` is not VK_NULL_HANDLE, and `resolveMode` is not `VK_RESOLVE_MODE_NONE`, `resolveImageView` must have a sample count of `VK_SAMPLE_COUNT_1_BIT`

- VUID-VkRenderingAttachmentInfo-imageView-06865
  If `imageView` is not VK_NULL_HANDLE, `resolveImageView` is not VK_NULL_HANDLE, and `resolveMode` is not `VK_RESOLVE_MODE_NONE`, `imageView` and `resolveImageView` must have the same VkFormat

- VUID-VkRenderingAttachmentInfo-imageView-06135
  If `imageView` is not VK_NULL_HANDLE, `imageLayout` must not be `VK_IMAGE_LAYOUT_UNDEFINED`, `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_TRANSFER_SRC_OPTIMAL`, `VK_IMAGE_LAYOUT_TRANSFER_DST_OPTIMAL`, or `VK_IMAGE_LAYOUT_PREINITIALIZED`

- VUID-VkRenderingAttachmentInfo-imageView-06136
  If `imageView` is not VK_NULL_HANDLE and `resolveMode` is not `VK_RESOLVE_MODE_NONE`, `resolveImageLayout` must not be `VK_IMAGE_LAYOUT_UNDEFINED`, `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_TRANSFER_SRC_OPTIMAL`, `VK_IMAGE_LAYOUT_TRANSFER_DST_OPTIMAL`, or `VK_IMAGE_LAYOUT_PREINITIALIZED`

- VUID-VkRenderingAttachmentInfo-imageView-06137
  If `imageView` is not VK_NULL_HANDLE and `resolveMode` is not `VK_RESOLVE_MODE_NONE`, `resolveImageLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderingAttachmentInfo-imageView-06138
  If `imageView` is not VK_NULL_HANDLE, `imageLayout` must not be `VK_IMAGE_LAYOUT_SHADING_RATE_OPTIMAL_NV`

- VUID-VkRenderingAttachmentInfo-imageView-06139
  If `imageView` is not VK_NULL_HANDLE and `resolveMode` is not `VK_RESOLVE_MODE_NONE`, `resolveImageLayout` must not be `VK_IMAGE_LAYOUT_SHADING_RATE_OPTIMAL_NV`

- VUID-VkRenderingAttachmentInfo-imageView-06140
  If `imageView` is not VK_NULL_HANDLE, `imageLayout` must not be `VK_IMAGE_LAYOUT_FRAGMENT_DENSITY_MAP_OPTIMAL_EXT`

- VUID-VkRenderingAttachmentInfo-imageView-06141
  If `imageView` is not VK_NULL_HANDLE and `resolveMode` is not `VK_RESOLVE_MODE_NONE`, `resolveImageLayout` must not be `VK_IMAGE_LAYOUT_FRAGMENT_DENSITY_MAP_OPTIMAL_EXT`

- VUID-VkRenderingAttachmentInfo-imageView-06142
  If `imageView` is not VK_NULL_HANDLE and `resolveMode` is not `VK_RESOLVE_MODE_NONE`, `resolveImageLayout` must not be `VK_IMAGE_LAYOUT_READ_ONLY_OPTIMAL_KHR`

- VUID-VkRenderingAttachmentInfo-imageView-06143
  If `imageView` is not VK_NULL_HANDLE, `imageLayout` must not be `VK_IMAGE_LAYOUT_FRAGMENT_SHADING_RATE_ATTACHMENT_OPTIMAL_KHR`

- VUID-VkRenderingAttachmentInfo-imageView-06144
  If `imageView` is not VK_NULL_HANDLE and `resolveMode` is not `VK_RESOLVE_MODE_NONE`, `resolveImageLayout` must not be `VK_IMAGE_LAYOUT_FRAGMENT_SHADING_RATE_ATTACHMENT_OPTIMAL_KHR`

- VUID-VkRenderingAttachmentInfo-imageView-06145
  If `imageView` is not VK_NULL_HANDLE, `imageLayout` must not be `VK_IMAGE_LAYOUT_PRESENT_SRC_KHR`

- VUID-VkRenderingAttachmentInfo-imageView-06146
  If `imageView` is not VK_NULL_HANDLE and `resolveMode` is not `VK_RESOLVE_MODE_NONE`, `resolveImageLayout` must not be `VK_IMAGE_LAYOUT_PRESENT_SRC_KHR`

- VUID-VkRenderingAttachmentInfo-externalFormatResolve-09323
  If the `externalFormatResolve` feature is not enabled, `resolveMode` must not be `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`

- VUID-VkRenderingAttachmentInfo-resolveMode-09324
  If `resolveMode` is `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, `resolveImageView` must be a valid image view

- VUID-VkRenderingAttachmentInfo-nullColorAttachmentWithExternalFormatResolve-09325
  If the `nullColorAttachmentWithExternalFormatResolve` property is `VK_TRUE` and `resolveMode` is `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, `resolveImageView` must have been created with an image with a `samples` value of `VK_SAMPLE_COUNT_1_BIT`

- VUID-VkRenderingAttachmentInfo-resolveMode-09326
  If `resolveMode` is `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, `resolveImageView` must have been created with an external format specified by VkExternalFormatANDROID

- VUID-VkRenderingAttachmentInfo-resolveMode-09327
  If `resolveMode` is `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`, `resolveImageView` must have been created with a `subresourceRange.layerCount` of `1`

- VUID-VkRenderingAttachmentInfo-resolveMode-09328
  If `resolveMode` is `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID` and `nullColorAttachmentWithExternalFormatResolve` is `VK_TRUE`, `imageView` must be VK_NULL_HANDLE

- VUID-VkRenderingAttachmentInfo-resolveMode-09329
  If `resolveMode` is `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID` and `nullColorAttachmentWithExternalFormatResolve` is `VK_FALSE`, `imageView` must be a valid VkImageView

- VUID-VkRenderingAttachmentInfo-resolveMode-09330
  If `resolveMode` is `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID` and `nullColorAttachmentWithExternalFormatResolve` is `VK_FALSE`, `imageView` must have a format equal to the value of VkAndroidHardwareBufferFormatResolvePropertiesANDROID::`colorAttachmentFormat` as returned by a call to vkGetAndroidHardwareBufferPropertiesANDROID for the Android hardware buffer that was used to create `resolveImageView`

Valid Usage (Implicit)

- VUID-VkRenderingAttachmentInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDERING_ATTACHMENT_INFO`

- VUID-VkRenderingAttachmentInfo-pNext-pNext
  `pNext` must be `NULL`

- VUID-VkRenderingAttachmentInfo-imageView-parameter
  If `imageView` is not VK_NULL_HANDLE, `imageView` must be a valid VkImageView handle

- VUID-VkRenderingAttachmentInfo-imageLayout-parameter
  `imageLayout` must be a valid VkImageLayout value

- VUID-VkRenderingAttachmentInfo-resolveMode-parameter
  If `resolveMode` is not `0`, `resolveMode` must be a valid VkResolveModeFlagBits value

- VUID-VkRenderingAttachmentInfo-resolveImageView-parameter
  If `resolveImageView` is not VK_NULL_HANDLE, `resolveImageView` must be a valid VkImageView handle

- VUID-VkRenderingAttachmentInfo-resolveImageLayout-parameter
  `resolveImageLayout` must be a valid VkImageLayout value

- VUID-VkRenderingAttachmentInfo-loadOp-parameter
  `loadOp` must be a valid VkAttachmentLoadOp value

- VUID-VkRenderingAttachmentInfo-storeOp-parameter
  `storeOp` must be a valid VkAttachmentStoreOp value

- VUID-VkRenderingAttachmentInfo-clearValue-parameter
  `clearValue` must be a valid VkClearValue union

- VUID-VkRenderingAttachmentInfo-commonparent
  Both of `imageView`, and `resolveImageView` that are valid handles of non-ignored parameters must have been created, allocated, or retrieved from the same VkDevice

The `VkRenderingFragmentShadingRateAttachmentInfoKHR` structure is defined as:

    // Provided by VK_KHR_fragment_shading_rate with VK_VERSION_1_3 or VK_KHR_dynamic_rendering
    typedef struct VkRenderingFragmentShadingRateAttachmentInfoKHR {
        VkStructureType    sType;
        const void*        pNext;
        VkImageView        imageView;
        VkImageLayout      imageLayout;
        VkExtent2D         shadingRateAttachmentTexelSize;
    } VkRenderingFragmentShadingRateAttachmentInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `imageView` is the image view that will be used as a fragment shading rate attachment.

- `imageLayout` is the layout that `imageView` will be in during rendering.

- `shadingRateAttachmentTexelSize` specifies the number of pixels corresponding to each texel in `imageView`.

This structure can be included in the `pNext` chain of VkRenderingInfo to define a fragment shading rate attachment. If `imageView` is VK_NULL_HANDLE, or if this structure is not specified, the implementation behaves as if a valid shading rate attachment was specified with all texels specifying a single pixel per fragment.

Valid Usage

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-imageView-06147
  If `imageView` is not VK_NULL_HANDLE, `layout` must be `VK_IMAGE_LAYOUT_GENERAL` or `VK_IMAGE_LAYOUT_FRAGMENT_SHADING_RATE_ATTACHMENT_OPTIMAL_KHR`

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-imageView-06148
  If `imageView` is not VK_NULL_HANDLE, it must have been created with `VK_IMAGE_USAGE_FRAGMENT_SHADING_RATE_ATTACHMENT_BIT_KHR`

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-imageView-06149
  If `imageView` is not VK_NULL_HANDLE, `shadingRateAttachmentTexelSize.width` must be a power of two value

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-imageView-06150
  If `imageView` is not VK_NULL_HANDLE, `shadingRateAttachmentTexelSize.width` must be less than or equal to `maxFragmentShadingRateAttachmentTexelSize.width`

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-imageView-06151
  If `imageView` is not VK_NULL_HANDLE, `shadingRateAttachmentTexelSize.width` must be greater than or equal to `minFragmentShadingRateAttachmentTexelSize.width`

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-imageView-06152
  If `imageView` is not VK_NULL_HANDLE, `shadingRateAttachmentTexelSize.height` must be a power of two value

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-imageView-06153
  If `imageView` is not VK_NULL_HANDLE, `shadingRateAttachmentTexelSize.height` must be less than or equal to `maxFragmentShadingRateAttachmentTexelSize.height`

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-imageView-06154
  If `imageView` is not VK_NULL_HANDLE, `shadingRateAttachmentTexelSize.height` must be greater than or equal to `minFragmentShadingRateAttachmentTexelSize.height`

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-imageView-06155
  If `imageView` is not VK_NULL_HANDLE, the quotient of `shadingRateAttachmentTexelSize.width` and `shadingRateAttachmentTexelSize.height` must be less than or equal to `maxFragmentShadingRateAttachmentTexelSizeAspectRatio`

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-imageView-06156
  If `imageView` is not VK_NULL_HANDLE, the quotient of `shadingRateAttachmentTexelSize.height` and `shadingRateAttachmentTexelSize.width` must be less than or equal to `maxFragmentShadingRateAttachmentTexelSizeAspectRatio`

Valid Usage (Implicit)

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDERING_FRAGMENT_SHADING_RATE_ATTACHMENT_INFO_KHR`

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-imageView-parameter
  If `imageView` is not VK_NULL_HANDLE, `imageView` must be a valid VkImageView handle

- VUID-VkRenderingFragmentShadingRateAttachmentInfoKHR-imageLayout-parameter
  `imageLayout` must be a valid VkImageLayout value

The `VkRenderingFragmentDensityMapAttachmentInfoEXT` structure is defined as:

    // Provided by VK_EXT_fragment_density_map with VK_VERSION_1_3 or VK_KHR_dynamic_rendering
    typedef struct VkRenderingFragmentDensityMapAttachmentInfoEXT {
        VkStructureType    sType;
        const void*        pNext;
        VkImageView        imageView;
        VkImageLayout      imageLayout;
    } VkRenderingFragmentDensityMapAttachmentInfoEXT;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `imageView` is the image view that will be used as a fragment density map attachment.

- `imageLayout` is the layout that `imageView` will be in during rendering.

This structure can be included in the `pNext` chain of VkRenderingInfo to define a fragment density map. If this structure is not included in the `pNext` chain, `imageView` is treated as VK_NULL_HANDLE.

Valid Usage

- VUID-VkRenderingFragmentDensityMapAttachmentInfoEXT-imageView-06157
  If `imageView` is not VK_NULL_HANDLE, `imageLayout` must be `VK_IMAGE_LAYOUT_GENERAL` or `VK_IMAGE_LAYOUT_FRAGMENT_DENSITY_MAP_OPTIMAL_EXT`

- VUID-VkRenderingFragmentDensityMapAttachmentInfoEXT-imageView-06158
  If `imageView` is not VK_NULL_HANDLE, it must have been created with `VK_IMAGE_USAGE_FRAGMENT_DENSITY_MAP_BIT_EXT`

- VUID-VkRenderingFragmentDensityMapAttachmentInfoEXT-imageView-06159
  If `imageView` is not VK_NULL_HANDLE, it must not have been created with `VK_IMAGE_CREATE_SUBSAMPLED_BIT_EXT`

- VUID-VkRenderingFragmentDensityMapAttachmentInfoEXT-apiVersion-07908
  If the `multiview` feature is not enabled, VkPhysicalDeviceProperties::`apiVersion` is less than Vulkan 1.1, and `imageView` is not VK_NULL_HANDLE, it must have a `layerCount` equal to `1`

Valid Usage (Implicit)

- VUID-VkRenderingFragmentDensityMapAttachmentInfoEXT-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDERING_FRAGMENT_DENSITY_MAP_ATTACHMENT_INFO_EXT`

- VUID-VkRenderingFragmentDensityMapAttachmentInfoEXT-imageView-parameter
  `imageView` must be a valid VkImageView handle

- VUID-VkRenderingFragmentDensityMapAttachmentInfoEXT-imageLayout-parameter
  `imageLayout` must be a valid VkImageLayout value

To query the render area granularity for a render pass instance, call:

    // Provided by VK_VERSION_1_4
    void vkGetRenderingAreaGranularity(
        VkDevice                                    device,
        const VkRenderingAreaInfo*                  pRenderingAreaInfo,
        VkExtent2D*                                 pGranularity);

or the equivalent command

    // Provided by VK_KHR_maintenance5
    void vkGetRenderingAreaGranularityKHR(
        VkDevice                                    device,
        const VkRenderingAreaInfo*                  pRenderingAreaInfo,
        VkExtent2D*                                 pGranularity);

- `device` is the logical device that owns the render pass instance.

- `pRenderingAreaInfo` is a pointer to a VkRenderingAreaInfo structure specifying details of the render pass instance to query the render area granularity for.

- `pGranularity` is a pointer to a VkExtent2D structure in which the granularity is returned.

The conditions leading to an optimal `renderArea` are:

- the `offset.x` member in `renderArea` is a multiple of the `width` member of the returned VkExtent2D (the horizontal granularity).

- the `offset.y` member in `renderArea` is a multiple of the `height` member of the returned VkExtent2D (the vertical granularity).

- either the `extent.width` member in `renderArea` is a multiple of the horizontal granularity or `offset.x`+`extent.width` is equal to the `width` of each attachment used in the render pass instance.

- either the `extent.height` member in `renderArea` is a multiple of the vertical granularity or `offset.y`+`extent.height` is equal to the `height` of each attachment used in the render pass instance.

Valid Usage (Implicit)

- VUID-vkGetRenderingAreaGranularity-device-parameter
  `device` must be a valid VkDevice handle

- VUID-vkGetRenderingAreaGranularity-pRenderingAreaInfo-parameter
  `pRenderingAreaInfo` must be a valid pointer to a valid VkRenderingAreaInfo structure

- VUID-vkGetRenderingAreaGranularity-pGranularity-parameter
  `pGranularity` must be a valid pointer to a VkExtent2D structure

The `VkRenderingAreaInfo` structure is defined as:

    // Provided by VK_VERSION_1_4
    typedef struct VkRenderingAreaInfo {
        VkStructureType    sType;
        const void*        pNext;
        uint32_t           viewMask;
        uint32_t           colorAttachmentCount;
        const VkFormat*    pColorAttachmentFormats;
        VkFormat           depthAttachmentFormat;
        VkFormat           stencilAttachmentFormat;
    } VkRenderingAreaInfo;

or the equivalent

    // Provided by VK_KHR_maintenance5
    typedef VkRenderingAreaInfo VkRenderingAreaInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `viewMask` is the viewMask used for rendering.

- `colorAttachmentCount` is the number of entries in `pColorAttachmentFormats`

- `pColorAttachmentFormats` is a pointer to an array of VkFormat values defining the format of color attachments used in the render pass instance.

- `depthAttachmentFormat` is a VkFormat value defining the format of the depth attachment used in the render pass instance.

- `stencilAttachmentFormat` is a VkFormat value defining the format of the stencil attachment used in the render pass instance.

Valid Usage (Implicit)

- VUID-VkRenderingAreaInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDERING_AREA_INFO`

- VUID-VkRenderingAreaInfo-pNext-pNext
  `pNext` must be `NULL`

The `VkRenderPassStripeBeginInfoARM` structure is defined as:

    // Provided by VK_ARM_render_pass_striped
    typedef struct VkRenderPassStripeBeginInfoARM {
        VkStructureType                     sType;
        const void*                         pNext;
        uint32_t                            stripeInfoCount;
        const VkRenderPassStripeInfoARM*    pStripeInfos;
    } VkRenderPassStripeBeginInfoARM;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `stripeInfoCount` is the number of stripes in this render pass instance

- `pStripeInfos` is a pointer to an array of `stripeInfoCount` VkRenderPassStripeInfoARM structures describing the stripes used by the render pass instance.

This structure can be included in the `pNext` chain of VkRenderPassBeginInfo or VkRenderingInfo to define how the render pass instance is split into stripes.

Valid Usage

- VUID-VkRenderPassStripeBeginInfoARM-stripeInfoCount-09450
  `stripeInfoCount` must be less than or equal to `VkPhysicalDeviceRenderPassStripedPropertiesARM`::`maxRenderPassStripes`

- VUID-VkRenderPassStripeBeginInfoARM-stripeArea-09451
  The `stripeArea` defined by each element of `pStripeInfos` must not overlap the `stripeArea` of any other element

Valid Usage (Implicit)

- VUID-VkRenderPassStripeBeginInfoARM-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_STRIPE_BEGIN_INFO_ARM`

- VUID-VkRenderPassStripeBeginInfoARM-pStripeInfos-parameter
  `pStripeInfos` must be a valid pointer to an array of `stripeInfoCount` valid VkRenderPassStripeInfoARM structures

- VUID-VkRenderPassStripeBeginInfoARM-stripeInfoCount-arraylength
  `stripeInfoCount` must be greater than `0`

The `VkRenderPassStripeInfoARM` structure is defined as:

    // Provided by VK_ARM_render_pass_striped
    typedef struct VkRenderPassStripeInfoARM {
        VkStructureType    sType;
        const void*        pNext;
        VkRect2D           stripeArea;
    } VkRenderPassStripeInfoARM;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `stripeArea` is the stripe area, and is described in more detail below.

`stripeArea` is the render area that is affected by this stripe of the render pass instance. It must be a subregion of the `renderArea` of the render pass instance.

Valid Usage

- VUID-VkRenderPassStripeInfoARM-stripeArea-09452
  `stripeArea.offset.x` must be a multiple of VkPhysicalDeviceRenderPassStripedPropertiesARM::`renderPassStripeGranularity.width`

- VUID-VkRenderPassStripeInfoARM-stripeArea-09453
  `stripeArea.extent.width` must be a multiple of VkPhysicalDeviceRenderPassStripedPropertiesARM::`renderPassStripeGranularity.width`, or the sum of `stripeArea.offset.x` and `stripeArea.extent.width` must be equal to the `renderArea.extent.width` of the render pass instance

- VUID-VkRenderPassStripeInfoARM-stripeArea-09454
  `stripeArea.offset.y` must be a multiple of VkPhysicalDeviceRenderPassStripedPropertiesARM::`renderPassStripeGranularity.height`

- VUID-VkRenderPassStripeInfoARM-stripeArea-09455
  `stripeArea.extent.height` must be a multiple of VkPhysicalDeviceRenderPassStripedPropertiesARM::`renderPassStripeGranularity.height`, or the sum of `stripeArea.offset.y` and `stripeArea.extent.height` must be equal to the `renderArea.extent.height` of the render pass instance

Valid Usage (Implicit)

- VUID-VkRenderPassStripeInfoARM-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_STRIPE_INFO_ARM`

- VUID-VkRenderPassStripeInfoARM-pNext-pNext
  `pNext` must be `NULL`

To end a render pass instance, call:

    // Provided by VK_VERSION_1_3
    void vkCmdEndRendering(
        VkCommandBuffer                             commandBuffer);

or the equivalent command

    // Provided by VK_KHR_dynamic_rendering
    void vkCmdEndRenderingKHR(
        VkCommandBuffer                             commandBuffer);

- `commandBuffer` is the command buffer in which to record the command.

If the value of `pRenderingInfo->flags` used to begin this render pass instance included `VK_RENDERING_SUSPENDING_BIT`, then this render pass is suspended and will be resumed later in submission order.

Valid Usage

- VUID-vkCmdEndRendering-None-06161
  The current render pass instance must have been begun with vkCmdBeginRendering

- VUID-vkCmdEndRendering-commandBuffer-06162
  The current render pass instance must have been begun in `commandBuffer`

- VUID-vkCmdEndRendering-None-06781
  This command must not be recorded when transform feedback is active

- VUID-vkCmdEndRendering-None-06999
  If `vkCmdBeginQuery`* was called within the render pass, the corresponding `vkCmdEndQuery`* must have been called subsequently within the same subpass

Valid Usage (Implicit)

- VUID-vkCmdEndRendering-commandBuffer-parameter
  `commandBuffer` must be a valid VkCommandBuffer handle

- VUID-vkCmdEndRendering-commandBuffer-recording
  `commandBuffer` must be in the recording state

- VUID-vkCmdEndRendering-commandBuffer-cmdpool
  The `VkCommandPool` that `commandBuffer` was allocated from must support graphics operations

- VUID-vkCmdEndRendering-renderpass
  This command must only be called inside of a render pass instance

- VUID-vkCmdEndRendering-videocoding
  This command must only be called outside of a video coding scope

Host Synchronization

- Host access to `commandBuffer` must be externally synchronized

- Host access to the `VkCommandPool` that `commandBuffer` was allocated from must be externally synchronized

Command Properties

Command Buffer Levels | Render Pass Scope | Video Coding Scope | Supported Queue Types | Command Type
--- | --- | --- | --- | ---
Primary Secondary | Inside | Outside | Graphics | Action State

Note | For more complex rendering graphs, it is possible to pre-define a static render pass object, which as well as allowing draw commands, allows the definition of framebuffer-local dependencies between multiple subpasses. These objects have a lot of setup cost compared to vkCmdBeginRendering, but use of subpass dependencies can confer important performance benefits on some devices.

The `VkTilePropertiesQCOM` structure is defined as:

    // Provided by VK_QCOM_tile_properties
    typedef struct VkTilePropertiesQCOM {
        VkStructureType    sType;
        void*              pNext;
        VkExtent3D         tileSize;
        VkExtent2D         apronSize;
        VkOffset2D         origin;
    } VkTilePropertiesQCOM;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `tileSize` is the dimensions of a tile, with width and height describing the width and height of a tile in pixels, and depth corresponding to the number of slices the tile spans.

- `apronSize` is the dimension of the apron.

- `origin` is the top-left corner of the first tile in attachment space.

All tiles will be tightly packed around the first tile, with edges being multiples of tile width and/or height from the origin.

Note | Reported value for `apronSize` will be zero and its functionality will be described in a future extension.

Valid Usage (Implicit)

- VUID-VkTilePropertiesQCOM-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_TILE_PROPERTIES_QCOM`

- VUID-VkTilePropertiesQCOM-pNext-pNext
  `pNext` must be `NULL`

To query the tile properties when using dynamic rendering, call:

    // Provided by VK_QCOM_tile_properties
    VkResult vkGetDynamicRenderingTilePropertiesQCOM(
        VkDevice                                    device,
        const VkRenderingInfo*                      pRenderingInfo,
        VkTilePropertiesQCOM*                       pProperties);

- `device` is a logical device associated with the render pass.

- `pRenderingInfo` is a pointer to the VkRenderingInfo structure specifying details of the render pass instance in dynamic rendering.

- `pProperties` is a pointer to a VkTilePropertiesQCOM structure in which the properties are returned.

Valid Usage (Implicit)

- VUID-vkGetDynamicRenderingTilePropertiesQCOM-device-parameter
  `device` must be a valid VkDevice handle

- VUID-vkGetDynamicRenderingTilePropertiesQCOM-pRenderingInfo-parameter
  `pRenderingInfo` must be a valid pointer to a valid VkRenderingInfo structure

- VUID-vkGetDynamicRenderingTilePropertiesQCOM-pProperties-parameter
  `pProperties` must be a valid pointer to a VkTilePropertiesQCOM structure

Return Codes

Success

  - `VK_SUCCESS`

Failure

  None

### 8.1. Render Pass Objects

A render pass object represents a collection of attachments, subpasses, and dependencies between the subpasses, and describes how the attachments are used over the course of the subpasses.

Render passes are represented by `VkRenderPass` handles:

    // Provided by VK_VERSION_1_0
    VK_DEFINE_NON_DISPATCHABLE_HANDLE(VkRenderPass)

An attachment description describes the properties of an attachment including its format, sample count, and how its contents are treated at the beginning and end of each render pass instance.

A subpass represents a phase of rendering that reads and writes a subset of the attachments in a render pass. Rendering commands are recorded into a particular subpass of a render pass instance.

A subpass description describes the subset of attachments that is involved in the execution of a subpass. Each subpass can read from some attachments as input attachments, write to some as color attachments or depth/stencil attachments, perform shader resolve operations to color_attachments or depth/stencil_attachments, and perform multisample resolve operations to resolve attachments. A subpass description can also include a set of preserve attachments, which are attachments that are not read or written by the subpass but whose contents must be preserved throughout the subpass.

A subpass uses an attachment if the attachment is a color, depth/stencil, resolve, depth/stencil resolve, fragment shading rate, or input attachment for that subpass (as determined by the `pColorAttachments`, `pDepthStencilAttachment`, `pResolveAttachments`, VkSubpassDescriptionDepthStencilResolve::`pDepthStencilResolveAttachment`, VkFragmentShadingRateAttachmentInfoKHR::`pFragmentShadingRateAttachment->attachment`, and `pInputAttachments` members of VkSubpassDescription, respectively). A subpass does not use an attachment if that attachment is preserved by the subpass. The first use of an attachment is in the lowest numbered subpass that uses that attachment. Similarly, the last use of an attachment is in the highest numbered subpass that uses that attachment.

The subpasses in a render pass all render to the same dimensions, and fragments for pixel (x,y,layer) in one subpass can only read attachment contents written by previous subpasses at that same (x,y,layer) location. For multi-pixel fragments, the pixel read from an input attachment is selected from the pixels covered by that fragment in an implementation-dependent manner. However, this selection must be made consistently for any fragment with the same shading rate for the lifetime of the VkDevice.

Note | By describing a complete set of subpasses in advance, render passes provide the implementation an opportunity to optimize the storage and transfer of attachment data between subpasses. In practice, this means that subpasses with a simple framebuffer-space dependency may be merged into a single tiled rendering pass, keeping the attachment data on-chip for the duration of a render pass instance. However, it is also quite common for a render pass to only contain a single subpass.

Subpass dependencies describe execution and memory dependencies between subpasses.

A subpass dependency chain is a sequence of subpass dependencies in a render pass, where the source subpass of each subpass dependency (after the first) equals the destination subpass of the previous dependency.

Execution of subpasses may overlap or execute out of order with regards to other subpasses, unless otherwise enforced by an execution dependency. Each subpass only respects submission order for commands recorded in the same subpass, and the vkCmdBeginRenderPass and vkCmdEndRenderPass commands that delimit the render pass - commands within other subpasses are not included. This affects most other implicit ordering guarantees.

A render pass describes the structure of subpasses and attachments independent of any specific image views for the attachments. The specific image views that will be used for the attachments, and their dimensions, are specified in `VkFramebuffer` objects. Framebuffers are created with respect to a specific render pass that the framebuffer is compatible with (see Render Pass Compatibility). Collectively, a render pass and a framebuffer define the complete render target state for one or more subpasses as well as the algorithmic dependencies between the subpasses.

The various pipeline stages of the drawing commands for a given subpass may execute concurrently and/or out of order, both within and across drawing commands, whilst still respecting pipeline order. However for a given (x,y,layer,sample) sample location, certain per-sample operations are performed in rasterization order.

`VK_ATTACHMENT_UNUSED` is a constant indicating that a render pass attachment is not used.

    #define VK_ATTACHMENT_UNUSED              (~0U)

### 8.2. Render Pass Creation

To create a render pass, call:

    // Provided by VK_VERSION_1_0
    VkResult vkCreateRenderPass(
        VkDevice                                    device,
        const VkRenderPassCreateInfo*               pCreateInfo,
        const VkAllocationCallbacks*                pAllocator,
        VkRenderPass*                               pRenderPass);

- `device` is the logical device that creates the render pass.

- `pCreateInfo` is a pointer to a VkRenderPassCreateInfo structure describing the parameters of the render pass.

- `pAllocator` controls host memory allocation as described in the Memory Allocation chapter.

- `pRenderPass` is a pointer to a VkRenderPass handle in which the resulting render pass object is returned.

Valid Usage

- VUID-vkCreateRenderPass-device-10000
  `device` must support at least one queue family with the `VK_QUEUE_GRAPHICS_BIT` capability

Valid Usage (Implicit)

- VUID-vkCreateRenderPass-device-parameter
  `device` must be a valid VkDevice handle

- VUID-vkCreateRenderPass-pCreateInfo-parameter
  `pCreateInfo` must be a valid pointer to a valid VkRenderPassCreateInfo structure

- VUID-vkCreateRenderPass-pAllocator-parameter
  If `pAllocator` is not `NULL`, `pAllocator` must be a valid pointer to a valid VkAllocationCallbacks structure

- VUID-vkCreateRenderPass-pRenderPass-parameter
  `pRenderPass` must be a valid pointer to a VkRenderPass handle

Return Codes

Success

  - `VK_SUCCESS`

Failure

  - `VK_ERROR_OUT_OF_HOST_MEMORY`

  - `VK_ERROR_OUT_OF_DEVICE_MEMORY`

The `VkRenderPassCreateInfo` structure is defined as:

    // Provided by VK_VERSION_1_0
    typedef struct VkRenderPassCreateInfo {
        VkStructureType                   sType;
        const void*                       pNext;
        VkRenderPassCreateFlags           flags;
        uint32_t                          attachmentCount;
        const VkAttachmentDescription*    pAttachments;
        uint32_t                          subpassCount;
        const VkSubpassDescription*       pSubpasses;
        uint32_t                          dependencyCount;
        const VkSubpassDependency*        pDependencies;
    } VkRenderPassCreateInfo;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `flags` is a bitmask of VkRenderPassCreateFlagBits

- `attachmentCount` is the number of attachments used by this render pass.

- `pAttachments` is a pointer to an array of `attachmentCount` VkAttachmentDescription structures describing the attachments used by the render pass.

- `subpassCount` is the number of subpasses to create.

- `pSubpasses` is a pointer to an array of `subpassCount` VkSubpassDescription structures describing each subpass.

- `dependencyCount` is the number of memory dependencies between pairs of subpasses.

- `pDependencies` is a pointer to an array of `dependencyCount` VkSubpassDependency structures describing dependencies between pairs of subpasses.

Note | Care should be taken to avoid a data race here; if any subpasses access attachments with overlapping memory locations, and one of those accesses is a write, a subpass dependency needs to be included between them.

Valid Usage

- VUID-VkRenderPassCreateInfo-attachment-00834
  If the `attachment` member of any element of `pInputAttachments`, `pColorAttachments`, `pResolveAttachments` or `pDepthStencilAttachment`, or any element of `pPreserveAttachments` in any element of `pSubpasses` is not `VK_ATTACHMENT_UNUSED`, then it must be less than `attachmentCount`

- VUID-VkRenderPassCreateInfo-fragmentDensityMapAttachment-06471
  If the pNext chain includes a VkRenderPassFragmentDensityMapCreateInfoEXT structure and the `fragmentDensityMapAttachment` member is not `VK_ATTACHMENT_UNUSED`, then `attachment` must be less than `attachmentCount`

- VUID-VkRenderPassCreateInfo-pAttachments-00836
  For any member of `pAttachments` with a `loadOp` equal to `VK_ATTACHMENT_LOAD_OP_CLEAR`, the first use of that attachment must not specify a `layout` equal to `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderPassCreateInfo-pAttachments-02511
  For any member of `pAttachments` with a `stencilLoadOp` equal to `VK_ATTACHMENT_LOAD_OP_CLEAR`, the first use of that attachment must not specify a `layout` equal to `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderPassCreateInfo-pAttachments-01566
  For any member of `pAttachments` with a `loadOp` equal to `VK_ATTACHMENT_LOAD_OP_CLEAR`, the first use of that attachment must not specify a `layout` equal to `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkRenderPassCreateInfo-pAttachments-01567
  For any member of `pAttachments` with a `stencilLoadOp` equal to `VK_ATTACHMENT_LOAD_OP_CLEAR`, the first use of that attachment must not specify a `layout` equal to `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderPassCreateInfo-pNext-01926
  If the `pNext` chain includes a VkRenderPassInputAttachmentAspectCreateInfo structure, the `subpass` member of each element of its `pAspectReferences` member must be less than `subpassCount`

- VUID-VkRenderPassCreateInfo-pNext-01927
  If the `pNext` chain includes a VkRenderPassInputAttachmentAspectCreateInfo structure, the `inputAttachmentIndex` member of each element of its `pAspectReferences` member must be less than the value of `inputAttachmentCount` in the element of `pSubpasses` identified by its `subpass` member

- VUID-VkRenderPassCreateInfo-pNext-01963
  If the `pNext` chain includes a VkRenderPassInputAttachmentAspectCreateInfo structure, for any element of the `pInputAttachments` member of any element of `pSubpasses` where the `attachment` member is not `VK_ATTACHMENT_UNUSED`, the `aspectMask` member of the corresponding element of VkRenderPassInputAttachmentAspectCreateInfo::`pAspectReferences` must only include aspects that are present in images of the format specified by the element of `pAttachments` at `attachment`

- VUID-VkRenderPassCreateInfo-pNext-01928
  If the `pNext` chain includes a VkRenderPassMultiviewCreateInfo structure, and its `subpassCount` member is not zero, that member must be equal to the value of `subpassCount`

- VUID-VkRenderPassCreateInfo-pNext-01929
  If the `pNext` chain includes a VkRenderPassMultiviewCreateInfo structure, if its `dependencyCount` member is not zero, it must be equal to `dependencyCount`

- VUID-VkRenderPassCreateInfo-pNext-01930
  If the `pNext` chain includes a VkRenderPassMultiviewCreateInfo structure, for each non-zero element of `pViewOffsets`, the `srcSubpass` and `dstSubpass` members of `pDependencies` at the same index must not be equal

- VUID-VkRenderPassCreateInfo-pNext-02512
  If the `pNext` chain includes a VkRenderPassMultiviewCreateInfo structure, for any element of `pDependencies` with a `dependencyFlags` member that does not include `VK_DEPENDENCY_VIEW_LOCAL_BIT`, the corresponding element of the `pViewOffsets` member of that VkRenderPassMultiviewCreateInfo instance must be `0`

- VUID-VkRenderPassCreateInfo-pNext-02513
  If the `pNext` chain includes a VkRenderPassMultiviewCreateInfo structure, elements of its `pViewMasks` member must either all be `0`, or all not be `0`

- VUID-VkRenderPassCreateInfo-pNext-02514
  If the `pNext` chain includes a VkRenderPassMultiviewCreateInfo structure, and each element of its `pViewMasks` member is `0`, the `dependencyFlags` member of each element of `pDependencies` must not include `VK_DEPENDENCY_VIEW_LOCAL_BIT`

- VUID-VkRenderPassCreateInfo-pNext-02515
  If the `pNext` chain includes a VkRenderPassMultiviewCreateInfo structure, and each element of its `pViewMasks` member is `0`, its `correlationMaskCount` member must be `0`

- VUID-VkRenderPassCreateInfo-pDependencies-00837
  For any element of `pDependencies`, if the `srcSubpass` is not `VK_SUBPASS_EXTERNAL`, all stage flags included in the `srcStageMask` member of that dependency must be a pipeline stage supported by the pipeline identified by the `pipelineBindPoint` member of the source subpass

- VUID-VkRenderPassCreateInfo-pDependencies-00838
  For any element of `pDependencies`, if the `dstSubpass` is not `VK_SUBPASS_EXTERNAL`, all stage flags included in the `dstStageMask` member of that dependency must be a pipeline stage supported by the pipeline identified by the `pipelineBindPoint` member of the destination subpass

- VUID-VkRenderPassCreateInfo-pDependencies-06866
  For any element of `pDependencies`, if its `srcSubpass` is not `VK_SUBPASS_EXTERNAL`, it must be less than `subpassCount`

- VUID-VkRenderPassCreateInfo-pDependencies-06867
  For any element of `pDependencies`, if its `dstSubpass` is not `VK_SUBPASS_EXTERNAL`, it must be less than `subpassCount`

Valid Usage (Implicit)

- VUID-VkRenderPassCreateInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_CREATE_INFO`

- VUID-VkRenderPassCreateInfo-pNext-pNext
  Each `pNext` member of any structure (including this one) in the `pNext` chain must be either `NULL` or a pointer to a valid instance of VkRenderPassFragmentDensityMapCreateInfoEXT, VkRenderPassInputAttachmentAspectCreateInfo, or VkRenderPassMultiviewCreateInfo

- VUID-VkRenderPassCreateInfo-sType-unique
  The `sType` value of each struct in the `pNext` chain must be unique

- VUID-VkRenderPassCreateInfo-flags-parameter
  `flags` must be a valid combination of VkRenderPassCreateFlagBits values

- VUID-VkRenderPassCreateInfo-pAttachments-parameter
  If `attachmentCount` is not `0`, `pAttachments` must be a valid pointer to an array of `attachmentCount` valid VkAttachmentDescription structures

- VUID-VkRenderPassCreateInfo-pSubpasses-parameter
  `pSubpasses` must be a valid pointer to an array of `subpassCount` valid VkSubpassDescription structures

- VUID-VkRenderPassCreateInfo-pDependencies-parameter
  If `dependencyCount` is not `0`, `pDependencies` must be a valid pointer to an array of `dependencyCount` valid VkSubpassDependency structures

- VUID-VkRenderPassCreateInfo-subpassCount-arraylength
  `subpassCount` must be greater than `0`

Bits which can be set in VkRenderPassCreateInfo::`flags`, describing additional properties of the render pass, are:

    // Provided by VK_VERSION_1_0
    typedef enum VkRenderPassCreateFlagBits {
      // Provided by VK_QCOM_render_pass_transform
        VK_RENDER_PASS_CREATE_TRANSFORM_BIT_QCOM = 0x00000002,
    } VkRenderPassCreateFlagBits;

- `VK_RENDER_PASS_CREATE_TRANSFORM_BIT_QCOM` specifies that the created render pass is compatible with render pass transform.

    // Provided by VK_VERSION_1_0
    typedef VkFlags VkRenderPassCreateFlags;

`VkRenderPassCreateFlags` is a bitmask type for setting a mask of zero or more VkRenderPassCreateFlagBits.

If the VkRenderPassCreateInfo::`pNext` chain includes a `VkRenderPassMultiviewCreateInfo` structure, then that structure includes an array of view masks, view offsets, and correlation masks for the render pass.

The `VkRenderPassMultiviewCreateInfo` structure is defined as:

    // Provided by VK_VERSION_1_1
    typedef struct VkRenderPassMultiviewCreateInfo {
        VkStructureType    sType;
        const void*        pNext;
        uint32_t           subpassCount;
        const uint32_t*    pViewMasks;
        uint32_t           dependencyCount;
        const int32_t*     pViewOffsets;
        uint32_t           correlationMaskCount;
        const uint32_t*    pCorrelationMasks;
    } VkRenderPassMultiviewCreateInfo;

or the equivalent

    // Provided by VK_KHR_multiview
    typedef VkRenderPassMultiviewCreateInfo VkRenderPassMultiviewCreateInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `subpassCount` is zero or the number of subpasses in the render pass.

- `pViewMasks` is a pointer to an array of `subpassCount` view masks, where each mask is a bitfield of view indices describing which views rendering is broadcast to in each subpass, when multiview is enabled. If `subpassCount` is zero, each view mask is treated as zero.

- `dependencyCount` is zero or the number of dependencies in the render pass.

- `pViewOffsets` is a pointer to an array of `dependencyCount` view offsets, one for each dependency. If `dependencyCount` is zero, each dependency’s view offset is treated as zero. Each view offset controls which views in the source subpass the views in the destination subpass depend on.

- `correlationMaskCount` is zero or the number of correlation masks.

- `pCorrelationMasks` is a pointer to an array of `correlationMaskCount` view masks indicating sets of views that may be more efficient to render concurrently.

When a subpass uses a non-zero view mask, multiview functionality is considered to be enabled. Multiview is all-or-nothing for a render pass - that is, either all subpasses must have a non-zero view mask (though some subpasses may have only one view) or all must be zero. Multiview causes all drawing and clear commands in the subpass to behave as if they were broadcast to each view, where a view is represented by one layer of the framebuffer attachments. All draws and clears are broadcast to each view index whose bit is set in the view mask. The view index is provided in the `ViewIndex` shader input variable, and color, depth/stencil, and input attachments all read/write the layer of the framebuffer corresponding to the view index.

If the view mask is zero for all subpasses, multiview is considered to be disabled and all drawing commands execute normally, without this additional broadcasting.

Some implementations may not support multiview in conjunction with mesh shaders, geometry shaders or tessellation shaders.

When multiview is enabled, the `VK_DEPENDENCY_VIEW_LOCAL_BIT` bit in a dependency can be used to express a view-local dependency, meaning that each view in the destination subpass depends on a single view in the source subpass. Unlike pipeline barriers, a subpass dependency can potentially have a different view mask in the source subpass and the destination subpass. If the dependency is view-local, then each view (dstView) in the destination subpass depends on the view dstView + `pViewOffsets`[dependency] in the source subpass. If there is not such a view in the source subpass, then this dependency does not affect that view in the destination subpass. If the dependency is not view-local, then all views in the destination subpass depend on all views in the source subpass, and the view offset is ignored. A non-zero view offset is not allowed in a self-dependency.

The elements of `pCorrelationMasks` are a set of masks of views indicating that views in the same mask may exhibit spatial coherency between the views, making it more efficient to render them concurrently. Correlation masks must not have a functional effect on the results of the multiview rendering.

When multiview is enabled, at the beginning of each subpass all non-render pass state is undefined. In particular, each time vkCmdBeginRenderPass or vkCmdNextSubpass is called the graphics pipeline must be bound, any relevant descriptor sets or vertex/index buffers must be bound, and any relevant dynamic state or push constants must be set before they are used.

A multiview subpass can declare that its shaders will write per-view attributes for all views in a single invocation, by setting the `VK_SUBPASS_DESCRIPTION_PER_VIEW_ATTRIBUTES_BIT_NVX` bit in the subpass description. The only supported per-view attributes are position and viewport mask, and per-view position and viewport masks are written to output array variables decorated with `PositionPerViewNV` and `ViewportMaskPerViewNV`, respectively. If the `VK_NV_viewport_array2` extension is not supported and enabled, `ViewportMaskPerViewNV` must not be used. Values written to elements of `PositionPerViewNV` and `ViewportMaskPerViewNV` must not depend on the `ViewIndex`. The shader must also write to an output variable decorated with `Position`, and the value written to `Position` must equal the value written to `PositionPerViewNV`[`ViewIndex`]. Similarly, if `ViewportMaskPerViewNV` is written to then the shader must also write to an output variable decorated with `ViewportMaskNV`, and the value written to `ViewportMaskNV` must equal the value written to `ViewportMaskPerViewNV`[`ViewIndex`]. Implementations will either use values taken from `Position` and `ViewportMaskNV` and invoke the shader once for each view, or will use values taken from `PositionPerViewNV` and `ViewportMaskPerViewNV` and invoke the shader fewer times. The values written to `Position` and `ViewportMaskNV` must not depend on the values written to `PositionPerViewNV` and `ViewportMaskPerViewNV`, or vice versa (to allow compilers to eliminate the unused outputs). All attributes that do not have `*PerViewNV` counterparts must not depend on `ViewIndex`.

Per-view attributes are all-or-nothing for a subpass. That is, all pipelines compiled against a subpass that includes the `VK_SUBPASS_DESCRIPTION_PER_VIEW_ATTRIBUTES_BIT_NVX` bit must write per-view attributes to the `*PerViewNV[]` shader outputs, in addition to the non-per-view (e.g. `Position`) outputs. Pipelines compiled against a subpass that does not include this bit must not include the `*PerViewNV[]` outputs in their interfaces.

Valid Usage

- VUID-VkRenderPassMultiviewCreateInfo-pCorrelationMasks-00841
  Each view index must not be set in more than one element of `pCorrelationMasks`

- VUID-VkRenderPassMultiviewCreateInfo-multiview-06555
  If the `multiview` feature is not enabled, each element of `pViewMasks` must be `0`

- VUID-VkRenderPassMultiviewCreateInfo-pViewMasks-06697
  The index of the most significant bit in each element of `pViewMasks` must be less than `maxMultiviewViewCount`

Valid Usage (Implicit)

- VUID-VkRenderPassMultiviewCreateInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_MULTIVIEW_CREATE_INFO`

- VUID-VkRenderPassMultiviewCreateInfo-pViewMasks-parameter
  If `subpassCount` is not `0`, `pViewMasks` must be a valid pointer to an array of `subpassCount` `uint32_t` values

- VUID-VkRenderPassMultiviewCreateInfo-pViewOffsets-parameter
  If `dependencyCount` is not `0`, `pViewOffsets` must be a valid pointer to an array of `dependencyCount` `int32_t` values

- VUID-VkRenderPassMultiviewCreateInfo-pCorrelationMasks-parameter
  If `correlationMaskCount` is not `0`, `pCorrelationMasks` must be a valid pointer to an array of `correlationMaskCount` `uint32_t` values

The `VkMultiviewPerViewAttributesInfoNVX` structure is defined as:

    // Provided by VK_NVX_multiview_per_view_attributes with VK_VERSION_1_3 or VK_KHR_dynamic_rendering
    typedef struct VkMultiviewPerViewAttributesInfoNVX {
        VkStructureType    sType;
        const void*        pNext;
        VkBool32           perViewAttributes;
        VkBool32           perViewAttributesPositionXOnly;
    } VkMultiviewPerViewAttributesInfoNVX;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `perViewAttributes` specifies that shaders compiled for this pipeline write the attributes for all views in a single invocation of each vertex processing stage. All pipelines executed within a render pass instance that includes this bit must write per-view attributes to the `*PerViewNV[]` shader outputs, in addition to the non-per-view (e.g. `Position`) outputs.

- `perViewAttributesPositionXOnly` specifies that shaders compiled for this pipeline use per-view positions which only differ in value in the x component. Per-view viewport mask can also be used.

When dynamic render pass instances are being used, instead of specifying `VK_SUBPASS_DESCRIPTION_PER_VIEW_ATTRIBUTES_BIT_NVX` or `VK_SUBPASS_DESCRIPTION_PER_VIEW_POSITION_X_ONLY_BIT_NVX` in the subpass description flags, the per-attribute properties of the render pass instance must be specified by the `VkMultiviewPerViewAttributesInfoNVX` structure Include the `VkMultiviewPerViewAttributesInfoNVX` structure in the `pNext` chain of VkGraphicsPipelineCreateInfo when creating a graphics pipeline for dynamic rendering, VkRenderingInfo when starting a dynamic render pass instance, and VkCommandBufferInheritanceInfo when specifying the dynamic render pass instance parameters for secondary command buffers.

Valid Usage (Implicit)

- VUID-VkMultiviewPerViewAttributesInfoNVX-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_MULTIVIEW_PER_VIEW_ATTRIBUTES_INFO_NVX`

If the VkRenderPassCreateInfo::`pNext` chain includes a `VkRenderPassFragmentDensityMapCreateInfoEXT` structure, then that structure includes a fragment density map attachment for the render pass.

The `VkRenderPassFragmentDensityMapCreateInfoEXT` structure is defined as:

    // Provided by VK_EXT_fragment_density_map
    typedef struct VkRenderPassFragmentDensityMapCreateInfoEXT {
        VkStructureType          sType;
        const void*              pNext;
        VkAttachmentReference    fragmentDensityMapAttachment;
    } VkRenderPassFragmentDensityMapCreateInfoEXT;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `fragmentDensityMapAttachment` is the fragment density map to use for the render pass.

The fragment density map is read at an implementation-dependent time with the following constraints determined by the attachment’s image view `flags`:

- `VK_IMAGE_VIEW_CREATE_FRAGMENT_DENSITY_MAP_DYNAMIC_BIT_EXT` specifies that the fragment density map will be read by the device during `VK_PIPELINE_STAGE_FRAGMENT_DENSITY_PROCESS_BIT_EXT`

- `VK_IMAGE_VIEW_CREATE_FRAGMENT_DENSITY_MAP_DEFERRED_BIT_EXT` specifies that the fragment density map will be read by the host during vkEndCommandBuffer of the primary command buffer that the render pass is recorded into

- Otherwise the fragment density map will be read by the host during vkCmdBeginRenderPass

The fragment density map may additionally be read by the device during `VK_PIPELINE_STAGE_FRAGMENT_DENSITY_PROCESS_BIT_EXT` for any mode.

If this structure is not present, it is as if `fragmentDensityMapAttachment` was given as `VK_ATTACHMENT_UNUSED`.

Valid Usage

- VUID-VkRenderPassFragmentDensityMapCreateInfoEXT-fragmentDensityMapAttachment-02548
  If `fragmentDensityMapAttachment` is not `VK_ATTACHMENT_UNUSED`, `fragmentDensityMapAttachment` must not be an element of `VkSubpassDescription`::`pInputAttachments`, `VkSubpassDescription`::`pColorAttachments`, `VkSubpassDescription`::`pResolveAttachments`, `VkSubpassDescription`::`pDepthStencilAttachment`, or `VkSubpassDescription`::`pPreserveAttachments` for any subpass

- VUID-VkRenderPassFragmentDensityMapCreateInfoEXT-fragmentDensityMapAttachment-02549
  If `fragmentDensityMapAttachment` is not `VK_ATTACHMENT_UNUSED`, `layout` must be equal to `VK_IMAGE_LAYOUT_FRAGMENT_DENSITY_MAP_OPTIMAL_EXT`, or `VK_IMAGE_LAYOUT_GENERAL`

- VUID-VkRenderPassFragmentDensityMapCreateInfoEXT-fragmentDensityMapAttachment-02550
  If `fragmentDensityMapAttachment` is not `VK_ATTACHMENT_UNUSED`, `fragmentDensityMapAttachment` must reference an attachment with a `loadOp` equal to `VK_ATTACHMENT_LOAD_OP_LOAD` or `VK_ATTACHMENT_LOAD_OP_DONT_CARE`

- VUID-VkRenderPassFragmentDensityMapCreateInfoEXT-fragmentDensityMapAttachment-02551
  If `fragmentDensityMapAttachment` is not `VK_ATTACHMENT_UNUSED`, `fragmentDensityMapAttachment` must reference an attachment with a `storeOp` equal to `VK_ATTACHMENT_STORE_OP_DONT_CARE`

Valid Usage (Implicit)

- VUID-VkRenderPassFragmentDensityMapCreateInfoEXT-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_FRAGMENT_DENSITY_MAP_CREATE_INFO_EXT`

- VUID-VkRenderPassFragmentDensityMapCreateInfoEXT-fragmentDensityMapAttachment-parameter
  `fragmentDensityMapAttachment` must be a valid VkAttachmentReference structure

The `VkAttachmentDescription` structure is defined as:

    // Provided by VK_VERSION_1_0
    typedef struct VkAttachmentDescription {
        VkAttachmentDescriptionFlags    flags;
        VkFormat                        format;
        VkSampleCountFlagBits           samples;
        VkAttachmentLoadOp              loadOp;
        VkAttachmentStoreOp             storeOp;
        VkAttachmentLoadOp              stencilLoadOp;
        VkAttachmentStoreOp             stencilStoreOp;
        VkImageLayout                   initialLayout;
        VkImageLayout                   finalLayout;
    } VkAttachmentDescription;

- `flags` is a bitmask of VkAttachmentDescriptionFlagBits specifying additional properties of the attachment.

- `format` is a VkFormat value specifying the format of the image view that will be used for the attachment.

- `samples` is a VkSampleCountFlagBits value specifying the number of samples of the image.

- `loadOp` is a VkAttachmentLoadOp value specifying how the contents of color and depth components of the attachment are treated at the beginning of the subpass where it is first used.

- `storeOp` is a VkAttachmentStoreOp value specifying how the contents of color and depth components of the attachment are treated at the end of the subpass where it is last used.

- `stencilLoadOp` is a VkAttachmentLoadOp value specifying how the contents of stencil components of the attachment are treated at the beginning of the subpass where it is first used.

- `stencilStoreOp` is a VkAttachmentStoreOp value specifying how the contents of stencil components of the attachment are treated at the end of the last subpass where it is used.

- `initialLayout` is the layout the attachment image subresource will be in when a render pass instance begins.

- `finalLayout` is the layout the attachment image subresource will be transitioned to when a render pass instance ends.

If the attachment uses a color format, then `loadOp` and `storeOp` are used, and `stencilLoadOp` and `stencilStoreOp` are ignored. If the format has depth and/or stencil components, `loadOp` and `storeOp` apply only to the depth data, while `stencilLoadOp` and `stencilStoreOp` define how the stencil data is handled. `loadOp` and `stencilLoadOp` define the load operations for the attachment. `storeOp` and `stencilStoreOp` define the store operations for the attachment. If an attachment is not used by any subpass, `loadOp`, `storeOp`, `stencilStoreOp`, and `stencilLoadOp` will be ignored for that attachment, and no load or store ops will be performed. However, any transition specified by `initialLayout` and `finalLayout` will still be executed.

If `flags` includes `VK_ATTACHMENT_DESCRIPTION_MAY_ALIAS_BIT`, then the attachment is treated as if it shares physical memory with another attachment in the same render pass. This information limits the ability of the implementation to reorder certain operations (like layout transitions and the `loadOp`) such that it is not improperly reordered against other uses of the same physical memory via a different attachment. This is described in more detail below.

If a render pass uses multiple attachments that alias the same device memory, those attachments must each include the `VK_ATTACHMENT_DESCRIPTION_MAY_ALIAS_BIT` bit in their attachment description flags. Attachments aliasing the same memory occurs in multiple ways:

- Multiple attachments being assigned the same image view as part of framebuffer creation.

- Attachments using distinct image views that correspond to the same image subresource of an image.

- Attachments using views of distinct image subresources which are bound to overlapping memory ranges.

Note | Render passes must include subpass dependencies (either directly or via a subpass dependency chain) between any two subpasses that operate on the same attachment or aliasing attachments and those subpass dependencies must include execution and memory dependencies separating uses of the aliases, if at least one of those subpasses writes to one of the aliases. These dependencies must not include the `VK_DEPENDENCY_BY_REGION_BIT` if the aliases are views of distinct image subresources which overlap in memory.

Multiple attachments that alias the same memory must not be used in a single subpass. A given attachment index must not be used multiple times in a single subpass, with one exception: two subpass attachments can use the same attachment index if at least one use is as an input attachment and neither use is as a resolve or preserve attachment. In other words, the same view can be used simultaneously as an input and color or depth/stencil attachment, but must not be used as multiple color or depth/stencil attachments nor as resolve or preserve attachments.

If a set of attachments alias each other, then all except the first to be used in the render pass must use an `initialLayout` of `VK_IMAGE_LAYOUT_UNDEFINED`, since the earlier uses of the other aliases make their contents undefined. Once an alias has been used and a different alias has been used after it, the first alias must not be used in any later subpasses. However, an application can assign the same image view to multiple aliasing attachment indices, which allows that image view to be used multiple times even if other aliases are used in between.

Note | Once an attachment needs the `VK_ATTACHMENT_DESCRIPTION_MAY_ALIAS_BIT` bit, there should be no additional cost of introducing additional aliases, and using these additional aliases may allow more efficient clearing of the attachments on multiple uses via `VK_ATTACHMENT_LOAD_OP_CLEAR`.

Valid Usage

- VUID-VkAttachmentDescription-format-06699
  If `format` includes a color or depth component and `loadOp` is `VK_ATTACHMENT_LOAD_OP_LOAD`, then `initialLayout` must not be `VK_IMAGE_LAYOUT_UNDEFINED`

- VUID-VkAttachmentDescription-finalLayout-00843
  `finalLayout` must not be `VK_IMAGE_LAYOUT_UNDEFINED` or `VK_IMAGE_LAYOUT_PREINITIALIZED`

- VUID-VkAttachmentDescription-format-03280
  If `format` is a color format, `initialLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription-format-03281
  If `format` is a depth/stencil format, `initialLayout` must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL`

- VUID-VkAttachmentDescription-format-03282
  If `format` is a color format, `finalLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription-format-03283
  If `format` is a depth/stencil format, `finalLayout` must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL`

- VUID-VkAttachmentDescription-format-06487
  If `format` is a color format, `initialLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkAttachmentDescription-format-06488
  If `format` is a color format, `finalLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkAttachmentDescription-separateDepthStencilLayouts-03284
  If the `separateDepthStencilLayouts` feature is not enabled, `initialLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`,

- VUID-VkAttachmentDescription-separateDepthStencilLayouts-03285
  If the `separateDepthStencilLayouts` feature is not enabled, `finalLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`,

- VUID-VkAttachmentDescription-format-03286
  If `format` is a color format, `initialLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription-format-03287
  If `format` is a color format, `finalLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription-format-06906
  If `format` is a depth/stencil format which includes both depth and stencil components, `initialLayout` must not be `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription-format-06907
  If `format` is a depth/stencil format which includes both depth and stencil components, `finalLayout` must not be `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription-format-03290
  If `format` is a depth/stencil format which includes only the depth component, `initialLayout` must not be `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription-format-03291
  If `format` is a depth/stencil format which includes only the depth component, `finalLayout` must not be `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription-synchronization2-06908
  If the `synchronization2` feature is not enabled, `initialLayout` must not be `VK_IMAGE_LAYOUT_ATTACHMENT_OPTIMAL_KHR` or `VK_IMAGE_LAYOUT_READ_ONLY_OPTIMAL_KHR`

- VUID-VkAttachmentDescription-synchronization2-06909
  If the `synchronization2` feature is not enabled, `finalLayout` must not be `VK_IMAGE_LAYOUT_ATTACHMENT_OPTIMAL_KHR` or `VK_IMAGE_LAYOUT_READ_ONLY_OPTIMAL_KHR`

- VUID-VkAttachmentDescription-attachmentFeedbackLoopLayout-07309
  If the `attachmentFeedbackLoopLayout` feature is not enabled, `initialLayout` must not be `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT`

- VUID-VkAttachmentDescription-attachmentFeedbackLoopLayout-07310
  If the `attachmentFeedbackLoopLayout` feature is not enabled, `finalLayout` must not be `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT`

- VUID-VkAttachmentDescription-samples-08745
  `samples` must be a valid VkSampleCountFlagBits value that is set in `imageCreateSampleCounts` (as defined in Image Creation Limits) for the given `format`

- VUID-VkAttachmentDescription-dynamicRenderingLocalRead-09544
  If the `dynamicRenderingLocalRead` feature is not enabled, `initialLayout` must not be `VK_IMAGE_LAYOUT_RENDERING_LOCAL_READ`

- VUID-VkAttachmentDescription-dynamicRenderingLocalRead-09545
  If the `dynamicRenderingLocalRead` feature is not enabled, `finalLayout` must not be `VK_IMAGE_LAYOUT_RENDERING_LOCAL_READ`

- VUID-VkAttachmentDescription-format-06698
  `format` must not be VK_FORMAT_UNDEFINED

- VUID-VkAttachmentDescription-format-06700
  If `format` includes a stencil component and `stencilLoadOp` is `VK_ATTACHMENT_LOAD_OP_LOAD`, then `initialLayout` must not be `VK_IMAGE_LAYOUT_UNDEFINED`

- VUID-VkAttachmentDescription-format-03292
  If `format` is a depth/stencil format which includes only the stencil component, `initialLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription-format-03293
  If `format` is a depth/stencil format which includes only the stencil component, `finalLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription-format-06242
  If `format` is a depth/stencil format which includes both depth and stencil components, `initialLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription-format-06243
  If `format` is a depth/stencil format which includes both depth and stencil components, `finalLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`

Valid Usage (Implicit)

- VUID-VkAttachmentDescription-flags-parameter
  `flags` must be a valid combination of VkAttachmentDescriptionFlagBits values

- VUID-VkAttachmentDescription-format-parameter
  `format` must be a valid VkFormat value

- VUID-VkAttachmentDescription-samples-parameter
  `samples` must be a valid VkSampleCountFlagBits value

- VUID-VkAttachmentDescription-loadOp-parameter
  `loadOp` must be a valid VkAttachmentLoadOp value

- VUID-VkAttachmentDescription-storeOp-parameter
  `storeOp` must be a valid VkAttachmentStoreOp value

- VUID-VkAttachmentDescription-stencilLoadOp-parameter
  `stencilLoadOp` must be a valid VkAttachmentLoadOp value

- VUID-VkAttachmentDescription-stencilStoreOp-parameter
  `stencilStoreOp` must be a valid VkAttachmentStoreOp value

- VUID-VkAttachmentDescription-initialLayout-parameter
  `initialLayout` must be a valid VkImageLayout value

- VUID-VkAttachmentDescription-finalLayout-parameter
  `finalLayout` must be a valid VkImageLayout value

Bits which can be set in VkAttachmentDescription::`flags`, describing additional properties of the attachment, are:

    // Provided by VK_VERSION_1_0
    typedef enum VkAttachmentDescriptionFlagBits {
        VK_ATTACHMENT_DESCRIPTION_MAY_ALIAS_BIT = 0x00000001,
    } VkAttachmentDescriptionFlagBits;

- `VK_ATTACHMENT_DESCRIPTION_MAY_ALIAS_BIT` specifies that the attachment aliases the same device memory as other attachments.

    // Provided by VK_VERSION_1_0
    typedef VkFlags VkAttachmentDescriptionFlags;

`VkAttachmentDescriptionFlags` is a bitmask type for setting a mask of zero or more VkAttachmentDescriptionFlagBits.

The `VkRenderPassInputAttachmentAspectCreateInfo` structure is defined as:

    // Provided by VK_VERSION_1_1
    typedef struct VkRenderPassInputAttachmentAspectCreateInfo {
        VkStructureType                            sType;
        const void*                                pNext;
        uint32_t                                   aspectReferenceCount;
        const VkInputAttachmentAspectReference*    pAspectReferences;
    } VkRenderPassInputAttachmentAspectCreateInfo;

or the equivalent

    // Provided by VK_KHR_maintenance2
    typedef VkRenderPassInputAttachmentAspectCreateInfo VkRenderPassInputAttachmentAspectCreateInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `aspectReferenceCount` is the number of elements in the `pAspectReferences` array.

- `pAspectReferences` is a pointer to an array of `aspectReferenceCount` VkInputAttachmentAspectReference structures containing a mask describing which aspect(s) can be accessed for a given input attachment within a given subpass.

To specify which aspects of an input attachment can be read, add a VkRenderPassInputAttachmentAspectCreateInfo structure to the `pNext` chain of the VkRenderPassCreateInfo structure:

An application can access any aspect of an input attachment that does not have a specified aspect mask in the `pAspectReferences` array. Otherwise, an application must not access aspect(s) of an input attachment other than those in its specified aspect mask.

Valid Usage (Implicit)

- VUID-VkRenderPassInputAttachmentAspectCreateInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_INPUT_ATTACHMENT_ASPECT_CREATE_INFO`

- VUID-VkRenderPassInputAttachmentAspectCreateInfo-pAspectReferences-parameter
  `pAspectReferences` must be a valid pointer to an array of `aspectReferenceCount` valid VkInputAttachmentAspectReference structures

- VUID-VkRenderPassInputAttachmentAspectCreateInfo-aspectReferenceCount-arraylength
  `aspectReferenceCount` must be greater than `0`

The `VkInputAttachmentAspectReference` structure is defined as:

    // Provided by VK_VERSION_1_1
    typedef struct VkInputAttachmentAspectReference {
        uint32_t              subpass;
        uint32_t              inputAttachmentIndex;
        VkImageAspectFlags    aspectMask;
    } VkInputAttachmentAspectReference;

or the equivalent

    // Provided by VK_KHR_maintenance2
    typedef VkInputAttachmentAspectReference VkInputAttachmentAspectReferenceKHR;

- `subpass` is an index into the `pSubpasses` array of the parent `VkRenderPassCreateInfo` structure.

- `inputAttachmentIndex` is an index into the `pInputAttachments` of the specified subpass.

- `aspectMask` is a mask of which aspect(s) can be accessed within the specified subpass.

This structure specifies an aspect mask for a specific input attachment of a specific subpass in the render pass.

`subpass` and `inputAttachmentIndex` index into the render pass as:

    pCreateInfo->pSubpasses[subpass].pInputAttachments[inputAttachmentIndex]

Valid Usage

- VUID-VkInputAttachmentAspectReference-aspectMask-01964
  `aspectMask` must not include `VK_IMAGE_ASPECT_METADATA_BIT`

- VUID-VkInputAttachmentAspectReference-aspectMask-02250
  `aspectMask` must not include `VK_IMAGE_ASPECT_MEMORY_PLANE_i_BIT_EXT` for any index i

Valid Usage (Implicit)

- VUID-VkInputAttachmentAspectReference-aspectMask-parameter
  `aspectMask` must be a valid combination of VkImageAspectFlagBits values

- VUID-VkInputAttachmentAspectReference-aspectMask-requiredbitmask
  `aspectMask` must not be `0`

The `VkSubpassDescription` structure is defined as:

    // Provided by VK_VERSION_1_0
    typedef struct VkSubpassDescription {
        VkSubpassDescriptionFlags       flags;
        VkPipelineBindPoint             pipelineBindPoint;
        uint32_t                        inputAttachmentCount;
        const VkAttachmentReference*    pInputAttachments;
        uint32_t                        colorAttachmentCount;
        const VkAttachmentReference*    pColorAttachments;
        const VkAttachmentReference*    pResolveAttachments;
        const VkAttachmentReference*    pDepthStencilAttachment;
        uint32_t                        preserveAttachmentCount;
        const uint32_t*                 pPreserveAttachments;
    } VkSubpassDescription;

- `flags` is a bitmask of VkSubpassDescriptionFlagBits specifying usage of the subpass.

- `pipelineBindPoint` is a VkPipelineBindPoint value specifying the pipeline type supported for this subpass.

- `inputAttachmentCount` is the number of input attachments.

- `pInputAttachments` is a pointer to an array of VkAttachmentReference structures defining the input attachments for this subpass and their layouts.

- `colorAttachmentCount` is the number of color attachments.

- `pColorAttachments` is a pointer to an array of `colorAttachmentCount` VkAttachmentReference structures defining the color attachments for this subpass and their layouts.

- `pResolveAttachments` is `NULL` or a pointer to an array of `colorAttachmentCount` VkAttachmentReference structures defining the resolve attachments for this subpass and their layouts.

- `pDepthStencilAttachment` is a pointer to a VkAttachmentReference structure specifying the depth/stencil attachment for this subpass and its layout.

- `preserveAttachmentCount` is the number of preserved attachments.

- `pPreserveAttachments` is a pointer to an array of `preserveAttachmentCount` render pass attachment indices identifying attachments that are not used by this subpass, but whose contents must be preserved throughout the subpass.

Each element of the `pInputAttachments` array corresponds to an input attachment index in a fragment shader, i.e. if a shader declares an image variable decorated with a `InputAttachmentIndex` value of X, then it uses the attachment provided in `pInputAttachments`[X]. Input attachments must also be bound to the pipeline in a descriptor set. If the `attachment` member of any element of `pInputAttachments` is `VK_ATTACHMENT_UNUSED`, the application must not read from the corresponding input attachment index. Fragment shaders can use subpass input variables to access the contents of an input attachment at the fragment’s (xf,yf) framebuffer coordinates and layer. Input attachments must not be used by any subpasses within a render pass that enables render pass transform.

Each element of the `pColorAttachments` array corresponds to an output location in the shader, i.e. if the shader declares an output variable decorated with a `Location` value of X, then it uses the attachment provided in `pColorAttachments`[X]. If the `attachment` member of any element of `pColorAttachments` is `VK_ATTACHMENT_UNUSED`, or if Color Write Enable has been disabled for the corresponding attachment index, then writes to the corresponding location by a fragment shader are discarded.

If `flags` does not include `VK_SUBPASS_DESCRIPTION_SHADER_RESOLVE_BIT_QCOM`, and if `pResolveAttachments` is not `NULL`, each of its elements corresponds to a color attachment (the element in `pColorAttachments` at the same index), and a multisample resolve operation is defined for each attachment unless the resolve attachment index is `VK_ATTACHMENT_UNUSED`.

Similarly, if `flags` does not include `VK_SUBPASS_DESCRIPTION_SHADER_RESOLVE_BIT_QCOM`, and VkSubpassDescriptionDepthStencilResolve::`pDepthStencilResolveAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED`, it corresponds to the depth/stencil attachment in `pDepthStencilAttachment`, and multisample resolve operation for depth and stencil are defined by VkSubpassDescriptionDepthStencilResolve::`depthResolveMode` and VkSubpassDescriptionDepthStencilResolve::`stencilResolveMode`, respectively. If VkSubpassDescriptionDepthStencilResolve::`depthResolveMode` is `VK_RESOLVE_MODE_NONE` or the `pDepthStencilResolveAttachment` does not have a depth aspect, no resolve operation is performed for the depth attachment. If VkSubpassDescriptionDepthStencilResolve::`stencilResolveMode` is `VK_RESOLVE_MODE_NONE` or the `pDepthStencilResolveAttachment` does not have a stencil aspect, no resolve operation is performed for the stencil attachment.

If the image subresource range referenced by the depth/stencil attachment is created with `VK_IMAGE_CREATE_SAMPLE_LOCATIONS_COMPATIBLE_DEPTH_BIT_EXT`, then the multisample resolve operation uses the sample locations state specified in the `sampleLocationsInfo` member of the element of the `VkRenderPassSampleLocationsBeginInfoEXT`::`pPostSubpassSampleLocations` for the subpass.

If `pDepthStencilAttachment` is `NULL`, or if its attachment index is `VK_ATTACHMENT_UNUSED`, it indicates that no depth/stencil attachment will be used in the subpass.

The contents of an attachment within the render area become undefined at the start of a subpass S if all of the following conditions are true:

- The attachment is used as a color, depth/stencil, or resolve attachment in any subpass in the render pass.

- There is a subpass S1 that uses or preserves the attachment, and a subpass dependency from S1 to S.

- The attachment is not used or preserved in subpass S.

In addition, the contents of an attachment within the render area become undefined at the start of a subpass S if all of the following conditions are true:

- `VK_SUBPASS_DESCRIPTION_SHADER_RESOLVE_BIT_QCOM` is set.

- The attachment is used as a color or depth/stencil in the subpass.

Once the contents of an attachment become undefined in subpass S, they remain undefined for subpasses in subpass dependency chains starting with subpass S until they are written again. However, they remain valid for subpasses in other subpass dependency chains starting with subpass S1 if those subpasses use or preserve the attachment.

Valid Usage

- VUID-VkSubpassDescription-attachment-06912
  If the `attachment` member of an element of `pInputAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkSubpassDescription-attachment-06913
  If the `attachment` member of an element of `pColorAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL`

- VUID-VkSubpassDescription-attachment-06914
  If the `attachment` member of an element of `pResolveAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL`

- VUID-VkSubpassDescription-attachment-06915
  If the `attachment` member of `pDepthStencilAttachment` is not `VK_ATTACHMENT_UNUSED`, ts `layout` member must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL`

- VUID-VkSubpassDescription-attachment-06916
  If the `attachment` member of an element of `pColorAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkSubpassDescription-attachment-06917
  If the `attachment` member of an element of `pResolveAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkSubpassDescription-attachment-06918
  If the `attachment` member of an element of `pInputAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkSubpassDescription-attachment-06919
  If the `attachment` member of an element of `pColorAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkSubpassDescription-attachment-06920
  If the `attachment` member of an element of `pResolveAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkSubpassDescription-attachment-06921
  If the `attachment` member of an element of `pInputAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_ATTACHMENT_OPTIMAL_KHR`

- VUID-VkSubpassDescription-attachment-06922
  If the `attachment` member of an element of `pColorAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_READ_ONLY_OPTIMAL_KHR`

- VUID-VkSubpassDescription-attachment-06923
  If the `attachment` member of an element of `pResolveAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_READ_ONLY_OPTIMAL_KHR`

- VUID-VkSubpassDescription-pipelineBindPoint-04952
  `pipelineBindPoint` must be `VK_PIPELINE_BIND_POINT_GRAPHICS` or `VK_PIPELINE_BIND_POINT_SUBPASS_SHADING_HUAWEI`

- VUID-VkSubpassDescription-colorAttachmentCount-00845
  `colorAttachmentCount` must be less than or equal to `VkPhysicalDeviceLimits`::`maxColorAttachments`

- VUID-VkSubpassDescription-loadOp-00846
  If the first use of an attachment in this render pass is as an input attachment, and the attachment is not also used as a color or depth/stencil attachment in the same subpass, then `loadOp` must not be `VK_ATTACHMENT_LOAD_OP_CLEAR`

- VUID-VkSubpassDescription-pResolveAttachments-00847
  If `pResolveAttachments` is not `NULL`, for each resolve attachment that is not `VK_ATTACHMENT_UNUSED`, the corresponding color attachment must not be `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescription-pResolveAttachments-00848
  If `pResolveAttachments` is not `NULL`, for each resolve attachment that is not `VK_ATTACHMENT_UNUSED`, the corresponding color attachment must not have a sample count of `VK_SAMPLE_COUNT_1_BIT`

- VUID-VkSubpassDescription-pResolveAttachments-00849
  If `pResolveAttachments` is not `NULL`, each resolve attachment that is not `VK_ATTACHMENT_UNUSED` must have a sample count of `VK_SAMPLE_COUNT_1_BIT`

- VUID-VkSubpassDescription-pResolveAttachments-00850
  If `pResolveAttachments` is not `NULL`, each resolve attachment that is not `VK_ATTACHMENT_UNUSED` must have the same VkFormat as its corresponding color attachment

- VUID-VkSubpassDescription-pColorAttachments-09430
  All attachments in `pColorAttachments` that are not `VK_ATTACHMENT_UNUSED` must have the same sample count

- VUID-VkSubpassDescription-pInputAttachments-02647
  All attachments in `pInputAttachments` that are not `VK_ATTACHMENT_UNUSED` must have image formats whose potential format features contain at least `VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT` or `VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkSubpassDescription-pColorAttachments-02648
  All attachments in `pColorAttachments` that are not `VK_ATTACHMENT_UNUSED` must have image formats whose potential format features contain `VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT`

- VUID-VkSubpassDescription-pResolveAttachments-02649
  All attachments in `pResolveAttachments` that are not `VK_ATTACHMENT_UNUSED` must have image formats whose potential format features contain `VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT`

- VUID-VkSubpassDescription-pDepthStencilAttachment-02650
  If `pDepthStencilAttachment` is not `NULL` and the attachment is not `VK_ATTACHMENT_UNUSED` then it must have an image format whose potential format features contain `VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkSubpassDescription-linearColorAttachment-06496
  If the `linearColorAttachment` feature is enabled and the image is created with `VK_IMAGE_TILING_LINEAR`, all attachments in `pInputAttachments` that are not `VK_ATTACHMENT_UNUSED` must have image formats whose potential format features must contain `VK_FORMAT_FEATURE_2_LINEAR_COLOR_ATTACHMENT_BIT_NV`

- VUID-VkSubpassDescription-linearColorAttachment-06497
  If the `linearColorAttachment` feature is enabled and the image is created with `VK_IMAGE_TILING_LINEAR`, all attachments in `pColorAttachments` that are not `VK_ATTACHMENT_UNUSED` must have image formats whose potential format features must contain `VK_FORMAT_FEATURE_2_LINEAR_COLOR_ATTACHMENT_BIT_NV`

- VUID-VkSubpassDescription-linearColorAttachment-06498
  If the `linearColorAttachment` feature is enabled and the image is created with `VK_IMAGE_TILING_LINEAR`, all attachments in `pResolveAttachments` that are not `VK_ATTACHMENT_UNUSED` must have image formats whose potential format features must contain `VK_FORMAT_FEATURE_2_LINEAR_COLOR_ATTACHMENT_BIT_NV`

- VUID-VkSubpassDescription-None-09431
  If either of the following is enabled:

  - The `VK_AMD_mixed_attachment_samples` extension

  - The `VK_NV_framebuffer_mixed_samples` extension

  all attachments in `pColorAttachments` that are not `VK_ATTACHMENT_UNUSED` must have a sample count that is smaller than or equal to the sample count of `pDepthStencilAttachment` if it is not `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescription-pDepthStencilAttachment-01418
  If `pDepthStencilAttachment` is not `VK_ATTACHMENT_UNUSED` and any attachments in `pColorAttachments` are not `VK_ATTACHMENT_UNUSED`, they must have the same sample count , if none of the following are enabled:

  - The `VK_AMD_mixed_attachment_samples` extension

  - The `VK_NV_framebuffer_mixed_samples` extension

- VUID-VkSubpassDescription-attachment-00853
  Each element of `pPreserveAttachments` must not be `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescription-pPreserveAttachments-00854
  Each element of `pPreserveAttachments` must not also be an element of any other member of the subpass description

- VUID-VkSubpassDescription-layout-02519
  If any attachment is used by more than one VkAttachmentReference member, then each use must use the same `layout`

- VUID-VkSubpassDescription-flags-00856
  If `flags` includes `VK_SUBPASS_DESCRIPTION_PER_VIEW_POSITION_X_ONLY_BIT_NVX`, it must also include `VK_SUBPASS_DESCRIPTION_PER_VIEW_ATTRIBUTES_BIT_NVX`

- VUID-VkSubpassDescription-flags-03341
  If `flags` includes `VK_SUBPASS_DESCRIPTION_SHADER_RESOLVE_BIT_QCOM`, and if `pResolveAttachments` is not `NULL`, then each resolve attachment must be `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescription-flags-03343
  If `flags` includes `VK_SUBPASS_DESCRIPTION_SHADER_RESOLVE_BIT_QCOM`, then the subpass must be the last subpass in a subpass dependency chain

- VUID-VkSubpassDescription-pInputAttachments-02868
  If the render pass is created with `VK_RENDER_PASS_CREATE_TRANSFORM_BIT_QCOM` each of the elements of `pInputAttachments` must be `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescription-pDepthStencilAttachment-04438
  `pDepthStencilAttachment` and `pColorAttachments` must not contain references to the same attachment

Valid Usage (Implicit)

- VUID-VkSubpassDescription-flags-parameter
  `flags` must be a valid combination of VkSubpassDescriptionFlagBits values

- VUID-VkSubpassDescription-pipelineBindPoint-parameter
  `pipelineBindPoint` must be a valid VkPipelineBindPoint value

- VUID-VkSubpassDescription-pInputAttachments-parameter
  If `inputAttachmentCount` is not `0`, `pInputAttachments` must be a valid pointer to an array of `inputAttachmentCount` valid VkAttachmentReference structures

- VUID-VkSubpassDescription-pColorAttachments-parameter
  If `colorAttachmentCount` is not `0`, `pColorAttachments` must be a valid pointer to an array of `colorAttachmentCount` valid VkAttachmentReference structures

- VUID-VkSubpassDescription-pResolveAttachments-parameter
  If `colorAttachmentCount` is not `0`, and `pResolveAttachments` is not `NULL`, `pResolveAttachments` must be a valid pointer to an array of `colorAttachmentCount` valid VkAttachmentReference structures

- VUID-VkSubpassDescription-pDepthStencilAttachment-parameter
  If `pDepthStencilAttachment` is not `NULL`, `pDepthStencilAttachment` must be a valid pointer to a valid VkAttachmentReference structure

- VUID-VkSubpassDescription-pPreserveAttachments-parameter
  If `preserveAttachmentCount` is not `0`, `pPreserveAttachments` must be a valid pointer to an array of `preserveAttachmentCount` `uint32_t` values

Bits which can be set in VkSubpassDescription::`flags`, specifying usage of the subpass, are:

    // Provided by VK_VERSION_1_0
    typedef enum VkSubpassDescriptionFlagBits {
      // Provided by VK_NVX_multiview_per_view_attributes
        VK_SUBPASS_DESCRIPTION_PER_VIEW_ATTRIBUTES_BIT_NVX = 0x00000001,
      // Provided by VK_NVX_multiview_per_view_attributes
        VK_SUBPASS_DESCRIPTION_PER_VIEW_POSITION_X_ONLY_BIT_NVX = 0x00000002,
      // Provided by VK_QCOM_render_pass_shader_resolve
        VK_SUBPASS_DESCRIPTION_FRAGMENT_REGION_BIT_QCOM = 0x00000004,
      // Provided by VK_QCOM_render_pass_shader_resolve
        VK_SUBPASS_DESCRIPTION_SHADER_RESOLVE_BIT_QCOM = 0x00000008,
      // Provided by VK_EXT_rasterization_order_attachment_access
        VK_SUBPASS_DESCRIPTION_RASTERIZATION_ORDER_ATTACHMENT_COLOR_ACCESS_BIT_EXT = 0x00000010,
      // Provided by VK_EXT_rasterization_order_attachment_access
        VK_SUBPASS_DESCRIPTION_RASTERIZATION_ORDER_ATTACHMENT_DEPTH_ACCESS_BIT_EXT = 0x00000020,
      // Provided by VK_EXT_rasterization_order_attachment_access
        VK_SUBPASS_DESCRIPTION_RASTERIZATION_ORDER_ATTACHMENT_STENCIL_ACCESS_BIT_EXT = 0x00000040,
      // Provided by VK_EXT_legacy_dithering
        VK_SUBPASS_DESCRIPTION_ENABLE_LEGACY_DITHERING_BIT_EXT = 0x00000080,
      // Provided by VK_ARM_rasterization_order_attachment_access
        VK_SUBPASS_DESCRIPTION_RASTERIZATION_ORDER_ATTACHMENT_COLOR_ACCESS_BIT_ARM = VK_SUBPASS_DESCRIPTION_RASTERIZATION_ORDER_ATTACHMENT_COLOR_ACCESS_BIT_EXT,
      // Provided by VK_ARM_rasterization_order_attachment_access
        VK_SUBPASS_DESCRIPTION_RASTERIZATION_ORDER_ATTACHMENT_DEPTH_ACCESS_BIT_ARM = VK_SUBPASS_DESCRIPTION_RASTERIZATION_ORDER_ATTACHMENT_DEPTH_ACCESS_BIT_EXT,
      // Provided by VK_ARM_rasterization_order_attachment_access
        VK_SUBPASS_DESCRIPTION_RASTERIZATION_ORDER_ATTACHMENT_STENCIL_ACCESS_BIT_ARM = VK_SUBPASS_DESCRIPTION_RASTERIZATION_ORDER_ATTACHMENT_STENCIL_ACCESS_BIT_EXT,
    } VkSubpassDescriptionFlagBits;

- `VK_SUBPASS_DESCRIPTION_PER_VIEW_ATTRIBUTES_BIT_NVX` specifies that shaders compiled for this subpass write the attributes for all views in a single invocation of each pre-rasterization shader stage. All pipelines compiled against a subpass that includes this bit must write per-view attributes to the `*PerViewNV[]` shader outputs, in addition to the non-per-view (e.g. `Position`) outputs.

- `VK_SUBPASS_DESCRIPTION_PER_VIEW_POSITION_X_ONLY_BIT_NVX` specifies that shaders compiled for this subpass use per-view positions which only differ in value in the x component. Per-view viewport mask can also be used.

- `VK_SUBPASS_DESCRIPTION_FRAGMENT_REGION_BIT_QCOM` specifies that the framebuffer region is the fragment region, that is, the minimum region dependencies are by pixel rather than by sample, such that any fragment shader invocation can access any sample associated with that fragment shader invocation.

- `VK_SUBPASS_DESCRIPTION_SHADER_RESOLVE_BIT_QCOM` specifies that the subpass performs shader resolve operations.

- `VK_SUBPASS_DESCRIPTION_RASTERIZATION_ORDER_ATTACHMENT_COLOR_ACCESS_BIT_EXT` specifies that this subpass supports pipelines created with `VK_PIPELINE_COLOR_BLEND_STATE_CREATE_RASTERIZATION_ORDER_ATTACHMENT_ACCESS_BIT_EXT`.

- `VK_SUBPASS_DESCRIPTION_RASTERIZATION_ORDER_ATTACHMENT_DEPTH_ACCESS_BIT_EXT` specifies that this subpass supports pipelines created with `VK_PIPELINE_DEPTH_STENCIL_STATE_CREATE_RASTERIZATION_ORDER_ATTACHMENT_DEPTH_ACCESS_BIT_EXT`.

- `VK_SUBPASS_DESCRIPTION_RASTERIZATION_ORDER_ATTACHMENT_STENCIL_ACCESS_BIT_EXT` specifies that this subpass supports pipelines created with `VK_PIPELINE_DEPTH_STENCIL_STATE_CREATE_RASTERIZATION_ORDER_ATTACHMENT_STENCIL_ACCESS_BIT_EXT`.

- `VK_SUBPASS_DESCRIPTION_ENABLE_LEGACY_DITHERING_BIT_EXT` specifies that Legacy Dithering is enabled for this subpass.

Note | Shader resolve operations allow for custom resolve operations, but overdrawing pixels may have a performance and/or power cost. Furthermore, since the content of any depth stencil attachment or color attachment is undefined at the beginning of a shader resolve subpass, any depth testing, stencil testing, or blending operation which sources these undefined values also has undefined result value.

    // Provided by VK_VERSION_1_0
    typedef VkFlags VkSubpassDescriptionFlags;

`VkSubpassDescriptionFlags` is a bitmask type for setting a mask of zero or more VkSubpassDescriptionFlagBits.

The `VkAttachmentReference` structure is defined as:

    // Provided by VK_VERSION_1_0
    typedef struct VkAttachmentReference {
        uint32_t         attachment;
        VkImageLayout    layout;
    } VkAttachmentReference;

- `attachment` is either an integer value identifying an attachment at the corresponding index in VkRenderPassCreateInfo::`pAttachments`, or `VK_ATTACHMENT_UNUSED` to signify that this attachment is not used.

- `layout` is a VkImageLayout value specifying the layout the attachment uses during the subpass.

Valid Usage

- VUID-VkAttachmentReference-layout-03077
  If `attachment` is not `VK_ATTACHMENT_UNUSED`, `layout` must not be `VK_IMAGE_LAYOUT_UNDEFINED`, `VK_IMAGE_LAYOUT_PREINITIALIZED`, or `VK_IMAGE_LAYOUT_PRESENT_SRC_KHR`

- VUID-VkAttachmentReference-separateDepthStencilLayouts-03313
  If the `separateDepthStencilLayouts` feature is not enabled, and `attachment` is not `VK_ATTACHMENT_UNUSED`, `layout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`,

- VUID-VkAttachmentReference-synchronization2-06910
  If the `synchronization2` feature is not enabled, `layout` must not be `VK_IMAGE_LAYOUT_ATTACHMENT_OPTIMAL_KHR` or `VK_IMAGE_LAYOUT_READ_ONLY_OPTIMAL_KHR`

- VUID-VkAttachmentReference-attachmentFeedbackLoopLayout-07311
  If the `attachmentFeedbackLoopLayout` feature is not enabled, `layout` must not be `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT`

- VUID-VkAttachmentReference-dynamicRenderingLocalRead-09546
  If the `dynamicRenderingLocalRead` feature is not enabled, `layout` must not be `VK_IMAGE_LAYOUT_RENDERING_LOCAL_READ`

Valid Usage (Implicit)

- VUID-VkAttachmentReference-layout-parameter
  `layout` must be a valid VkImageLayout value

`VK_SUBPASS_EXTERNAL` is a special subpass index value expanding synchronization scope outside a subpass. It is described in more detail by VkSubpassDependency.

    #define VK_SUBPASS_EXTERNAL               (~0U)

The `VkSubpassDependency` structure is defined as:

    // Provided by VK_VERSION_1_0
    typedef struct VkSubpassDependency {
        uint32_t                srcSubpass;
        uint32_t                dstSubpass;
        VkPipelineStageFlags    srcStageMask;
        VkPipelineStageFlags    dstStageMask;
        VkAccessFlags           srcAccessMask;
        VkAccessFlags           dstAccessMask;
        VkDependencyFlags       dependencyFlags;
    } VkSubpassDependency;

- `srcSubpass` is the subpass index of the first subpass in the dependency, or `VK_SUBPASS_EXTERNAL`.

- `dstSubpass` is the subpass index of the second subpass in the dependency, or `VK_SUBPASS_EXTERNAL`.

- `srcStageMask` is a bitmask of VkPipelineStageFlagBits specifying the source stage mask.

- `dstStageMask` is a bitmask of VkPipelineStageFlagBits specifying the destination stage mask

- `srcAccessMask` is a bitmask of VkAccessFlagBits specifying a source access mask.

- `dstAccessMask` is a bitmask of VkAccessFlagBits specifying a destination access mask.

- `dependencyFlags` is a bitmask of VkDependencyFlagBits.

If `srcSubpass` is equal to `dstSubpass` then the VkSubpassDependency does not directly define a dependency. Instead, it enables pipeline barriers to be used in a render pass instance within the identified subpass, where the scopes of one pipeline barrier must be a subset of those described by one subpass dependency. Subpass dependencies specified in this way that include framebuffer-space stages in the `srcStageMask` must only include framebuffer-space stages in `dstStageMask`, and must include `VK_DEPENDENCY_BY_REGION_BIT`. When a subpass dependency is specified in this way for a subpass that has more than one view in its view mask, its `dependencyFlags` must include `VK_DEPENDENCY_VIEW_LOCAL_BIT`.

If `srcSubpass` and `dstSubpass` are not equal, when a render pass instance which includes a subpass dependency is submitted to a queue, it defines a dependency between the subpasses identified by `srcSubpass` and `dstSubpass`.

If `srcSubpass` is equal to `VK_SUBPASS_EXTERNAL`, the first synchronization scope includes commands that occur earlier in submission order than the vkCmdBeginRenderPass used to begin the render pass instance. Otherwise, the first set of commands includes all commands submitted as part of the subpass instance identified by `srcSubpass` and any load, store, or multisample resolve operations on attachments used in `srcSubpass`. In either case, the first synchronization scope is limited to operations on the pipeline stages determined by the source stage mask specified by `srcStageMask`.

If `dstSubpass` is equal to `VK_SUBPASS_EXTERNAL`, the second synchronization scope includes commands that occur later in submission order than the vkCmdEndRenderPass used to end the render pass instance. Otherwise, the second set of commands includes all commands submitted as part of the subpass instance identified by `dstSubpass` and any load, store, and multisample resolve operations on attachments used in `dstSubpass`. In either case, the second synchronization scope is limited to operations on the pipeline stages determined by the destination stage mask specified by `dstStageMask`.

The first access scope is limited to accesses in the pipeline stages determined by the source stage mask specified by `srcStageMask`. It is also limited to access types in the source access mask specified by `srcAccessMask`.

The second access scope is limited to accesses in the pipeline stages determined by the destination stage mask specified by `dstStageMask`. It is also limited to access types in the destination access mask specified by `dstAccessMask`.

The availability and visibility operations defined by a subpass dependency affect the execution of image layout transitions within the render pass.

Note | For non-attachment resources, the memory dependency expressed by subpass dependency is nearly identical to that of a VkMemoryBarrier (with matching `srcAccessMask` and `dstAccessMask` parameters) submitted as a part of a vkCmdPipelineBarrier (with matching `srcStageMask` and `dstStageMask` parameters). The only difference being that its scopes are limited to the identified subpasses rather than potentially affecting everything before and after. For attachments however, subpass dependencies work more like a VkImageMemoryBarrier defined similarly to the VkMemoryBarrier above, the queue family indices set to `VK_QUEUE_FAMILY_IGNORED`, and layouts as follows: The equivalent to `oldLayout` is the attachment’s layout according to the subpass description for `srcSubpass`. The equivalent to `newLayout` is the attachment’s layout according to the subpass description for `dstSubpass`.

Valid Usage

- VUID-VkSubpassDependency-srcStageMask-04090
  If the `geometryShader` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_GEOMETRY_SHADER_BIT`

- VUID-VkSubpassDependency-srcStageMask-04091
  If the `tessellationShader` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_TESSELLATION_CONTROL_SHADER_BIT` or `VK_PIPELINE_STAGE_TESSELLATION_EVALUATION_SHADER_BIT`

- VUID-VkSubpassDependency-srcStageMask-04092
  If the `conditionalRendering` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_CONDITIONAL_RENDERING_BIT_EXT`

- VUID-VkSubpassDependency-srcStageMask-04093
  If the `fragmentDensityMap` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_FRAGMENT_DENSITY_PROCESS_BIT_EXT`

- VUID-VkSubpassDependency-srcStageMask-04094
  If the `transformFeedback` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_TRANSFORM_FEEDBACK_BIT_EXT`

- VUID-VkSubpassDependency-srcStageMask-04095
  If the `meshShader` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_MESH_SHADER_BIT_EXT`

- VUID-VkSubpassDependency-srcStageMask-04096
  If the `taskShader` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_TASK_SHADER_BIT_EXT`

- VUID-VkSubpassDependency-srcStageMask-07318
  If neither of the `shadingRateImage` or the `attachmentFragmentShadingRate` features are enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_FRAGMENT_SHADING_RATE_ATTACHMENT_BIT_KHR`

- VUID-VkSubpassDependency-srcStageMask-03937
  If the `synchronization2` feature is not enabled, `srcStageMask` must not be `0`

- VUID-VkSubpassDependency-srcStageMask-07949
  If neither the VK_NV_ray_tracing extension or the `rayTracingPipeline` feature are enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_RAY_TRACING_SHADER_BIT_KHR`

- VUID-VkSubpassDependency-dstStageMask-04090
  If the `geometryShader` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_GEOMETRY_SHADER_BIT`

- VUID-VkSubpassDependency-dstStageMask-04091
  If the `tessellationShader` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_TESSELLATION_CONTROL_SHADER_BIT` or `VK_PIPELINE_STAGE_TESSELLATION_EVALUATION_SHADER_BIT`

- VUID-VkSubpassDependency-dstStageMask-04092
  If the `conditionalRendering` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_CONDITIONAL_RENDERING_BIT_EXT`

- VUID-VkSubpassDependency-dstStageMask-04093
  If the `fragmentDensityMap` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_FRAGMENT_DENSITY_PROCESS_BIT_EXT`

- VUID-VkSubpassDependency-dstStageMask-04094
  If the `transformFeedback` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_TRANSFORM_FEEDBACK_BIT_EXT`

- VUID-VkSubpassDependency-dstStageMask-04095
  If the `meshShader` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_MESH_SHADER_BIT_EXT`

- VUID-VkSubpassDependency-dstStageMask-04096
  If the `taskShader` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_TASK_SHADER_BIT_EXT`

- VUID-VkSubpassDependency-dstStageMask-07318
  If neither of the `shadingRateImage` or the `attachmentFragmentShadingRate` features are enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_FRAGMENT_SHADING_RATE_ATTACHMENT_BIT_KHR`

- VUID-VkSubpassDependency-dstStageMask-03937
  If the `synchronization2` feature is not enabled, `dstStageMask` must not be `0`

- VUID-VkSubpassDependency-dstStageMask-07949
  If neither the VK_NV_ray_tracing extension or the `rayTracingPipeline` feature are enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_RAY_TRACING_SHADER_BIT_KHR`

- VUID-VkSubpassDependency-srcSubpass-00864
  `srcSubpass` must be less than or equal to `dstSubpass`, unless one of them is `VK_SUBPASS_EXTERNAL`, to avoid cyclic dependencies and ensure a valid execution order

- VUID-VkSubpassDependency-srcSubpass-00865
  `srcSubpass` and `dstSubpass` must not both be equal to `VK_SUBPASS_EXTERNAL`

- VUID-VkSubpassDependency-srcSubpass-06809
  If `srcSubpass` is equal to `dstSubpass` and `srcStageMask` includes a framebuffer-space stage, `dstStageMask` must only contain framebuffer-space stages

- VUID-VkSubpassDependency-srcAccessMask-00868
  Any access flag included in `srcAccessMask` must be supported by one of the pipeline stages in `srcStageMask`, as specified in the table of supported access types

- VUID-VkSubpassDependency-dstAccessMask-00869
  Any access flag included in `dstAccessMask` must be supported by one of the pipeline stages in `dstStageMask`, as specified in the table of supported access types

- VUID-VkSubpassDependency-srcSubpass-02243
  If `srcSubpass` equals `dstSubpass`, and `srcStageMask` and `dstStageMask` both include a framebuffer-space stage, then `dependencyFlags` must include `VK_DEPENDENCY_BY_REGION_BIT`

- VUID-VkSubpassDependency-dependencyFlags-02520
  If `dependencyFlags` includes `VK_DEPENDENCY_VIEW_LOCAL_BIT`, `srcSubpass` must not be equal to `VK_SUBPASS_EXTERNAL`

- VUID-VkSubpassDependency-dependencyFlags-02521
  If `dependencyFlags` includes `VK_DEPENDENCY_VIEW_LOCAL_BIT`, `dstSubpass` must not be equal to `VK_SUBPASS_EXTERNAL`

- VUID-VkSubpassDependency-srcSubpass-00872
  If `srcSubpass` equals `dstSubpass` and that subpass has more than one bit set in the view mask, then `dependencyFlags` must include `VK_DEPENDENCY_VIEW_LOCAL_BIT`

Valid Usage (Implicit)

- VUID-VkSubpassDependency-srcStageMask-parameter
  `srcStageMask` must be a valid combination of VkPipelineStageFlagBits values

- VUID-VkSubpassDependency-dstStageMask-parameter
  `dstStageMask` must be a valid combination of VkPipelineStageFlagBits values

- VUID-VkSubpassDependency-srcAccessMask-parameter
  `srcAccessMask` must be a valid combination of VkAccessFlagBits values

- VUID-VkSubpassDependency-dstAccessMask-parameter
  `dstAccessMask` must be a valid combination of VkAccessFlagBits values

- VUID-VkSubpassDependency-dependencyFlags-parameter
  `dependencyFlags` must be a valid combination of VkDependencyFlagBits values

When multiview is enabled, the execution of the multiple views of one subpass may not occur simultaneously or even back-to-back, and rather may be interleaved with the execution of other subpasses. The load and store operations apply to attachments on a per-view basis. For example, an attachment using `VK_ATTACHMENT_LOAD_OP_CLEAR` will have each view cleared on first use, but the first use of one view may be temporally distant from the first use of another view.

Note | A good mental model for multiview is to think of a multiview subpass as if it were a collection of individual (per-view) subpasses that are logically grouped together and described as a single multiview subpass in the API. Similarly, a multiview attachment can be thought of like several individual attachments that happen to be layers in a single image. A view-local dependency between two multiview subpasses acts like a set of one-to-one dependencies between corresponding pairs of per-view subpasses. A view-global dependency between two multiview subpasses acts like a set of N × M dependencies between all pairs of per-view subpasses in the source and destination. Thus, it is a more compact representation which also makes clear the commonality and reuse that is present between views in a subpass. This interpretation motivates the answers to questions like “when does the load op apply” - it is on the first use of each view of an attachment, as if each view was a separate attachment. The content of each view follows the description in attachment content behavior. In particular, if an attachment is preserved, all views within the attachment are preserved.

If any two subpasses of a render pass activate transform feedback to the same bound transform feedback buffers, a subpass dependency must be included (either directly or via some intermediate subpasses) between them.

If there is no subpass dependency from `VK_SUBPASS_EXTERNAL` to the first subpass that uses an attachment, then an implicit subpass dependency exists from `VK_SUBPASS_EXTERNAL` to the first subpass it is used in. The implicit subpass dependency only exists if there exists an automatic layout transition away from `initialLayout`. The subpass dependency operates as if defined with the following parameters:

    VkSubpassDependency implicitDependency = {
        .srcSubpass = VK_SUBPASS_EXTERNAL,
        .dstSubpass = firstSubpass, // First subpass attachment is used in
        .srcStageMask = VK_PIPELINE_STAGE_NONE,
        .dstStageMask = VK_PIPELINE_STAGE_ALL_COMMANDS_BIT,
        .srcAccessMask = 0,
        .dstAccessMask = VK_ACCESS_INPUT_ATTACHMENT_READ_BIT |
                         VK_ACCESS_COLOR_ATTACHMENT_READ_BIT |
                         VK_ACCESS_COLOR_ATTACHMENT_WRITE_BIT |
                         VK_ACCESS_DEPTH_STENCIL_ATTACHMENT_READ_BIT |
                         VK_ACCESS_DEPTH_STENCIL_ATTACHMENT_WRITE_BIT,
        .dependencyFlags = 0
    };

Similarly, if there is no subpass dependency from the last subpass that uses an attachment to `VK_SUBPASS_EXTERNAL`, then an implicit subpass dependency exists from the last subpass it is used in to `VK_SUBPASS_EXTERNAL`. The implicit subpass dependency only exists if there exists an automatic layout transition into `finalLayout`. The subpass dependency operates as if defined with the following parameters:

    VkSubpassDependency implicitDependency = {
        .srcSubpass = lastSubpass, // Last subpass attachment is used in
        .dstSubpass = VK_SUBPASS_EXTERNAL,
        .srcStageMask = VK_PIPELINE_STAGE_ALL_COMMANDS_BIT,
        .dstStageMask = VK_PIPELINE_STAGE_NONE,
        .srcAccessMask = VK_ACCESS_COLOR_ATTACHMENT_WRITE_BIT |
                         VK_ACCESS_DEPTH_STENCIL_ATTACHMENT_WRITE_BIT,
        .dstAccessMask = 0,
        .dependencyFlags = 0
    };

As subpasses may overlap or execute out of order with regards to other subpasses unless a subpass dependency chain describes otherwise, the layout transitions required between subpasses cannot be known to an application. Instead, an application provides the layout that each attachment must be in at the start and end of a render pass, and the layout it must be in during each subpass it is used in. The implementation then must execute layout transitions between subpasses in order to guarantee that the images are in the layouts required by each subpass, and in the final layout at the end of the render pass.

Automatic layout transitions apply to the entire image subresource attached to the framebuffer. If multiview is not enabled and the attachment is a view of a 1D or 2D image, the automatic layout transitions apply to the number of layers specified by VkFramebufferCreateInfo::`layers`. If multiview is enabled and the attachment is a view of a 1D or 2D image, the automatic layout transitions apply to the layers corresponding to views which are used by some subpass in the render pass, even if that subpass does not reference the given attachment. If the attachment view is a 2D or 2D array view of a 3D image, even if the attachment view only refers to a subset of the slices of the selected mip level of the 3D image, automatic layout transitions apply to the entire subresource referenced which is the entire mip level in this case.

Automatic layout transitions away from the layout used in a subpass happen-after the availability operations for all dependencies with that subpass as the `srcSubpass`.

Automatic layout transitions into the layout used in a subpass happen-before the visibility operations for all dependencies with that subpass as the `dstSubpass`.

Automatic layout transitions away from `initialLayout` happen-after the availability operations for all dependencies with a `srcSubpass` equal to `VK_SUBPASS_EXTERNAL`, where `dstSubpass` uses the attachment that will be transitioned. For attachments created with `VK_ATTACHMENT_DESCRIPTION_MAY_ALIAS_BIT`, automatic layout transitions away from `initialLayout` happen-after the availability operations for all dependencies with a `srcSubpass` equal to `VK_SUBPASS_EXTERNAL`, where `dstSubpass` uses any aliased attachment.

Automatic layout transitions into `finalLayout` happen-before the visibility operations for all dependencies with a `dstSubpass` equal to `VK_SUBPASS_EXTERNAL`, where `srcSubpass` uses the attachment that will be transitioned. For attachments created with `VK_ATTACHMENT_DESCRIPTION_MAY_ALIAS_BIT`, automatic layout transitions into `finalLayout` happen-before the visibility operations for all dependencies with a `dstSubpass` equal to `VK_SUBPASS_EXTERNAL`, where `srcSubpass` uses any aliased attachment.

The image layout of the depth aspect of a depth/stencil attachment referring to an image created with `VK_IMAGE_CREATE_SAMPLE_LOCATIONS_COMPATIBLE_DEPTH_BIT_EXT` is dependent on the last sample locations used to render to the attachment, thus automatic layout transitions use the sample locations state specified in VkRenderPassSampleLocationsBeginInfoEXT.

Automatic layout transitions of an attachment referring to a depth/stencil image created with `VK_IMAGE_CREATE_SAMPLE_LOCATIONS_COMPATIBLE_DEPTH_BIT_EXT` use the sample locations the image subresource range referenced by the attachment was last rendered with. If the current render pass does not use the attachment as a depth/stencil attachment in any subpass that happens-before, the automatic layout transition uses the sample locations state specified in the `sampleLocationsInfo` member of the element of the `VkRenderPassSampleLocationsBeginInfoEXT`::`pAttachmentInitialSampleLocations` array for which the `attachmentIndex` member equals the attachment index of the attachment, if one is specified. Otherwise, the automatic layout transition uses the sample locations state specified in the `sampleLocationsInfo` member of the element of the `VkRenderPassSampleLocationsBeginInfoEXT`::`pPostSubpassSampleLocations` array for which the `subpassIndex` member equals the index of the subpass that last used the attachment as a depth/stencil attachment, if one is specified.

If no sample locations state has been specified for an automatic layout transition performed on an attachment referring to a depth/stencil image created with `VK_IMAGE_CREATE_SAMPLE_LOCATIONS_COMPATIBLE_DEPTH_BIT_EXT` the contents of the depth aspect of the depth/stencil attachment become undefined as if the layout of the attachment was transitioned from the `VK_IMAGE_LAYOUT_UNDEFINED` layout.

If two subpasses use the same attachment, and both subpasses use the attachment in a read-only layout, no subpass dependency needs to be specified between those subpasses. If an implementation treats those layouts separately, it must insert an implicit subpass dependency between those subpasses to separate the uses in each layout. The subpass dependency operates as if defined with the following parameters:

    // Used for input attachments
    VkPipelineStageFlags inputAttachmentStages = VK_PIPELINE_STAGE_FRAGMENT_SHADER_BIT;
    VkAccessFlags inputAttachmentDstAccess = VK_ACCESS_INPUT_ATTACHMENT_READ_BIT;

    // Used for depth/stencil attachments
    VkPipelineStageFlags depthStencilAttachmentStages = VK_PIPELINE_STAGE_EARLY_FRAGMENT_TESTS_BIT | VK_PIPELINE_STAGE_LATE_FRAGMENT_TESTS_BIT;
    VkAccessFlags depthStencilAttachmentDstAccess = VK_ACCESS_DEPTH_STENCIL_ATTACHMENT_READ_BIT;

    VkSubpassDependency implicitDependency = {
        .srcSubpass = firstSubpass;
        .dstSubpass = secondSubpass;
        .srcStageMask = inputAttachmentStages | depthStencilAttachmentStages;
        .dstStageMask = inputAttachmentStages | depthStencilAttachmentStages;
        .srcAccessMask = 0;
        .dstAccessMask = inputAttachmentDstAccess | depthStencilAttachmentDstAccess;
        .dependencyFlags = 0;
    };

When drawing using shader objects, or when the graphics pipeline is created with `VK_DYNAMIC_STATE_ATTACHMENT_FEEDBACK_LOOP_ENABLE_EXT` set in VkPipelineDynamicStateCreateInfo::`pDynamicStates`, the application must specify which types of attachments that are written to during a render pass will also be accessed as non-attachments in the render pass.

To dynamically set whether a pipeline can access a resource as a non-attachment while it is also used as an attachment that is written to, call:

    // Provided by VK_EXT_attachment_feedback_loop_dynamic_state
    void vkCmdSetAttachmentFeedbackLoopEnableEXT(
        VkCommandBuffer                             commandBuffer,
        VkImageAspectFlags                          aspectMask);

- `commandBuffer` is the command buffer into which the command will be recorded.

- `aspectMask` specifies the types of attachments for which feedback loops will be enabled. Attachment types whose aspects are not included in `aspectMask` will have feedback loops disabled.

For attachments that are written to in a render pass, only attachments with the aspects specified in `aspectMask` can be accessed as non-attachments by subsequent drawing commands.

Valid Usage

- VUID-vkCmdSetAttachmentFeedbackLoopEnableEXT-attachmentFeedbackLoopDynamicState-08862
  The `attachmentFeedbackLoopDynamicState` feature must be enabled

- VUID-vkCmdSetAttachmentFeedbackLoopEnableEXT-aspectMask-08863
  `aspectMask` must only include `VK_IMAGE_ASPECT_NONE`, `VK_IMAGE_ASPECT_COLOR_BIT`, `VK_IMAGE_ASPECT_DEPTH_BIT`, and `VK_IMAGE_ASPECT_STENCIL_BIT`

- VUID-vkCmdSetAttachmentFeedbackLoopEnableEXT-attachmentFeedbackLoopLayout-08864
  If the `attachmentFeedbackLoopLayout` feature is not enabled, `aspectMask` must be `VK_IMAGE_ASPECT_NONE`

Valid Usage (Implicit)

- VUID-vkCmdSetAttachmentFeedbackLoopEnableEXT-commandBuffer-parameter
  `commandBuffer` must be a valid VkCommandBuffer handle

- VUID-vkCmdSetAttachmentFeedbackLoopEnableEXT-aspectMask-parameter
  `aspectMask` must be a valid combination of VkImageAspectFlagBits values

- VUID-vkCmdSetAttachmentFeedbackLoopEnableEXT-commandBuffer-recording
  `commandBuffer` must be in the recording state

- VUID-vkCmdSetAttachmentFeedbackLoopEnableEXT-commandBuffer-cmdpool
  The `VkCommandPool` that `commandBuffer` was allocated from must support graphics operations

- VUID-vkCmdSetAttachmentFeedbackLoopEnableEXT-videocoding
  This command must only be called outside of a video coding scope

Host Synchronization

- Host access to `commandBuffer` must be externally synchronized

- Host access to the `VkCommandPool` that `commandBuffer` was allocated from must be externally synchronized

Command Properties

Command Buffer Levels | Render Pass Scope | Video Coding Scope | Supported Queue Types | Command Type
--- | --- | --- | --- | ---
Primary Secondary | Both | Outside | Graphics | State

A more extensible version of render pass creation is also defined below.

To create a render pass, call:

    // Provided by VK_VERSION_1_2
    VkResult vkCreateRenderPass2(
        VkDevice                                    device,
        const VkRenderPassCreateInfo2*              pCreateInfo,
        const VkAllocationCallbacks*                pAllocator,
        VkRenderPass*                               pRenderPass);

or the equivalent command

    // Provided by VK_KHR_create_renderpass2
    VkResult vkCreateRenderPass2KHR(
        VkDevice                                    device,
        const VkRenderPassCreateInfo2*              pCreateInfo,
        const VkAllocationCallbacks*                pAllocator,
        VkRenderPass*                               pRenderPass);

- `device` is the logical device that creates the render pass.

- `pCreateInfo` is a pointer to a VkRenderPassCreateInfo2 structure describing the parameters of the render pass.

- `pAllocator` controls host memory allocation as described in the Memory Allocation chapter.

- `pRenderPass` is a pointer to a VkRenderPass handle in which the resulting render pass object is returned.

This command is functionally identical to vkCreateRenderPass, but includes extensible sub-structures that include `sType` and `pNext` parameters, allowing them to be more easily extended.

Valid Usage

- VUID-vkCreateRenderPass2-device-10001
  `device` must support at least one queue family with the `VK_QUEUE_GRAPHICS_BIT` capability

Valid Usage (Implicit)

- VUID-vkCreateRenderPass2-device-parameter
  `device` must be a valid VkDevice handle

- VUID-vkCreateRenderPass2-pCreateInfo-parameter
  `pCreateInfo` must be a valid pointer to a valid VkRenderPassCreateInfo2 structure

- VUID-vkCreateRenderPass2-pAllocator-parameter
  If `pAllocator` is not `NULL`, `pAllocator` must be a valid pointer to a valid VkAllocationCallbacks structure

- VUID-vkCreateRenderPass2-pRenderPass-parameter
  `pRenderPass` must be a valid pointer to a VkRenderPass handle

Return Codes

Success

  - `VK_SUCCESS`

Failure

  - `VK_ERROR_OUT_OF_HOST_MEMORY`

  - `VK_ERROR_OUT_OF_DEVICE_MEMORY`

The `VkRenderPassCreateInfo2` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkRenderPassCreateInfo2 {
        VkStructureType                    sType;
        const void*                        pNext;
        VkRenderPassCreateFlags            flags;
        uint32_t                           attachmentCount;
        const VkAttachmentDescription2*    pAttachments;
        uint32_t                           subpassCount;
        const VkSubpassDescription2*       pSubpasses;
        uint32_t                           dependencyCount;
        const VkSubpassDependency2*        pDependencies;
        uint32_t                           correlatedViewMaskCount;
        const uint32_t*                    pCorrelatedViewMasks;
    } VkRenderPassCreateInfo2;

or the equivalent

    // Provided by VK_KHR_create_renderpass2
    typedef VkRenderPassCreateInfo2 VkRenderPassCreateInfo2KHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `flags` is reserved for future use.

- `attachmentCount` is the number of attachments used by this render pass.

- `pAttachments` is a pointer to an array of `attachmentCount` VkAttachmentDescription2 structures describing the attachments used by the render pass.

- `subpassCount` is the number of subpasses to create.

- `pSubpasses` is a pointer to an array of `subpassCount` VkSubpassDescription2 structures describing each subpass.

- `dependencyCount` is the number of dependencies between pairs of subpasses.

- `pDependencies` is a pointer to an array of `dependencyCount` VkSubpassDependency2 structures describing dependencies between pairs of subpasses.

- `correlatedViewMaskCount` is the number of correlation masks.

- `pCorrelatedViewMasks` is a pointer to an array of view masks indicating sets of views that may be more efficient to render concurrently.

Parameters defined by this structure with the same name as those in VkRenderPassCreateInfo have the identical effect to those parameters; the child structures are variants of those used in VkRenderPassCreateInfo which add `sType` and `pNext` parameters, allowing them to be extended.

If the VkSubpassDescription2::`viewMask` member of any element of `pSubpasses` is not zero, multiview functionality is considered to be enabled for this render pass.

`correlatedViewMaskCount` and `pCorrelatedViewMasks` have the same effect as VkRenderPassMultiviewCreateInfo::`correlationMaskCount` and VkRenderPassMultiviewCreateInfo::`pCorrelationMasks`, respectively.

Valid Usage

- VUID-VkRenderPassCreateInfo2-None-03049
  If any two subpasses operate on attachments with overlapping ranges of the same `VkDeviceMemory` object, and at least one subpass writes to that area of `VkDeviceMemory`, a subpass dependency must be included (either directly or via some intermediate subpasses) between them

- VUID-VkRenderPassCreateInfo2-attachment-03050
  If the `attachment` member of any element of `pInputAttachments`, `pColorAttachments`, `pResolveAttachments` or `pDepthStencilAttachment`, or the attachment indexed by any element of `pPreserveAttachments` in any element of `pSubpasses` is bound to a range of a `VkDeviceMemory` object that overlaps with any other attachment in any subpass (including the same subpass), the `VkAttachmentDescription2` structures describing them must include `VK_ATTACHMENT_DESCRIPTION_MAY_ALIAS_BIT` in `flags`

- VUID-VkRenderPassCreateInfo2-attachment-03051
  If the `attachment` member of any element of `pInputAttachments`, `pColorAttachments`, `pResolveAttachments` or `pDepthStencilAttachment`, or any element of `pPreserveAttachments` in any element of `pSubpasses` is not `VK_ATTACHMENT_UNUSED`, then it must be less than `attachmentCount`

- VUID-VkRenderPassCreateInfo2-fragmentDensityMapAttachment-06472
  If the pNext chain includes a VkRenderPassFragmentDensityMapCreateInfoEXT structure and the `fragmentDensityMapAttachment` member is not `VK_ATTACHMENT_UNUSED`, then `attachment` must be less than `attachmentCount`

- VUID-VkRenderPassCreateInfo2-pSubpasses-06473
  If the `pSubpasses` pNext chain includes a VkSubpassDescriptionDepthStencilResolve structure and the `pDepthStencilResolveAttachment` member is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED`, then `attachment` must be less than `attachmentCount`

- VUID-VkRenderPassCreateInfo2-pAttachments-02522
  For any member of `pAttachments` with a `loadOp` equal to `VK_ATTACHMENT_LOAD_OP_CLEAR`, the first use of that attachment must not specify a `layout` equal to `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`, or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkRenderPassCreateInfo2-pAttachments-02523
  For any member of `pAttachments` with a `stencilLoadOp` equal to `VK_ATTACHMENT_LOAD_OP_CLEAR`, the first use of that attachment must not specify a `layout` equal to `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`, or `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkRenderPassCreateInfo2-pDependencies-03054
  For any element of `pDependencies`, if the `srcSubpass` is not `VK_SUBPASS_EXTERNAL`, all stage flags included in the `srcStageMask` member of that dependency must be a pipeline stage supported by the pipeline identified by the `pipelineBindPoint` member of the source subpass

- VUID-VkRenderPassCreateInfo2-pDependencies-03055
  For any element of `pDependencies`, if the `dstSubpass` is not `VK_SUBPASS_EXTERNAL`, all stage flags included in the `dstStageMask` member of that dependency must be a pipeline stage supported by the pipeline identified by the `pipelineBindPoint` member of the destination subpass

- VUID-VkRenderPassCreateInfo2-pCorrelatedViewMasks-03056
  The set of bits included in any element of `pCorrelatedViewMasks` must not overlap with the set of bits included in any other element of `pCorrelatedViewMasks`

- VUID-VkRenderPassCreateInfo2-viewMask-03057
  If the VkSubpassDescription2::`viewMask` member of all elements of `pSubpasses` is `0`, `correlatedViewMaskCount` must be `0`

- VUID-VkRenderPassCreateInfo2-viewMask-03058
  The VkSubpassDescription2::`viewMask` member of all elements of `pSubpasses` must either all be `0`, or all not be `0`

- VUID-VkRenderPassCreateInfo2-viewMask-03059
  If the VkSubpassDescription2::`viewMask` member of all elements of `pSubpasses` is `0`, the `dependencyFlags` member of any element of `pDependencies` must not include `VK_DEPENDENCY_VIEW_LOCAL_BIT`

- VUID-VkRenderPassCreateInfo2-pDependencies-03060
  For any element of `pDependencies` where its `srcSubpass` member equals its `dstSubpass` member, if the `viewMask` member of the corresponding element of `pSubpasses` includes more than one bit, its `dependencyFlags` member must include `VK_DEPENDENCY_VIEW_LOCAL_BIT`

- VUID-VkRenderPassCreateInfo2-attachment-02525
  If the `attachment` member of any element of the `pInputAttachments` member of any element of `pSubpasses` is not `VK_ATTACHMENT_UNUSED`, the `aspectMask` member of that element of `pInputAttachments` must only include aspects that are present in images of the format specified by the element of `pAttachments` specified by `attachment`

- VUID-VkRenderPassCreateInfo2-srcSubpass-02526
  The `srcSubpass` member of each element of `pDependencies` must be less than `subpassCount`

- VUID-VkRenderPassCreateInfo2-dstSubpass-02527
  The `dstSubpass` member of each element of `pDependencies` must be less than `subpassCount`

- VUID-VkRenderPassCreateInfo2-pAttachments-04585
  If any element of `pAttachments` is used as a fragment shading rate attachment in any subpass, it must not be used as any other attachment in the render pass

- VUID-VkRenderPassCreateInfo2-pAttachments-09387
  If any element of `pAttachments` is used as a fragment shading rate attachment, the `loadOp` for that attachment must not be `VK_ATTACHMENT_LOAD_OP_CLEAR`

- VUID-VkRenderPassCreateInfo2-flags-04521
  If `flags` includes `VK_RENDER_PASS_CREATE_TRANSFORM_BIT_QCOM`, an element of `pSubpasses` includes an instance of VkFragmentShadingRateAttachmentInfoKHR in its `pNext` chain, and the `pFragmentShadingRateAttachment` member of that structure is not equal to `NULL`, the `attachment` member of `pFragmentShadingRateAttachment` must be `VK_ATTACHMENT_UNUSED`

- VUID-VkRenderPassCreateInfo2-pAttachments-04586
  If any element of `pAttachments` is used as a fragment shading rate attachment in any subpass, it must have an image format whose potential format features contain `VK_FORMAT_FEATURE_FRAGMENT_SHADING_RATE_ATTACHMENT_BIT_KHR`

- VUID-VkRenderPassCreateInfo2-rasterizationSamples-04905
  If the pipeline is being created with fragment shader state, and the `VK_QCOM_render_pass_shader_resolve extension` is enabled, and if subpass has any input attachments, and if the subpass description contains `VK_SUBPASS_DESCRIPTION_FRAGMENT_REGION_BIT_QCOM`, then the sample count of the input attachments must equal `rasterizationSamples`

- VUID-VkRenderPassCreateInfo2-sampleShadingEnable-04906
  If the pipeline is being created with fragment shader state, and the `VK_QCOM_render_pass_shader_resolve` extension is enabled, and if the subpass description contains `VK_SUBPASS_DESCRIPTION_FRAGMENT_REGION_BIT_QCOM`, then `sampleShadingEnable` must be false

- VUID-VkRenderPassCreateInfo2-flags-04907
  If `flags` includes `VK_SUBPASS_DESCRIPTION_SHADER_RESOLVE_BIT_QCOM`, and if `pResolveAttachments` is not `NULL`, then each resolve attachment must be `VK_ATTACHMENT_UNUSED`

- VUID-VkRenderPassCreateInfo2-flags-04908
  If `flags` includes `VK_SUBPASS_DESCRIPTION_SHADER_RESOLVE_BIT_QCOM`, and if `pDepthStencilResolveAttachment` is not `NULL`, then the depth/stencil resolve attachment must be `VK_ATTACHMENT_UNUSED`

- VUID-VkRenderPassCreateInfo2-flags-04909
  If `flags` includes `VK_SUBPASS_DESCRIPTION_SHADER_RESOLVE_BIT_QCOM`, then the subpass must be the last subpass in a subpass dependency chain

- VUID-VkRenderPassCreateInfo2-attachment-06244
  If the `attachment` member of the `pDepthStencilAttachment` member of an element of `pSubpasses` is not `VK_ATTACHMENT_UNUSED`, the `layout` member of that same structure is either `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, and the `pNext` chain of that structure does not include a VkAttachmentReferenceStencilLayout structure, then the element of `pAttachments` with an index equal to `attachment` must not have a `format` that includes both depth and stencil components

- VUID-VkRenderPassCreateInfo2-attachment-06245
  If the `attachment` member of the `pDepthStencilAttachment` member of an element of `pSubpasses` is not `VK_ATTACHMENT_UNUSED` and the `layout` member of that same structure is either `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`, then the element of `pAttachments` with an index equal to `attachment` must have a `format` that includes only a stencil component

- VUID-VkRenderPassCreateInfo2-attachment-06246
  If the `attachment` member of the `pDepthStencilAttachment` member of an element of `pSubpasses` is not `VK_ATTACHMENT_UNUSED` and the `layout` member of that same structure is either `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, then the element of `pAttachments` with an index equal to `attachment` must not have a `format` that includes only a stencil component

- VUID-VkRenderPassCreateInfo2-pResolveAttachments-09331
  If any element of `pResolveAttachments` of any element of `pSubpasses` references an attachment description with a format of `VK_FORMAT_UNDEFINED`, VkRenderPassFragmentDensityMapCreateInfoEXT::`fragmentDensityMapAttachment->attachment` must be `VK_ATTACHMENT_UNUSED`

Valid Usage (Implicit)

- VUID-VkRenderPassCreateInfo2-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_CREATE_INFO_2`

- VUID-VkRenderPassCreateInfo2-pNext-pNext
  Each `pNext` member of any structure (including this one) in the `pNext` chain must be either `NULL` or a pointer to a valid instance of VkRenderPassCreationControlEXT, VkRenderPassCreationFeedbackCreateInfoEXT, or VkRenderPassFragmentDensityMapCreateInfoEXT

- VUID-VkRenderPassCreateInfo2-sType-unique
  The `sType` value of each struct in the `pNext` chain must be unique

- VUID-VkRenderPassCreateInfo2-flags-parameter
  `flags` must be a valid combination of VkRenderPassCreateFlagBits values

- VUID-VkRenderPassCreateInfo2-pAttachments-parameter
  If `attachmentCount` is not `0`, `pAttachments` must be a valid pointer to an array of `attachmentCount` valid VkAttachmentDescription2 structures

- VUID-VkRenderPassCreateInfo2-pSubpasses-parameter
  `pSubpasses` must be a valid pointer to an array of `subpassCount` valid VkSubpassDescription2 structures

- VUID-VkRenderPassCreateInfo2-pDependencies-parameter
  If `dependencyCount` is not `0`, `pDependencies` must be a valid pointer to an array of `dependencyCount` valid VkSubpassDependency2 structures

- VUID-VkRenderPassCreateInfo2-pCorrelatedViewMasks-parameter
  If `correlatedViewMaskCount` is not `0`, `pCorrelatedViewMasks` must be a valid pointer to an array of `correlatedViewMaskCount` `uint32_t` values

- VUID-VkRenderPassCreateInfo2-subpassCount-arraylength
  `subpassCount` must be greater than `0`

The `VkAttachmentDescription2` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkAttachmentDescription2 {
        VkStructureType                 sType;
        const void*                     pNext;
        VkAttachmentDescriptionFlags    flags;
        VkFormat                        format;
        VkSampleCountFlagBits           samples;
        VkAttachmentLoadOp              loadOp;
        VkAttachmentStoreOp             storeOp;
        VkAttachmentLoadOp              stencilLoadOp;
        VkAttachmentStoreOp             stencilStoreOp;
        VkImageLayout                   initialLayout;
        VkImageLayout                   finalLayout;
    } VkAttachmentDescription2;

or the equivalent

    // Provided by VK_KHR_create_renderpass2
    typedef VkAttachmentDescription2 VkAttachmentDescription2KHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `flags` is a bitmask of VkAttachmentDescriptionFlagBits specifying additional properties of the attachment.

- `format` is a VkFormat value specifying the format of the image that will be used for the attachment.

- `samples` is a VkSampleCountFlagBits value specifying the number of samples of the image.

- `loadOp` is a VkAttachmentLoadOp value specifying how the contents of color and depth components of the attachment are treated at the beginning of the subpass where it is first used.

- `storeOp` is a VkAttachmentStoreOp value specifying how the contents of color and depth components of the attachment are treated at the end of the subpass where it is last used.

- `stencilLoadOp` is a VkAttachmentLoadOp value specifying how the contents of stencil components of the attachment are treated at the beginning of the subpass where it is first used.

- `stencilStoreOp` is a VkAttachmentStoreOp value specifying how the contents of stencil components of the attachment are treated at the end of the last subpass where it is used.

- `initialLayout` is the layout the attachment image subresource will be in when a render pass instance begins.

- `finalLayout` is the layout the attachment image subresource will be transitioned to when a render pass instance ends.

Parameters defined by this structure with the same name as those in VkAttachmentDescription have the identical effect to those parameters.

If the `separateDepthStencilLayouts` feature is enabled, and `format` is a depth/stencil format, `initialLayout` and `finalLayout` can be set to a layout that only specifies the layout of the depth aspect.

If the `pNext` chain includes a VkAttachmentDescriptionStencilLayout structure, then the `stencilInitialLayout` and `stencilFinalLayout` members specify the initial and final layouts of the stencil aspect of a depth/stencil format, and `initialLayout` and `finalLayout` only apply to the depth aspect. For depth-only formats, the VkAttachmentDescriptionStencilLayout structure is ignored. For stencil-only formats, the initial and final layouts of the stencil aspect are taken from the VkAttachmentDescriptionStencilLayout structure if present, or `initialLayout` and `finalLayout` if not present.

If `format` is a depth/stencil format, and either `initialLayout` or `finalLayout` does not specify a layout for the stencil aspect, then the application must specify the initial and final layouts of the stencil aspect by including a VkAttachmentDescriptionStencilLayout structure in the `pNext` chain.

`loadOp` and `storeOp` are ignored for fragment shading rate attachments. No access to the shading rate attachment is performed in `loadOp` and `storeOp`. Instead, access to `VK_ACCESS_FRAGMENT_SHADING_RATE_ATTACHMENT_READ_BIT_KHR` is performed as fragments are rasterized.

Valid Usage

- VUID-VkAttachmentDescription2-format-06699
  If `format` includes a color or depth component and `loadOp` is `VK_ATTACHMENT_LOAD_OP_LOAD`, then `initialLayout` must not be `VK_IMAGE_LAYOUT_UNDEFINED`

- VUID-VkAttachmentDescription2-finalLayout-00843
  `finalLayout` must not be `VK_IMAGE_LAYOUT_UNDEFINED` or `VK_IMAGE_LAYOUT_PREINITIALIZED`

- VUID-VkAttachmentDescription2-format-03280
  If `format` is a color format, `initialLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription2-format-03281
  If `format` is a depth/stencil format, `initialLayout` must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL`

- VUID-VkAttachmentDescription2-format-03282
  If `format` is a color format, `finalLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription2-format-03283
  If `format` is a depth/stencil format, `finalLayout` must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL`

- VUID-VkAttachmentDescription2-format-06487
  If `format` is a color format, `initialLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkAttachmentDescription2-format-06488
  If `format` is a color format, `finalLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkAttachmentDescription2-separateDepthStencilLayouts-03284
  If the `separateDepthStencilLayouts` feature is not enabled, `initialLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`,

- VUID-VkAttachmentDescription2-separateDepthStencilLayouts-03285
  If the `separateDepthStencilLayouts` feature is not enabled, `finalLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`,

- VUID-VkAttachmentDescription2-format-03286
  If `format` is a color format, `initialLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription2-format-03287
  If `format` is a color format, `finalLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription2-format-06906
  If `format` is a depth/stencil format which includes both depth and stencil components, `initialLayout` must not be `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription2-format-06907
  If `format` is a depth/stencil format which includes both depth and stencil components, `finalLayout` must not be `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription2-format-03290
  If `format` is a depth/stencil format which includes only the depth component, `initialLayout` must not be `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription2-format-03291
  If `format` is a depth/stencil format which includes only the depth component, `finalLayout` must not be `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription2-synchronization2-06908
  If the `synchronization2` feature is not enabled, `initialLayout` must not be `VK_IMAGE_LAYOUT_ATTACHMENT_OPTIMAL_KHR` or `VK_IMAGE_LAYOUT_READ_ONLY_OPTIMAL_KHR`

- VUID-VkAttachmentDescription2-synchronization2-06909
  If the `synchronization2` feature is not enabled, `finalLayout` must not be `VK_IMAGE_LAYOUT_ATTACHMENT_OPTIMAL_KHR` or `VK_IMAGE_LAYOUT_READ_ONLY_OPTIMAL_KHR`

- VUID-VkAttachmentDescription2-attachmentFeedbackLoopLayout-07309
  If the `attachmentFeedbackLoopLayout` feature is not enabled, `initialLayout` must not be `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT`

- VUID-VkAttachmentDescription2-attachmentFeedbackLoopLayout-07310
  If the `attachmentFeedbackLoopLayout` feature is not enabled, `finalLayout` must not be `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT`

- VUID-VkAttachmentDescription2-samples-08745
  `samples` must be a valid VkSampleCountFlagBits value that is set in `imageCreateSampleCounts` (as defined in Image Creation Limits) for the given `format`

- VUID-VkAttachmentDescription2-dynamicRenderingLocalRead-09544
  If the `dynamicRenderingLocalRead` feature is not enabled, `initialLayout` must not be `VK_IMAGE_LAYOUT_RENDERING_LOCAL_READ`

- VUID-VkAttachmentDescription2-dynamicRenderingLocalRead-09545
  If the `dynamicRenderingLocalRead` feature is not enabled, `finalLayout` must not be `VK_IMAGE_LAYOUT_RENDERING_LOCAL_READ`

- VUID-VkAttachmentDescription2-pNext-06704
  If the `pNext` chain does not include a VkAttachmentDescriptionStencilLayout structure, `format` includes a stencil component, and `stencilLoadOp` is `VK_ATTACHMENT_LOAD_OP_LOAD`, then `initialLayout` must not be `VK_IMAGE_LAYOUT_UNDEFINED`

- VUID-VkAttachmentDescription2-pNext-06705
  If the `pNext` chain includes a VkAttachmentDescriptionStencilLayout structure, `format` includes a stencil component, and `stencilLoadOp` is `VK_ATTACHMENT_LOAD_OP_LOAD`, then VkAttachmentDescriptionStencilLayout::`stencilInitialLayout` must not be `VK_IMAGE_LAYOUT_UNDEFINED`

- VUID-VkAttachmentDescription2-format-06249
  If `format` is a depth/stencil format which includes both depth and stencil components, and `initialLayout` is `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, the `pNext` chain must include a VkAttachmentDescriptionStencilLayout structure

- VUID-VkAttachmentDescription2-format-06250
  If `format` is a depth/stencil format which includes both depth and stencil components, and `finalLayout` is `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, the `pNext` chain must include a VkAttachmentDescriptionStencilLayout structure

- VUID-VkAttachmentDescription2-format-06247
  If the `pNext` chain does not include a VkAttachmentDescriptionStencilLayout structure and `format` only includes a stencil component, `initialLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription2-format-06248
  If the `pNext` chain does not include a VkAttachmentDescriptionStencilLayout structure and `format` only includes a stencil component, `finalLayout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`

- VUID-VkAttachmentDescription2-format-09332
  If the `externalFormatResolve` feature is not enabled, `format` must not be `VK_FORMAT_UNDEFINED`

- VUID-VkAttachmentDescription2-format-09334
  If `format` is `VK_FORMAT_UNDEFINED`, there must be a VkExternalFormatANDROID structure in the `pNext` chain with a `externalFormat` that is not equal to `0`

Valid Usage (Implicit)

- VUID-VkAttachmentDescription2-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_ATTACHMENT_DESCRIPTION_2`

- VUID-VkAttachmentDescription2-pNext-pNext
  Each `pNext` member of any structure (including this one) in the `pNext` chain must be either `NULL` or a pointer to a valid instance of VkAttachmentDescriptionStencilLayout or VkExternalFormatANDROID

- VUID-VkAttachmentDescription2-sType-unique
  The `sType` value of each struct in the `pNext` chain must be unique

- VUID-VkAttachmentDescription2-flags-parameter
  `flags` must be a valid combination of VkAttachmentDescriptionFlagBits values

- VUID-VkAttachmentDescription2-format-parameter
  `format` must be a valid VkFormat value

- VUID-VkAttachmentDescription2-samples-parameter
  `samples` must be a valid VkSampleCountFlagBits value

- VUID-VkAttachmentDescription2-loadOp-parameter
  `loadOp` must be a valid VkAttachmentLoadOp value

- VUID-VkAttachmentDescription2-storeOp-parameter
  `storeOp` must be a valid VkAttachmentStoreOp value

- VUID-VkAttachmentDescription2-stencilLoadOp-parameter
  `stencilLoadOp` must be a valid VkAttachmentLoadOp value

- VUID-VkAttachmentDescription2-stencilStoreOp-parameter
  `stencilStoreOp` must be a valid VkAttachmentStoreOp value

- VUID-VkAttachmentDescription2-initialLayout-parameter
  `initialLayout` must be a valid VkImageLayout value

- VUID-VkAttachmentDescription2-finalLayout-parameter
  `finalLayout` must be a valid VkImageLayout value

The `VkAttachmentDescriptionStencilLayout` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkAttachmentDescriptionStencilLayout {
        VkStructureType    sType;
        void*              pNext;
        VkImageLayout      stencilInitialLayout;
        VkImageLayout      stencilFinalLayout;
    } VkAttachmentDescriptionStencilLayout;

or the equivalent

    // Provided by VK_KHR_separate_depth_stencil_layouts
    typedef VkAttachmentDescriptionStencilLayout VkAttachmentDescriptionStencilLayoutKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `stencilInitialLayout` is the layout the stencil aspect of the attachment image subresource will be in when a render pass instance begins.

- `stencilFinalLayout` is the layout the stencil aspect of the attachment image subresource will be transitioned to when a render pass instance ends.

Valid Usage

- VUID-VkAttachmentDescriptionStencilLayout-stencilInitialLayout-03308
  `stencilInitialLayout` must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL`, or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkAttachmentDescriptionStencilLayout-stencilFinalLayout-03309
  `stencilFinalLayout` must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL`, or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkAttachmentDescriptionStencilLayout-stencilFinalLayout-03310
  `stencilFinalLayout` must not be `VK_IMAGE_LAYOUT_UNDEFINED` or `VK_IMAGE_LAYOUT_PREINITIALIZED`

Valid Usage (Implicit)

- VUID-VkAttachmentDescriptionStencilLayout-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_ATTACHMENT_DESCRIPTION_STENCIL_LAYOUT`

- VUID-VkAttachmentDescriptionStencilLayout-stencilInitialLayout-parameter
  `stencilInitialLayout` must be a valid VkImageLayout value

- VUID-VkAttachmentDescriptionStencilLayout-stencilFinalLayout-parameter
  `stencilFinalLayout` must be a valid VkImageLayout value

The `VkSubpassDescription2` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkSubpassDescription2 {
        VkStructureType                  sType;
        const void*                      pNext;
        VkSubpassDescriptionFlags        flags;
        VkPipelineBindPoint              pipelineBindPoint;
        uint32_t                         viewMask;
        uint32_t                         inputAttachmentCount;
        const VkAttachmentReference2*    pInputAttachments;
        uint32_t                         colorAttachmentCount;
        const VkAttachmentReference2*    pColorAttachments;
        const VkAttachmentReference2*    pResolveAttachments;
        const VkAttachmentReference2*    pDepthStencilAttachment;
        uint32_t                         preserveAttachmentCount;
        const uint32_t*                  pPreserveAttachments;
    } VkSubpassDescription2;

or the equivalent

    // Provided by VK_KHR_create_renderpass2
    typedef VkSubpassDescription2 VkSubpassDescription2KHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `flags` is a bitmask of VkSubpassDescriptionFlagBits specifying usage of the subpass.

- `pipelineBindPoint` is a VkPipelineBindPoint value specifying the pipeline type supported for this subpass.

- `viewMask` is a bitfield of view indices describing which views rendering is broadcast to in this subpass, when multiview is enabled.

- `inputAttachmentCount` is the number of input attachments.

- `pInputAttachments` is a pointer to an array of VkAttachmentReference2 structures defining the input attachments for this subpass and their layouts.

- `colorAttachmentCount` is the number of color attachments.

- `pColorAttachments` is a pointer to an array of `colorAttachmentCount` VkAttachmentReference2 structures defining the color attachments for this subpass and their layouts.

- `pResolveAttachments` is `NULL` or a pointer to an array of `colorAttachmentCount` VkAttachmentReference2 structures defining the resolve attachments for this subpass and their layouts.

- `pDepthStencilAttachment` is a pointer to a VkAttachmentReference2 structure specifying the depth/stencil attachment for this subpass and its layout.

- `preserveAttachmentCount` is the number of preserved attachments.

- `pPreserveAttachments` is a pointer to an array of `preserveAttachmentCount` render pass attachment indices identifying attachments that are not used by this subpass, but whose contents must be preserved throughout the subpass.

Parameters defined by this structure with the same name as those in VkSubpassDescription have the identical effect to those parameters.

`viewMask` has the same effect for the described subpass as VkRenderPassMultiviewCreateInfo::`pViewMasks` has on each corresponding subpass.

If a VkFragmentShadingRateAttachmentInfoKHR structure is included in the `pNext` chain, `pFragmentShadingRateAttachment` is not `NULL`, and its `attachment` member is not `VK_ATTACHMENT_UNUSED`, the identified attachment defines a fragment shading rate attachment for that subpass.

If any element of `pResolveAttachments` is an image specified with an VkExternalFormatANDROID, values in the corresponding color attachment will be resolved to the resolve attachment in the same manner as specified for `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`.

If the `nullColorAttachmentWithExternalFormatResolve` limit is `VK_TRUE`, values in the color attachment will be loaded from the resolve attachment at the start of rendering, and may also be reloaded any time after a resolve occurs or the resolve attachment is written to; if this occurs it must happen-before any writes to the color attachment are performed which happen-after the resolve that triggers this. If any color component in the external format is subsampled, values will be read from the nearest sample in the image when they are loaded. If the color attachment is also used as an input attachment, the same behavior applies.

Setting the color attachment to `VK_ATTACHMENT_UNUSED` when an external resolve attachment is used and the `nullColorAttachmentWithExternalFormatResolve` limit is `VK_TRUE` will not result in color attachment writes to be discarded for that attachment.

When `nullColorAttachmentWithExternalFormatResolve` is `VK_TRUE`, the color output from the subpass can still be read via an input attachment; but the application cannot bind an image view for the color attachment as there is no such image view bound. Instead to access the data as an input attachment applications can use the resolve attachment in its place - using the resolve attachment image for the descriptor, and setting the corresponding element of `pInputAttachments` to the index of the resolve attachment.

Loads or input attachment reads from the resolve attachment are performed as if using a VkSamplerYcbcrConversionCreateInfo with the following parameters:

    VkSamplerYcbcrConversionCreateInfo createInfo = {
        .sType = VK_STRUCTURE_TYPE_SAMPLER_YCBCR_CONVERSION_CREATE_INFO,
        .pNext = NULL,
        .format = VK_FORMAT_UNDEFINED,
        .ycbcrModel = VK_SAMPLER_YCBCR_MODEL_CONVERSION_RGB_IDENTITY,
        .ycbcrRange = VK_SAMPLER_YCBCR_RANGE_ITU_FULL,
        .components = {
            .r = VK_COMPONENT_SWIZZLE_B
            .g = VK_COMPONENT_SWIZZLE_R
            .b = VK_COMPONENT_SWIZZLE_G
            .a = VK_COMPONENT_SWIZZLE_IDENTITY},
        .xChromaOffset = properties.chromaOffsetX,
        .yChromaOffset = properties.chromaOffsetY,
        .chromaFilter = VK_FILTER_NEAREST,
        .forceExplicitReconstruction = ... };

where `properties` is equal to VkPhysicalDeviceExternalFormatResolvePropertiesANDROID returned by the device and `forceExplicitReconstruction` is effectively ignored as the `VK_SAMPLER_YCBCR_MODEL_CONVERSION_RGB_IDENTITY` model is used. The applied swizzle is the same effective swizzle that would be applied by the `VK_SAMPLER_YCBCR_MODEL_CONVERSION_YCBCR_IDENTITY` model, but no range expansion is applied.

Valid Usage

- VUID-VkSubpassDescription2-attachment-06912
  If the `attachment` member of an element of `pInputAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkSubpassDescription2-attachment-06913
  If the `attachment` member of an element of `pColorAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL`

- VUID-VkSubpassDescription2-attachment-06914
  If the `attachment` member of an element of `pResolveAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL`

- VUID-VkSubpassDescription2-attachment-06915
  If the `attachment` member of `pDepthStencilAttachment` is not `VK_ATTACHMENT_UNUSED`, ts `layout` member must not be `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL`

- VUID-VkSubpassDescription2-attachment-06916
  If the `attachment` member of an element of `pColorAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkSubpassDescription2-attachment-06917
  If the `attachment` member of an element of `pResolveAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL` or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkSubpassDescription2-attachment-06918
  If the `attachment` member of an element of `pInputAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`

- VUID-VkSubpassDescription2-attachment-06919
  If the `attachment` member of an element of `pColorAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkSubpassDescription2-attachment-06920
  If the `attachment` member of an element of `pResolveAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkSubpassDescription2-attachment-06921
  If the `attachment` member of an element of `pInputAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_ATTACHMENT_OPTIMAL_KHR`

- VUID-VkSubpassDescription2-attachment-06922
  If the `attachment` member of an element of `pColorAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_READ_ONLY_OPTIMAL_KHR`

- VUID-VkSubpassDescription2-attachment-06923
  If the `attachment` member of an element of `pResolveAttachments` is not `VK_ATTACHMENT_UNUSED`, its `layout` member must not be `VK_IMAGE_LAYOUT_READ_ONLY_OPTIMAL_KHR`

- VUID-VkSubpassDescription2-attachment-06251
  If the `attachment` member of `pDepthStencilAttachment` is not `VK_ATTACHMENT_UNUSED` and its `pNext` chain includes a VkAttachmentReferenceStencilLayout structure, the `layout` member of `pDepthStencilAttachment` must not be `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL` or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`

- VUID-VkSubpassDescription2-pipelineBindPoint-04953
  `pipelineBindPoint` must be `VK_PIPELINE_BIND_POINT_GRAPHICS` or `VK_PIPELINE_BIND_POINT_SUBPASS_SHADING_HUAWEI`

- VUID-VkSubpassDescription2-colorAttachmentCount-03063
  `colorAttachmentCount` must be less than or equal to `VkPhysicalDeviceLimits`::`maxColorAttachments`

- VUID-VkSubpassDescription2-loadOp-03064
  If the first use of an attachment in this render pass is as an input attachment, and the attachment is not also used as a color or depth/stencil attachment in the same subpass, then `loadOp` must not be `VK_ATTACHMENT_LOAD_OP_CLEAR`

- VUID-VkSubpassDescription2-pResolveAttachments-03067
  If `pResolveAttachments` is not `NULL`, each resolve attachment that is not `VK_ATTACHMENT_UNUSED` must have a sample count of `VK_SAMPLE_COUNT_1_BIT`

- VUID-VkSubpassDescription2-externalFormatResolve-09335
  If the `externalFormatResolve` feature is not enabled and `pResolveAttachments` is not `NULL`, for each resolve attachment that does not have the value `VK_ATTACHMENT_UNUSED`, the corresponding color attachment must not have the value `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescription2-nullColorAttachmentWithExternalFormatResolve-09336
  If the `nullColorAttachmentWithExternalFormatResolve` property is `VK_FALSE` and `pResolveAttachments` is not `NULL`, for each resolve attachment that has a format of `VK_FORMAT_UNDEFINED`, the corresponding color attachment must not have the value `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescription2-nullColorAttachmentWithExternalFormatResolve-09337
  If the `nullColorAttachmentWithExternalFormatResolve` property is `VK_TRUE` and `pResolveAttachments` is not `NULL`, for each resolve attachment that has a format of `VK_FORMAT_UNDEFINED`, the corresponding color attachment must have the value `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescription2-externalFormatResolve-09338
  If the `externalFormatResolve` feature is not enabled and `pResolveAttachments` is not `NULL`, for each resolve attachment that is not `VK_ATTACHMENT_UNUSED`, the corresponding color attachment must not have a sample count of `VK_SAMPLE_COUNT_1_BIT`

- VUID-VkSubpassDescription2-externalFormatResolve-09339
  If the `externalFormatResolve` feature is not enabled, each element of `pResolveAttachments` must have the same VkFormat as its corresponding color attachment

- VUID-VkSubpassDescription2-multisampledRenderToSingleSampled-06869
  If the `multisampledRenderToSingleSampled` feature is not enabled, all attachments in `pColorAttachments` that are not `VK_ATTACHMENT_UNUSED` must have the same sample count

- VUID-VkSubpassDescription2-pInputAttachments-02897
  All attachments in `pInputAttachments` that are not `VK_ATTACHMENT_UNUSED` and any of the following is true:

  - the `externalFormatResolve` feature is not enabled

  - the `nullColorAttachmentWithExternalFormatResolve` property is `VK_FALSE`

  - does not have a non-zero value of VkExternalFormatANDROID::`externalFormat`

  must have image formats whose potential format features contain at least `VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT` or `VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkSubpassDescription2-pColorAttachments-02898
  All attachments in `pColorAttachments` that are not `VK_ATTACHMENT_UNUSED` must have image formats whose potential format features contain `VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT`

- VUID-VkSubpassDescription2-pResolveAttachments-09343
  All attachments in `pResolveAttachments` that are not `VK_ATTACHMENT_UNUSED` and do not have an image format of `VK_FORMAT_UNDEFINED` must have image formats whose potential format features contain `VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT`

- VUID-VkSubpassDescription2-pDepthStencilAttachment-02900
  If `pDepthStencilAttachment` is not `NULL` and the attachment is not `VK_ATTACHMENT_UNUSED` then it must have an image format whose potential format features contain `VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkSubpassDescription2-linearColorAttachment-06499
  If the `linearColorAttachment` feature is enabled and the image is created with `VK_IMAGE_TILING_LINEAR`, all attachments in `pInputAttachments` that are not `VK_ATTACHMENT_UNUSED` must have image formats whose potential format features must contain `VK_FORMAT_FEATURE_2_LINEAR_COLOR_ATTACHMENT_BIT_NV`

- VUID-VkSubpassDescription2-linearColorAttachment-06500
  If the `linearColorAttachment` feature is enabled and the image is created with `VK_IMAGE_TILING_LINEAR`, all attachments in `pColorAttachments` that are not `VK_ATTACHMENT_UNUSED` must have image formats whose potential format features must contain `VK_FORMAT_FEATURE_2_LINEAR_COLOR_ATTACHMENT_BIT_NV`

- VUID-VkSubpassDescription2-linearColorAttachment-06501
  If the `linearColorAttachment` feature is enabled and the image is created with `VK_IMAGE_TILING_LINEAR`, all attachments in `pResolveAttachments` that are not `VK_ATTACHMENT_UNUSED` must have image formats whose potential format features must contain `VK_FORMAT_FEATURE_2_LINEAR_COLOR_ATTACHMENT_BIT_NV`

- VUID-VkSubpassDescription2-None-09456
  If either of the following is enabled:

  - The `VK_AMD_mixed_attachment_samples` extension

  - The `VK_NV_framebuffer_mixed_samples` extension

  all attachments in `pColorAttachments` that are not `VK_ATTACHMENT_UNUSED` must have a sample count that is smaller than or equal to the sample count of `pDepthStencilAttachment` if it is not `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescription2-pNext-06870
  If the `pNext` chain includes a VkMultisampledRenderToSingleSampledInfoEXT structure with `multisampledRenderToSingleSampledEnable` equal to `VK_TRUE`, then all attachments in `pColorAttachments` and `pDepthStencilAttachment` that are not `VK_ATTACHMENT_UNUSED` must have a sample count that is either `VK_SAMPLE_COUNT_1_BIT` or equal to VkMultisampledRenderToSingleSampledInfoEXT::`rasterizationSamples`

- VUID-VkSubpassDescription2-pNext-06871
  If the `pNext` chain includes a VkMultisampledRenderToSingleSampledInfoEXT structure with `multisampledRenderToSingleSampledEnable` equal to `VK_TRUE`, and `pDepthStencilAttachment` is not `NULL`, does not have the value `VK_ATTACHMENT_UNUSED`, and has a sample count of `VK_SAMPLE_COUNT_1_BIT`, the `pNext` chain must also include a VkSubpassDescriptionDepthStencilResolve structure with `pDepthStencilResolveAttachment` that is either `NULL` or has the value `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescription2-multisampledRenderToSingleSampled-06872
  All attachments in `pDepthStencilAttachment` or `pColorAttachments` that are not `VK_ATTACHMENT_UNUSED` must have the same sample count , if none of the following are enabled:

  - The `VK_AMD_mixed_attachment_samples` extension

  - The `VK_NV_framebuffer_mixed_samples` extension

  - The `multisampledRenderToSingleSampled` feature,

- VUID-VkSubpassDescription2-attachment-03073
  Each element of `pPreserveAttachments` must not be `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescription2-pPreserveAttachments-03074
  Each element of `pPreserveAttachments` must not also be an element of any other member of the subpass description

- VUID-VkSubpassDescription2-layout-02528
  If any attachment is used by more than one VkAttachmentReference2 member, then each use must use the same `layout`

- VUID-VkSubpassDescription2-flags-03076
  If `flags` includes `VK_SUBPASS_DESCRIPTION_PER_VIEW_POSITION_X_ONLY_BIT_NVX`, it must also include `VK_SUBPASS_DESCRIPTION_PER_VIEW_ATTRIBUTES_BIT_NVX`

- VUID-VkSubpassDescription2-attachment-02799
  If the `attachment` member of any element of `pInputAttachments` is not `VK_ATTACHMENT_UNUSED`, then the `aspectMask` member must be a valid combination of VkImageAspectFlagBits

- VUID-VkSubpassDescription2-attachment-02800
  If the `attachment` member of any element of `pInputAttachments` is not `VK_ATTACHMENT_UNUSED`, then the `aspectMask` member must not be `0`

- VUID-VkSubpassDescription2-attachment-02801
  If the `attachment` member of any element of `pInputAttachments` is not `VK_ATTACHMENT_UNUSED`, then the `aspectMask` member must not include `VK_IMAGE_ASPECT_METADATA_BIT`

- VUID-VkSubpassDescription2-attachment-04563
  If the `attachment` member of any element of `pInputAttachments` is not `VK_ATTACHMENT_UNUSED`, then the `aspectMask` member must not include `VK_IMAGE_ASPECT_MEMORY_PLANE_i_BIT_EXT` for any index i

- VUID-VkSubpassDescription2-pDepthStencilAttachment-04440
  An attachment must not be used in both `pDepthStencilAttachment` and `pColorAttachments`

- VUID-VkSubpassDescription2-multiview-06558
  If the `multiview` feature is not enabled, `viewMask` must be `0`

- VUID-VkSubpassDescription2-viewMask-06706
  The index of the most significant bit in `viewMask` must be less than `maxMultiviewViewCount`

- VUID-VkSubpassDescription2-externalFormatResolve-09344
  If the `externalFormatResolve` feature is enabled, `pResolveAttachments` is not `NULL`, and `colorAttachmentCount` is not `1`, any element of `pResolveAttachments` that is not `VK_ATTACHMENT_UNUSED`, must not have a format of `VK_FORMAT_UNDEFINED`

- VUID-VkSubpassDescription2-externalFormatResolve-09345
  If the `externalFormatResolve` feature is enabled, `pResolveAttachments` is not `NULL`, any element of `pResolveAttachments` is not `VK_ATTACHMENT_UNUSED` and has a format of `VK_FORMAT_UNDEFINED`, and the corresponding element of `pColorAttachments` is not `VK_ATTACHMENT_UNUSED`, the color attachment must have a `samples` value of `1`

- VUID-VkSubpassDescription2-externalFormatResolve-09346
  If the `externalFormatResolve` feature is enabled, `pResolveAttachments` is not `NULL`, and any element of `pResolveAttachments` is not `VK_ATTACHMENT_UNUSED` and has a format of `VK_FORMAT_UNDEFINED`, `viewMask` must be `0`

- VUID-VkSubpassDescription2-externalFormatResolve-09347
  If the `externalFormatResolve` feature is enabled, `pResolveAttachments` is not `NULL`, and any element of `pResolveAttachments` is not `VK_ATTACHMENT_UNUSED` and has a format of `VK_FORMAT_UNDEFINED`, VkFragmentShadingRateAttachmentInfoKHR::`pFragmentShadingRateAttachment` must either be `NULL` or a VkAttachmentReference2 structure with an `attachment` value of `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescription2-externalFormatResolve-09348
  If the `externalFormatResolve` feature is enabled, `pResolveAttachments` is not `NULL`, and any element of `pResolveAttachments` is not `VK_ATTACHMENT_UNUSED` and has a format of `VK_FORMAT_UNDEFINED`, elements of `pInputAttachments` referencing either a color attachment or resolve attachment used in this subpass must not include `VK_IMAGE_ASPECT_PLANE_i_BIT` for any index i in its `aspectMask`

Valid Usage (Implicit)

- VUID-VkSubpassDescription2-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_SUBPASS_DESCRIPTION_2`

- VUID-VkSubpassDescription2-pNext-pNext
  Each `pNext` member of any structure (including this one) in the `pNext` chain must be either `NULL` or a pointer to a valid instance of VkFragmentShadingRateAttachmentInfoKHR, VkMultisampledRenderToSingleSampledInfoEXT, VkRenderPassCreationControlEXT, VkRenderPassSubpassFeedbackCreateInfoEXT, or VkSubpassDescriptionDepthStencilResolve

- VUID-VkSubpassDescription2-sType-unique
  The `sType` value of each struct in the `pNext` chain must be unique

- VUID-VkSubpassDescription2-flags-parameter
  `flags` must be a valid combination of VkSubpassDescriptionFlagBits values

- VUID-VkSubpassDescription2-pipelineBindPoint-parameter
  `pipelineBindPoint` must be a valid VkPipelineBindPoint value

- VUID-VkSubpassDescription2-pInputAttachments-parameter
  If `inputAttachmentCount` is not `0`, `pInputAttachments` must be a valid pointer to an array of `inputAttachmentCount` valid VkAttachmentReference2 structures

- VUID-VkSubpassDescription2-pColorAttachments-parameter
  If `colorAttachmentCount` is not `0`, `pColorAttachments` must be a valid pointer to an array of `colorAttachmentCount` valid VkAttachmentReference2 structures

- VUID-VkSubpassDescription2-pResolveAttachments-parameter
  If `colorAttachmentCount` is not `0`, and `pResolveAttachments` is not `NULL`, `pResolveAttachments` must be a valid pointer to an array of `colorAttachmentCount` valid VkAttachmentReference2 structures

- VUID-VkSubpassDescription2-pDepthStencilAttachment-parameter
  If `pDepthStencilAttachment` is not `NULL`, `pDepthStencilAttachment` must be a valid pointer to a valid VkAttachmentReference2 structure

- VUID-VkSubpassDescription2-pPreserveAttachments-parameter
  If `preserveAttachmentCount` is not `0`, `pPreserveAttachments` must be a valid pointer to an array of `preserveAttachmentCount` `uint32_t` values

The `VkSubpassDescriptionDepthStencilResolve` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkSubpassDescriptionDepthStencilResolve {
        VkStructureType                  sType;
        const void*                      pNext;
        VkResolveModeFlagBits            depthResolveMode;
        VkResolveModeFlagBits            stencilResolveMode;
        const VkAttachmentReference2*    pDepthStencilResolveAttachment;
    } VkSubpassDescriptionDepthStencilResolve;

or the equivalent

    // Provided by VK_KHR_depth_stencil_resolve
    typedef VkSubpassDescriptionDepthStencilResolve VkSubpassDescriptionDepthStencilResolveKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `depthResolveMode` is a VkResolveModeFlagBits value describing the depth resolve mode.

- `stencilResolveMode` is a VkResolveModeFlagBits value describing the stencil resolve mode.

- `pDepthStencilResolveAttachment` is `NULL` or a pointer to a VkAttachmentReference2 structure defining the depth/stencil resolve attachment for this subpass and its layout.

If the `pNext` chain of VkSubpassDescription2 includes a `VkSubpassDescriptionDepthStencilResolve` structure, then that structure describes multisample resolve operations for the depth/stencil attachment in a subpass. If this structure is not included in the `pNext` chain of VkSubpassDescription2, or if it is and either `pDepthStencilResolveAttachment` is `NULL` or its attachment index is `VK_ATTACHMENT_UNUSED`, it indicates that no depth/stencil resolve attachment will be used in the subpass.

Valid Usage

- VUID-VkSubpassDescriptionDepthStencilResolve-pDepthStencilResolveAttachment-03177
  If `pDepthStencilResolveAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED`, `pDepthStencilAttachment` must not be `NULL` or have the value `VK_ATTACHMENT_UNUSED`

- VUID-VkSubpassDescriptionDepthStencilResolve-pDepthStencilResolveAttachment-03179
  If `pDepthStencilResolveAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED`, `pDepthStencilAttachment` must not have a sample count of `VK_SAMPLE_COUNT_1_BIT`

- VUID-VkSubpassDescriptionDepthStencilResolve-pDepthStencilResolveAttachment-03180
  If `pDepthStencilResolveAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED`, `pDepthStencilResolveAttachment` must have a sample count of `VK_SAMPLE_COUNT_1_BIT`

- VUID-VkSubpassDescriptionDepthStencilResolve-pDepthStencilResolveAttachment-02651
  If `pDepthStencilResolveAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED` then it must have an image format whose potential format features contain `VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkSubpassDescriptionDepthStencilResolve-pDepthStencilResolveAttachment-03181
  If `pDepthStencilResolveAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED` and VkFormat of `pDepthStencilResolveAttachment` has a depth component, then the VkFormat of `pDepthStencilAttachment` must have a depth component with the same number of bits and numeric format

- VUID-VkSubpassDescriptionDepthStencilResolve-pDepthStencilResolveAttachment-03182
  If `pDepthStencilResolveAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED`, and VkFormat of `pDepthStencilResolveAttachment` has a stencil component, then the VkFormat of `pDepthStencilAttachment` must have a stencil component with the same number of bits and numeric format

- VUID-VkSubpassDescriptionDepthStencilResolve-pDepthStencilResolveAttachment-03178
  If `pDepthStencilResolveAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED`, `depthResolveMode` and `stencilResolveMode` must not both be `VK_RESOLVE_MODE_NONE`

- VUID-VkSubpassDescriptionDepthStencilResolve-depthResolveMode-03183
  If `pDepthStencilResolveAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED` and the VkFormat of `pDepthStencilResolveAttachment` has a depth component, then the value of `depthResolveMode` must be one of the bits set in VkPhysicalDeviceDepthStencilResolveProperties::`supportedDepthResolveModes` or `VK_RESOLVE_MODE_NONE`

- VUID-VkSubpassDescriptionDepthStencilResolve-stencilResolveMode-03184
  If `pDepthStencilResolveAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED` and the VkFormat of `pDepthStencilResolveAttachment` has a stencil component, then the value of `stencilResolveMode` must be one of the bits set in VkPhysicalDeviceDepthStencilResolveProperties::`supportedStencilResolveModes` or `VK_RESOLVE_MODE_NONE`

- VUID-VkSubpassDescriptionDepthStencilResolve-pDepthStencilResolveAttachment-03185
  If `pDepthStencilResolveAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED`, the VkFormat of `pDepthStencilResolveAttachment` has both depth and stencil components, VkPhysicalDeviceDepthStencilResolveProperties::`independentResolve` is `VK_FALSE`, and VkPhysicalDeviceDepthStencilResolveProperties::`independentResolveNone` is `VK_FALSE`, then the values of `depthResolveMode` and `stencilResolveMode` must be identical

- VUID-VkSubpassDescriptionDepthStencilResolve-pDepthStencilResolveAttachment-03186
  If `pDepthStencilResolveAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED`, the VkFormat of `pDepthStencilResolveAttachment` has both depth and stencil components, VkPhysicalDeviceDepthStencilResolveProperties::`independentResolve` is `VK_FALSE` and VkPhysicalDeviceDepthStencilResolveProperties::`independentResolveNone` is `VK_TRUE`, then the values of `depthResolveMode` and `stencilResolveMode` must be identical or one of them must be `VK_RESOLVE_MODE_NONE`

- VUID-VkSubpassDescriptionDepthStencilResolve-pNext-06873
  If the `pNext` chain of VkSubpassDescription2 includes a `VkMultisampledRenderToSingleSampledInfoEXT` structure, the `multisampledRenderToSingleSampledEnable` field is `VK_TRUE`, and `pDepthStencilAttachment` is not `NULL` and does not have the value `VK_ATTACHMENT_UNUSED`, `depthResolveMode` and `stencilResolveMode` must not both be `VK_RESOLVE_MODE_NONE`

- VUID-VkSubpassDescriptionDepthStencilResolve-pNext-06874
  If the `pNext` chain of VkSubpassDescription2 includes a `VkMultisampledRenderToSingleSampledInfoEXT` structure whose `multisampledRenderToSingleSampledEnable` field is `VK_TRUE`, and `pDepthStencilAttachment` is not `NULL`, does not have the value `VK_ATTACHMENT_UNUSED`, and has a VkFormat that has a depth component, then the value of `depthResolveMode` must be one of the bits set in VkPhysicalDeviceDepthStencilResolveProperties::`supportedDepthResolveModes` or `VK_RESOLVE_MODE_NONE`

- VUID-VkSubpassDescriptionDepthStencilResolve-pNext-06875
  If the `pNext` chain of VkSubpassDescription2 includes a `VkMultisampledRenderToSingleSampledInfoEXT` structure whose `multisampledRenderToSingleSampledEnable` field is `VK_TRUE`, and `pDepthStencilAttachment` is not `NULL`, does not have the value `VK_ATTACHMENT_UNUSED`, and has a VkFormat with a stencil component, then the value of `stencilResolveMode` must be one of the bits set in VkPhysicalDeviceDepthStencilResolveProperties::`supportedStencilResolveModes` or `VK_RESOLVE_MODE_NONE`

- VUID-VkSubpassDescriptionDepthStencilResolve-pNext-06876
  If the `pNext` chain of VkSubpassDescription2 includes a `VkMultisampledRenderToSingleSampledInfoEXT` structure whose `multisampledRenderToSingleSampledEnable` field is `VK_TRUE`, `pDepthStencilAttachment` is not `NULL`, does not have the value `VK_ATTACHMENT_UNUSED`, and has a VkFormat with both depth and stencil components, and both VkPhysicalDeviceDepthStencilResolveProperties::`independentResolve` and VkPhysicalDeviceDepthStencilResolveProperties::`independentResolveNone` are `VK_FALSE`, then the values of `depthResolveMode` and `stencilResolveMode` must be identical

- VUID-VkSubpassDescriptionDepthStencilResolve-pNext-06877
  If the `pNext` chain of VkSubpassDescription2 includes a `VkMultisampledRenderToSingleSampledInfoEXT` structure whose `multisampledRenderToSingleSampledEnable` field is `VK_TRUE`, `pDepthStencilAttachment` is not `NULL`, does not have the value `VK_ATTACHMENT_UNUSED`, and has a VkFormat with both depth and stencil components, VkPhysicalDeviceDepthStencilResolveProperties::`independentResolve` is `VK_FALSE`, and VkPhysicalDeviceDepthStencilResolveProperties::`independentResolveNone` is `VK_TRUE`, then the values of `depthResolveMode` and `stencilResolveMode` must be identical or one of them must be `VK_RESOLVE_MODE_NONE`

Valid Usage (Implicit)

- VUID-VkSubpassDescriptionDepthStencilResolve-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_SUBPASS_DESCRIPTION_DEPTH_STENCIL_RESOLVE`

- VUID-VkSubpassDescriptionDepthStencilResolve-pDepthStencilResolveAttachment-parameter
  If `pDepthStencilResolveAttachment` is not `NULL`, `pDepthStencilResolveAttachment` must be a valid pointer to a valid VkAttachmentReference2 structure

The `VkFragmentShadingRateAttachmentInfoKHR` structure is defined as:

    // Provided by VK_KHR_fragment_shading_rate
    typedef struct VkFragmentShadingRateAttachmentInfoKHR {
        VkStructureType                  sType;
        const void*                      pNext;
        const VkAttachmentReference2*    pFragmentShadingRateAttachment;
        VkExtent2D                       shadingRateAttachmentTexelSize;
    } VkFragmentShadingRateAttachmentInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `pFragmentShadingRateAttachment` is `NULL` or a pointer to a VkAttachmentReference2 structure defining the fragment shading rate attachment for this subpass.

- `shadingRateAttachmentTexelSize` specifies the size of the portion of the framebuffer corresponding to each texel in `pFragmentShadingRateAttachment`.

If no shading rate attachment is specified, or if this structure is not specified, the implementation behaves as if a valid shading rate attachment was specified with all texels specifying a single pixel per fragment.

Valid Usage

- VUID-VkFragmentShadingRateAttachmentInfoKHR-pFragmentShadingRateAttachment-04524
  If `pFragmentShadingRateAttachment` is not `NULL` and its `attachment` member is not `VK_ATTACHMENT_UNUSED`, its `layout` member must be equal to `VK_IMAGE_LAYOUT_GENERAL` or `VK_IMAGE_LAYOUT_FRAGMENT_SHADING_RATE_ATTACHMENT_OPTIMAL_KHR`

- VUID-VkFragmentShadingRateAttachmentInfoKHR-pFragmentShadingRateAttachment-04525
  If `pFragmentShadingRateAttachment` is not `NULL` and its `attachment` member is not `VK_ATTACHMENT_UNUSED`, `shadingRateAttachmentTexelSize.width` must be a power of two value

- VUID-VkFragmentShadingRateAttachmentInfoKHR-pFragmentShadingRateAttachment-04526
  If `pFragmentShadingRateAttachment` is not `NULL` and its `attachment` member is not `VK_ATTACHMENT_UNUSED`, `shadingRateAttachmentTexelSize.width` must be less than or equal to `maxFragmentShadingRateAttachmentTexelSize.width`

- VUID-VkFragmentShadingRateAttachmentInfoKHR-pFragmentShadingRateAttachment-04527
  If `pFragmentShadingRateAttachment` is not `NULL` and its `attachment` member is not `VK_ATTACHMENT_UNUSED`, `shadingRateAttachmentTexelSize.width` must be greater than or equal to `minFragmentShadingRateAttachmentTexelSize.width`

- VUID-VkFragmentShadingRateAttachmentInfoKHR-pFragmentShadingRateAttachment-04528
  If `pFragmentShadingRateAttachment` is not `NULL` and its `attachment` member is not `VK_ATTACHMENT_UNUSED`, `shadingRateAttachmentTexelSize.height` must be a power of two value

- VUID-VkFragmentShadingRateAttachmentInfoKHR-pFragmentShadingRateAttachment-04529
  If `pFragmentShadingRateAttachment` is not `NULL` and its `attachment` member is not `VK_ATTACHMENT_UNUSED`, `shadingRateAttachmentTexelSize.height` must be less than or equal to `maxFragmentShadingRateAttachmentTexelSize.height`

- VUID-VkFragmentShadingRateAttachmentInfoKHR-pFragmentShadingRateAttachment-04530
  If `pFragmentShadingRateAttachment` is not `NULL` and its `attachment` member is not `VK_ATTACHMENT_UNUSED`, `shadingRateAttachmentTexelSize.height` must be greater than or equal to `minFragmentShadingRateAttachmentTexelSize.height`

- VUID-VkFragmentShadingRateAttachmentInfoKHR-pFragmentShadingRateAttachment-04531
  If `pFragmentShadingRateAttachment` is not `NULL` and its `attachment` member is not `VK_ATTACHMENT_UNUSED`, the quotient of `shadingRateAttachmentTexelSize.width` and `shadingRateAttachmentTexelSize.height` must be less than or equal to `maxFragmentShadingRateAttachmentTexelSizeAspectRatio`

- VUID-VkFragmentShadingRateAttachmentInfoKHR-pFragmentShadingRateAttachment-04532
  If `pFragmentShadingRateAttachment` is not `NULL` and its `attachment` member is not `VK_ATTACHMENT_UNUSED`, the quotient of `shadingRateAttachmentTexelSize.height` and `shadingRateAttachmentTexelSize.width` must be less than or equal to `maxFragmentShadingRateAttachmentTexelSizeAspectRatio`

Valid Usage (Implicit)

- VUID-VkFragmentShadingRateAttachmentInfoKHR-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_FRAGMENT_SHADING_RATE_ATTACHMENT_INFO_KHR`

- VUID-VkFragmentShadingRateAttachmentInfoKHR-pFragmentShadingRateAttachment-parameter
  If `pFragmentShadingRateAttachment` is not `NULL`, `pFragmentShadingRateAttachment` must be a valid pointer to a valid VkAttachmentReference2 structure

If the `pNext` chain of VkSubpassDescription2 or VkRenderingInfo includes a `VkMultisampledRenderToSingleSampledInfoEXT` structure, then that structure describes how multisampled rendering is performed on single sampled attachments in that subpass.

The `VkMultisampledRenderToSingleSampledInfoEXT` structure is defined as:

    // Provided by VK_EXT_multisampled_render_to_single_sampled
    typedef struct VkMultisampledRenderToSingleSampledInfoEXT {
        VkStructureType          sType;
        const void*              pNext;
        VkBool32                 multisampledRenderToSingleSampledEnable;
        VkSampleCountFlagBits    rasterizationSamples;
    } VkMultisampledRenderToSingleSampledInfoEXT;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `multisampledRenderToSingleSampledEnable` controls whether multisampled rendering to single-sampled attachments is performed as described below.

- `rasterizationSamples` is a VkSampleCountFlagBits specifying the number of samples used in rasterization.

Valid Usage

- VUID-VkMultisampledRenderToSingleSampledInfoEXT-rasterizationSamples-06878
  The value of `rasterizationSamples` must not be `VK_SAMPLE_COUNT_1_BIT`

- VUID-VkMultisampledRenderToSingleSampledInfoEXT-pNext-06880
  If added to the `pNext` chain of VkRenderingInfo, each `imageView` member of any element of VkRenderingInfo::`pColorAttachments`, VkRenderingInfo::`pDepthAttachment`, or VkRenderingInfo::`pStencilAttachment` that is not VK_NULL_HANDLE must have a format that supports the sample count specified in `rasterizationSamples`

Valid Usage (Implicit)

- VUID-VkMultisampledRenderToSingleSampledInfoEXT-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_MULTISAMPLED_RENDER_TO_SINGLE_SAMPLED_INFO_EXT`

- VUID-VkMultisampledRenderToSingleSampledInfoEXT-rasterizationSamples-parameter
  `rasterizationSamples` must be a valid VkSampleCountFlagBits value

If the `pNext` chain of VkSubpassDescription2 or VkRenderingInfo includes a VkMultisampledRenderToSingleSampledInfoEXT structure whose `multisampledRenderToSingleSampledEnable` field is `VK_TRUE`, the graphics pipelines must have VkGraphicsPipelineCreateInfo::`rasterizationSamples` equal to VkMultisampledRenderToSingleSampledInfoEXT::`rasterizationSamples`, and the subpass attachments can have a sample count of `VK_SAMPLE_COUNT_1_BIT`. For attachments with a sample count of `VK_SAMPLE_COUNT_1_BIT`, multisampled rendering is performed to an intermediate multisampled image with VkMultisampledRenderToSingleSampledInfoEXT::`rasterizationSamples` samples, implicitly allocated by the implementation for the duration of the subpass. For such attachments:

- If `loadOp` equals to `VK_ATTACHMENT_LOAD_OP_LOAD`, samples of the implicit image are initialized by replicating the value from the corresponding pixel in the attachment.

- If `storeOp` or `stencilStoreOp` is equal to `VK_ATTACHMENT_STORE_OP_STORE`, the implicit image is implicitly resolved prior to storage in the attachment.

Memory constraints due to high primitive counts may result in an implicit split of the subpass. This is the equivalent of partial rasterization of geometry in a render pass that ends in `storeOp` and `stencilStoreOp` equal to `VK_ATTACHMENT_STORE_OP_STORE`, followed by another render pass with `loadOp` and `stencilLoadOp` equal to `VK_ATTACHMENT_LOAD_OP_LOAD` with appropriate barriers in between. When VkMultisampledRenderToSingleSampledInfoEXT is used, the implementation is allowed to resolve attachments with a sample count of `VK_SAMPLE_COUNT_1_BIT` and lose multisampled data on such splits. The implementation may similarly split the render pass at subpass boundaries even if they use the same value for VkMultisampledRenderToSingleSampledInfoEXT::`rasterizationSamples`.

The `VkAttachmentReference2` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkAttachmentReference2 {
        VkStructureType       sType;
        const void*           pNext;
        uint32_t              attachment;
        VkImageLayout         layout;
        VkImageAspectFlags    aspectMask;
    } VkAttachmentReference2;

or the equivalent

    // Provided by VK_KHR_create_renderpass2
    typedef VkAttachmentReference2 VkAttachmentReference2KHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `attachment` is either an integer value identifying an attachment at the corresponding index in VkRenderPassCreateInfo2::`pAttachments`, or `VK_ATTACHMENT_UNUSED` to signify that this attachment is not used.

- `layout` is a VkImageLayout value specifying the layout the attachment uses during the subpass.

- `aspectMask` is a mask of which aspect(s) can be accessed within the specified subpass as an input attachment.

Parameters defined by this structure with the same name as those in VkAttachmentReference have the identical effect to those parameters.

`aspectMask` is ignored when this structure is used to describe anything other than an input attachment reference.

If the `separateDepthStencilLayouts` feature is enabled, and `attachment` has a depth/stencil format, `layout` can be set to a layout that only specifies the layout of the depth aspect.

If `layout` only specifies the layout of the depth aspect of the attachment, the layout of the stencil aspect is specified by the `stencilLayout` member of a VkAttachmentReferenceStencilLayout structure included in the `pNext` chain. Otherwise, `layout` describes the layout for all relevant image aspects.

Valid Usage

- VUID-VkAttachmentReference2-layout-03077
  If `attachment` is not `VK_ATTACHMENT_UNUSED`, `layout` must not be `VK_IMAGE_LAYOUT_UNDEFINED`, `VK_IMAGE_LAYOUT_PREINITIALIZED`, or `VK_IMAGE_LAYOUT_PRESENT_SRC_KHR`

- VUID-VkAttachmentReference2-separateDepthStencilLayouts-03313
  If the `separateDepthStencilLayouts` feature is not enabled, and `attachment` is not `VK_ATTACHMENT_UNUSED`, `layout` must not be `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL`,

- VUID-VkAttachmentReference2-synchronization2-06910
  If the `synchronization2` feature is not enabled, `layout` must not be `VK_IMAGE_LAYOUT_ATTACHMENT_OPTIMAL_KHR` or `VK_IMAGE_LAYOUT_READ_ONLY_OPTIMAL_KHR`

- VUID-VkAttachmentReference2-attachmentFeedbackLoopLayout-07311
  If the `attachmentFeedbackLoopLayout` feature is not enabled, `layout` must not be `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT`

- VUID-VkAttachmentReference2-dynamicRenderingLocalRead-09546
  If the `dynamicRenderingLocalRead` feature is not enabled, `layout` must not be `VK_IMAGE_LAYOUT_RENDERING_LOCAL_READ`

Valid Usage (Implicit)

- VUID-VkAttachmentReference2-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_ATTACHMENT_REFERENCE_2`

- VUID-VkAttachmentReference2-pNext-pNext
  `pNext` must be `NULL` or a pointer to a valid instance of VkAttachmentReferenceStencilLayout

- VUID-VkAttachmentReference2-sType-unique
  The `sType` value of each struct in the `pNext` chain must be unique

- VUID-VkAttachmentReference2-layout-parameter
  `layout` must be a valid VkImageLayout value

The `VkAttachmentReferenceStencilLayout` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkAttachmentReferenceStencilLayout {
        VkStructureType    sType;
        void*              pNext;
        VkImageLayout      stencilLayout;
    } VkAttachmentReferenceStencilLayout;

or the equivalent

    // Provided by VK_KHR_separate_depth_stencil_layouts
    typedef VkAttachmentReferenceStencilLayout VkAttachmentReferenceStencilLayoutKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `stencilLayout` is a VkImageLayout value specifying the layout the stencil aspect of the attachment uses during the subpass.

Valid Usage

- VUID-VkAttachmentReferenceStencilLayout-stencilLayout-03318
  `stencilLayout` must not be `VK_IMAGE_LAYOUT_UNDEFINED`, `VK_IMAGE_LAYOUT_PREINITIALIZED`, `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_PRESENT_SRC_KHR`

Valid Usage (Implicit)

- VUID-VkAttachmentReferenceStencilLayout-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_ATTACHMENT_REFERENCE_STENCIL_LAYOUT`

- VUID-VkAttachmentReferenceStencilLayout-stencilLayout-parameter
  `stencilLayout` must be a valid VkImageLayout value

The `VkSubpassDependency2` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkSubpassDependency2 {
        VkStructureType         sType;
        const void*             pNext;
        uint32_t                srcSubpass;
        uint32_t                dstSubpass;
        VkPipelineStageFlags    srcStageMask;
        VkPipelineStageFlags    dstStageMask;
        VkAccessFlags           srcAccessMask;
        VkAccessFlags           dstAccessMask;
        VkDependencyFlags       dependencyFlags;
        int32_t                 viewOffset;
    } VkSubpassDependency2;

or the equivalent

    // Provided by VK_KHR_create_renderpass2
    typedef VkSubpassDependency2 VkSubpassDependency2KHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `srcSubpass` is the subpass index of the first subpass in the dependency, or `VK_SUBPASS_EXTERNAL`.

- `dstSubpass` is the subpass index of the second subpass in the dependency, or `VK_SUBPASS_EXTERNAL`.

- `srcStageMask` is a bitmask of VkPipelineStageFlagBits specifying the source stage mask.

- `dstStageMask` is a bitmask of VkPipelineStageFlagBits specifying the destination stage mask

- `srcAccessMask` is a bitmask of VkAccessFlagBits specifying a source access mask.

- `dstAccessMask` is a bitmask of VkAccessFlagBits specifying a destination access mask.

- `dependencyFlags` is a bitmask of VkDependencyFlagBits.

- `viewOffset` controls which views in the source subpass the views in the destination subpass depend on.

Parameters defined by this structure with the same name as those in VkSubpassDependency have the identical effect to those parameters.

`viewOffset` has the same effect for the described subpass dependency as VkRenderPassMultiviewCreateInfo::`pViewOffsets` has on each corresponding subpass dependency.

If a VkMemoryBarrier2 is included in the `pNext` chain, `srcStageMask`, `dstStageMask`, `srcAccessMask`, and `dstAccessMask` parameters are ignored. The synchronization and access scopes instead are defined by the parameters of VkMemoryBarrier2.

Valid Usage

- VUID-VkSubpassDependency2-srcStageMask-04090
  If the `geometryShader` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_GEOMETRY_SHADER_BIT`

- VUID-VkSubpassDependency2-srcStageMask-04091
  If the `tessellationShader` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_TESSELLATION_CONTROL_SHADER_BIT` or `VK_PIPELINE_STAGE_TESSELLATION_EVALUATION_SHADER_BIT`

- VUID-VkSubpassDependency2-srcStageMask-04092
  If the `conditionalRendering` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_CONDITIONAL_RENDERING_BIT_EXT`

- VUID-VkSubpassDependency2-srcStageMask-04093
  If the `fragmentDensityMap` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_FRAGMENT_DENSITY_PROCESS_BIT_EXT`

- VUID-VkSubpassDependency2-srcStageMask-04094
  If the `transformFeedback` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_TRANSFORM_FEEDBACK_BIT_EXT`

- VUID-VkSubpassDependency2-srcStageMask-04095
  If the `meshShader` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_MESH_SHADER_BIT_EXT`

- VUID-VkSubpassDependency2-srcStageMask-04096
  If the `taskShader` feature is not enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_TASK_SHADER_BIT_EXT`

- VUID-VkSubpassDependency2-srcStageMask-07318
  If neither of the `shadingRateImage` or the `attachmentFragmentShadingRate` features are enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_FRAGMENT_SHADING_RATE_ATTACHMENT_BIT_KHR`

- VUID-VkSubpassDependency2-srcStageMask-03937
  If the `synchronization2` feature is not enabled, `srcStageMask` must not be `0`

- VUID-VkSubpassDependency2-srcStageMask-07949
  If neither the VK_NV_ray_tracing extension or the `rayTracingPipeline` feature are enabled, `srcStageMask` must not contain `VK_PIPELINE_STAGE_RAY_TRACING_SHADER_BIT_KHR`

- VUID-VkSubpassDependency2-dstStageMask-04090
  If the `geometryShader` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_GEOMETRY_SHADER_BIT`

- VUID-VkSubpassDependency2-dstStageMask-04091
  If the `tessellationShader` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_TESSELLATION_CONTROL_SHADER_BIT` or `VK_PIPELINE_STAGE_TESSELLATION_EVALUATION_SHADER_BIT`

- VUID-VkSubpassDependency2-dstStageMask-04092
  If the `conditionalRendering` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_CONDITIONAL_RENDERING_BIT_EXT`

- VUID-VkSubpassDependency2-dstStageMask-04093
  If the `fragmentDensityMap` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_FRAGMENT_DENSITY_PROCESS_BIT_EXT`

- VUID-VkSubpassDependency2-dstStageMask-04094
  If the `transformFeedback` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_TRANSFORM_FEEDBACK_BIT_EXT`

- VUID-VkSubpassDependency2-dstStageMask-04095
  If the `meshShader` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_MESH_SHADER_BIT_EXT`

- VUID-VkSubpassDependency2-dstStageMask-04096
  If the `taskShader` feature is not enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_TASK_SHADER_BIT_EXT`

- VUID-VkSubpassDependency2-dstStageMask-07318
  If neither of the `shadingRateImage` or the `attachmentFragmentShadingRate` features are enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_FRAGMENT_SHADING_RATE_ATTACHMENT_BIT_KHR`

- VUID-VkSubpassDependency2-dstStageMask-03937
  If the `synchronization2` feature is not enabled, `dstStageMask` must not be `0`

- VUID-VkSubpassDependency2-dstStageMask-07949
  If neither the VK_NV_ray_tracing extension or the `rayTracingPipeline` feature are enabled, `dstStageMask` must not contain `VK_PIPELINE_STAGE_RAY_TRACING_SHADER_BIT_KHR`

- VUID-VkSubpassDependency2-srcSubpass-03084
  `srcSubpass` must be less than or equal to `dstSubpass`, unless one of them is `VK_SUBPASS_EXTERNAL`, to avoid cyclic dependencies and ensure a valid execution order

- VUID-VkSubpassDependency2-srcSubpass-03085
  `srcSubpass` and `dstSubpass` must not both be equal to `VK_SUBPASS_EXTERNAL`

- VUID-VkSubpassDependency2-srcSubpass-06810
  If `srcSubpass` is equal to `dstSubpass` and `srcStageMask` includes a framebuffer-space stage, `dstStageMask` must only contain framebuffer-space stages

- VUID-VkSubpassDependency2-srcAccessMask-03088
  Any access flag included in `srcAccessMask` must be supported by one of the pipeline stages in `srcStageMask`, as specified in the table of supported access types

- VUID-VkSubpassDependency2-dstAccessMask-03089
  Any access flag included in `dstAccessMask` must be supported by one of the pipeline stages in `dstStageMask`, as specified in the table of supported access types

- VUID-VkSubpassDependency2-dependencyFlags-03090
  If `dependencyFlags` includes `VK_DEPENDENCY_VIEW_LOCAL_BIT`, `srcSubpass` must not be equal to `VK_SUBPASS_EXTERNAL`

- VUID-VkSubpassDependency2-dependencyFlags-03091
  If `dependencyFlags` includes `VK_DEPENDENCY_VIEW_LOCAL_BIT`, `dstSubpass` must not be equal to `VK_SUBPASS_EXTERNAL`

- VUID-VkSubpassDependency2-srcSubpass-02245
  If `srcSubpass` equals `dstSubpass`, and `srcStageMask` and `dstStageMask` both include a framebuffer-space stage, then `dependencyFlags` must include `VK_DEPENDENCY_BY_REGION_BIT`

- VUID-VkSubpassDependency2-viewOffset-02530
  If `viewOffset` is not equal to `0`, `srcSubpass` must not be equal to `dstSubpass`

- VUID-VkSubpassDependency2-dependencyFlags-03092
  If `dependencyFlags` does not include `VK_DEPENDENCY_VIEW_LOCAL_BIT`, `viewOffset` must be `0`

Valid Usage (Implicit)

- VUID-VkSubpassDependency2-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_SUBPASS_DEPENDENCY_2`

- VUID-VkSubpassDependency2-pNext-pNext
  `pNext` must be `NULL` or a pointer to a valid instance of VkMemoryBarrier2

- VUID-VkSubpassDependency2-sType-unique
  The `sType` value of each struct in the `pNext` chain must be unique

- VUID-VkSubpassDependency2-srcStageMask-parameter
  `srcStageMask` must be a valid combination of VkPipelineStageFlagBits values

- VUID-VkSubpassDependency2-dstStageMask-parameter
  `dstStageMask` must be a valid combination of VkPipelineStageFlagBits values

- VUID-VkSubpassDependency2-srcAccessMask-parameter
  `srcAccessMask` must be a valid combination of VkAccessFlagBits values

- VUID-VkSubpassDependency2-dstAccessMask-parameter
  `dstAccessMask` must be a valid combination of VkAccessFlagBits values

- VUID-VkSubpassDependency2-dependencyFlags-parameter
  `dependencyFlags` must be a valid combination of VkDependencyFlagBits values

To destroy a render pass, call:

    // Provided by VK_VERSION_1_0
    void vkDestroyRenderPass(
        VkDevice                                    device,
        VkRenderPass                                renderPass,
        const VkAllocationCallbacks*                pAllocator);

- `device` is the logical device that destroys the render pass.

- `renderPass` is the handle of the render pass to destroy.

- `pAllocator` controls host memory allocation as described in the Memory Allocation chapter.

Valid Usage

- VUID-vkDestroyRenderPass-renderPass-00873
  All submitted commands that refer to `renderPass` must have completed execution

- VUID-vkDestroyRenderPass-renderPass-00874
  If `VkAllocationCallbacks` were provided when `renderPass` was created, a compatible set of callbacks must be provided here

- VUID-vkDestroyRenderPass-renderPass-00875
  If no `VkAllocationCallbacks` were provided when `renderPass` was created, `pAllocator` must be `NULL`

Valid Usage (Implicit)

- VUID-vkDestroyRenderPass-device-parameter
  `device` must be a valid VkDevice handle

- VUID-vkDestroyRenderPass-renderPass-parameter
  If `renderPass` is not VK_NULL_HANDLE, `renderPass` must be a valid VkRenderPass handle

- VUID-vkDestroyRenderPass-pAllocator-parameter
  If `pAllocator` is not `NULL`, `pAllocator` must be a valid pointer to a valid VkAllocationCallbacks structure

- VUID-vkDestroyRenderPass-renderPass-parent
  If `renderPass` is a valid handle, it must have been created, allocated, or retrieved from `device`

Host Synchronization

- Host access to `renderPass` must be externally synchronized

### 8.3. Render Pass Compatibility

Framebuffers and graphics pipelines are created based on a specific render pass object. They must only be used with that render pass object, or one compatible with it.

Two attachment references are compatible if they have matching format and sample count, or are both `VK_ATTACHMENT_UNUSED` or the pointer that would contain the reference is `NULL`.

Two arrays of attachment references are compatible if all corresponding pairs of attachments are compatible. If the arrays are of different lengths, attachment references not present in the smaller array are treated as `VK_ATTACHMENT_UNUSED`.

Two render passes are compatible if their corresponding color, input, resolve, and depth/stencil attachment references are compatible and if they are otherwise identical except for:

- Initial and final image layout in attachment descriptions

- Load and store operations in attachment descriptions

- Image layout in attachment references

As an additional special case, if two render passes have a single subpass, the resolve attachment reference and depth/stencil resolve mode compatibility requirements are ignored.

A framebuffer is compatible with a render pass if it was created using the same render pass or a compatible render pass.

### 8.4. Framebuffers

Render passes operate in conjunction with framebuffers. Framebuffers represent a collection of specific memory attachments that a render pass instance uses.

Framebuffers are represented by `VkFramebuffer` handles:

    // Provided by VK_VERSION_1_0
    VK_DEFINE_NON_DISPATCHABLE_HANDLE(VkFramebuffer)

To create a framebuffer, call:

    // Provided by VK_VERSION_1_0
    VkResult vkCreateFramebuffer(
        VkDevice                                    device,
        const VkFramebufferCreateInfo*              pCreateInfo,
        const VkAllocationCallbacks*                pAllocator,
        VkFramebuffer*                              pFramebuffer);

- `device` is the logical device that creates the framebuffer.

- `pCreateInfo` is a pointer to a VkFramebufferCreateInfo structure describing additional information about framebuffer creation.

- `pAllocator` controls host memory allocation as described in the Memory Allocation chapter.

- `pFramebuffer` is a pointer to a VkFramebuffer handle in which the resulting framebuffer object is returned.

Valid Usage

- VUID-vkCreateFramebuffer-device-10002
  `device` must support at least one queue family with the `VK_QUEUE_GRAPHICS_BIT` capability

- VUID-vkCreateFramebuffer-pCreateInfo-02777
  If `pCreateInfo->flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, and `attachmentCount` is not `0`, each element of `pCreateInfo->pAttachments` must have been created on `device`

Valid Usage (Implicit)

- VUID-vkCreateFramebuffer-device-parameter
  `device` must be a valid VkDevice handle

- VUID-vkCreateFramebuffer-pCreateInfo-parameter
  `pCreateInfo` must be a valid pointer to a valid VkFramebufferCreateInfo structure

- VUID-vkCreateFramebuffer-pAllocator-parameter
  If `pAllocator` is not `NULL`, `pAllocator` must be a valid pointer to a valid VkAllocationCallbacks structure

- VUID-vkCreateFramebuffer-pFramebuffer-parameter
  `pFramebuffer` must be a valid pointer to a VkFramebuffer handle

Return Codes

Success

  - `VK_SUCCESS`

Failure

  - `VK_ERROR_OUT_OF_HOST_MEMORY`

  - `VK_ERROR_OUT_OF_DEVICE_MEMORY`

The `VkFramebufferCreateInfo` structure is defined as:

    // Provided by VK_VERSION_1_0
    typedef struct VkFramebufferCreateInfo {
        VkStructureType             sType;
        const void*                 pNext;
        VkFramebufferCreateFlags    flags;
        VkRenderPass                renderPass;
        uint32_t                    attachmentCount;
        const VkImageView*          pAttachments;
        uint32_t                    width;
        uint32_t                    height;
        uint32_t                    layers;
    } VkFramebufferCreateInfo;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `flags` is a bitmask of VkFramebufferCreateFlagBits

- `renderPass` is a render pass defining what render passes the framebuffer will be compatible with. See Render Pass Compatibility for details.

- `attachmentCount` is the number of attachments.

- `pAttachments` is a pointer to an array of VkImageView handles, each of which will be used as the corresponding attachment in a render pass instance. If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, this parameter is ignored.

- `width`, `height` and `layers` define the dimensions of the framebuffer. If the render pass uses multiview, then `layers` must be one and each attachment requires a number of layers that is greater than the maximum bit index set in the view mask in the subpasses in which it is used.

It is legal for a subpass to use no color or depth/stencil attachments, either because it has no attachment references or because all of them are `VK_ATTACHMENT_UNUSED`. This kind of subpass can use shader side effects such as image stores and atomics to produce an output. In this case, the subpass continues to use the `width`, `height`, and `layers` of the framebuffer to define the dimensions of the rendering area, and the `rasterizationSamples` from each pipeline’s VkPipelineMultisampleStateCreateInfo to define the number of samples used in rasterization; however, if VkPhysicalDeviceFeatures::`variableMultisampleRate` is `VK_FALSE`, then all pipelines to be bound with the subpass must have the same value for VkPipelineMultisampleStateCreateInfo::`rasterizationSamples`. In all such cases, `rasterizationSamples` must be a valid VkSampleCountFlagBits value that is set in VkPhysicalDeviceLimits::`framebufferNoAttachmentsSampleCounts`.

Valid Usage

- VUID-VkFramebufferCreateInfo-attachmentCount-00876
  `attachmentCount` must be equal to the attachment count specified in `renderPass`

- VUID-VkFramebufferCreateInfo-flags-02778
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT` and `attachmentCount` is not `0`, `pAttachments` must be a valid pointer to an array of `attachmentCount` valid VkImageView handles

- VUID-VkFramebufferCreateInfo-pAttachments-00877
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` that is used as a color attachment or resolve attachment by `renderPass` must have been created with a `usage` value including `VK_IMAGE_USAGE_COLOR_ATTACHMENT_BIT`

- VUID-VkFramebufferCreateInfo-pAttachments-02633
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` that is used as a depth/stencil attachment by `renderPass` must have been created with a `usage` value including `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkFramebufferCreateInfo-pAttachments-02634
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` that is used as a depth/stencil resolve attachment by `renderPass` must have been created with a `usage` value including `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkFramebufferCreateInfo-pAttachments-00879
  If `renderpass` is not VK_NULL_HANDLE, `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` that is used as an input attachment by `renderPass` must have been created with a `usage` value including `VK_IMAGE_USAGE_INPUT_ATTACHMENT_BIT`

- VUID-VkFramebufferCreateInfo-pAttachments-02552
  Each element of `pAttachments` that is used as a fragment density map attachment by `renderPass` must not have been created with a `flags` value including `VK_IMAGE_CREATE_SUBSAMPLED_BIT_EXT`

- VUID-VkFramebufferCreateInfo-renderPass-02553
  If `renderPass` has a fragment density map attachment and the `fragmentDensityMapNonSubsampledImages` feature is not enabled, each element of `pAttachments` must have been created with a `flags` value including `VK_IMAGE_CREATE_SUBSAMPLED_BIT_EXT` unless that element is the fragment density map attachment

- VUID-VkFramebufferCreateInfo-renderPass-06502
  If `renderPass` was created with fragment density map offsets other than (0,0), each element of `pAttachments` must have been created with a `flags` value including `VK_IMAGE_CREATE_FRAGMENT_DENSITY_MAP_OFFSET_BIT_QCOM`

- VUID-VkFramebufferCreateInfo-pAttachments-00880
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` must have been created with a VkFormat value that matches the VkFormat specified by the corresponding `VkAttachmentDescription` in `renderPass`

- VUID-VkFramebufferCreateInfo-pAttachments-00881
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` must have been created with a `samples` value that matches the `samples` value specified by the corresponding `VkAttachmentDescription` in `renderPass`

- VUID-VkFramebufferCreateInfo-flags-04533
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` that is used as an input, color, resolve, or depth/stencil attachment by `renderPass` must have been created with a VkImageCreateInfo::`extent.width` greater than or equal to `width`

- VUID-VkFramebufferCreateInfo-flags-04534
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` that is used as an input, color, resolve, or depth/stencil attachment by `renderPass` must have been created with a VkImageCreateInfo::`extent.height` greater than or equal to `height`

- VUID-VkFramebufferCreateInfo-flags-04535
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` that is used as an input, color, resolve, or depth/stencil attachment by `renderPass` must have been created with a VkImageViewCreateInfo::`subresourceRange.layerCount` greater than or equal to `layers`

- VUID-VkFramebufferCreateInfo-renderPass-04536
  If `renderPass` was specified with non-zero view masks, each element of `pAttachments` that is used as an input, color, resolve, or depth/stencil attachment by `renderPass` must have a `layerCount` greater than the index of the most significant bit set in any of those view masks

- VUID-VkFramebufferCreateInfo-renderPass-02746
  Each element of `pAttachments` that is referenced by `fragmentDensityMapAttachment` must have a `layerCount` equal to `1` or if `renderPass` was specified with non-zero view masks, greater than the index of the most significant bit set in any of those view masks

- VUID-VkFramebufferCreateInfo-pAttachments-02555
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, an element of `pAttachments` that is referenced by `fragmentDensityMapAttachment` must have a width at least as large as ⌈ma x F r a g m e n t De n s i t y T e x e lS i z e w i d t h​w i d t h​⌉

- VUID-VkFramebufferCreateInfo-pAttachments-02556
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, an element of `pAttachments` that is referenced by `fragmentDensityMapAttachment` must have a height at least as large as ⌈ma x F r a g m e n t De n s i t y T e x e lS i z e h e i g h t​h e i g h t​⌉

- VUID-VkFramebufferCreateInfo-flags-04537
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, and `renderPass` was specified with non-zero view masks, each element of `pAttachments` that is used as a fragment shading rate attachment by `renderPass` must have a `layerCount` that is either `1`, or greater than the index of the most significant bit set in any of those view masks

- VUID-VkFramebufferCreateInfo-flags-04538
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, and `renderPass` was not specified with non-zero view masks, each element of `pAttachments` that is used as a fragment shading rate attachment by `renderPass` must have a `layerCount` that is either `1`, or greater than `layers`

- VUID-VkFramebufferCreateInfo-flags-04539
  If the `maintenance7` feature is not enabled or the `robustFragmentShadingRateAttachmentAccess` limit is `VK_FALSE` or the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure was created with VkImageSubresourceRange::`baseMipLevel` greater than 0, `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, an element of `pAttachments` that is used as a fragment shading rate attachment must have a width at least as large as ⌈`width` / `texelWidth`⌉, where `texelWidth` is the largest value of `shadingRateAttachmentTexelSize.width` in a VkFragmentShadingRateAttachmentInfoKHR which references that attachment

- VUID-VkFramebufferCreateInfo-flags-04540
  If the `maintenance7` feature is not enabled or the `robustFragmentShadingRateAttachmentAccess` limit is `VK_FALSE` or the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure was created with VkImageSubresourceRange::`baseMipLevel` greater than 0, `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, an element of `pAttachments` that is used as a fragment shading rate attachment must have a height at least as large as ⌈`height` / `texelHeight`⌉, where `texelHeight` is the largest value of `shadingRateAttachmentTexelSize.height` in a VkFragmentShadingRateAttachmentInfoKHR which references that attachment

- VUID-VkFramebufferCreateInfo-pAttachments-00883
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` must only specify a single mip level

- VUID-VkFramebufferCreateInfo-pAttachments-00884
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` must have been created with the identity swizzle

- VUID-VkFramebufferCreateInfo-width-00885
  `width` must be greater than `0`

- VUID-VkFramebufferCreateInfo-width-00886
  `width` must be less than or equal to `maxFramebufferWidth`

- VUID-VkFramebufferCreateInfo-height-00887
  `height` must be greater than `0`

- VUID-VkFramebufferCreateInfo-height-00888
  `height` must be less than or equal to `maxFramebufferHeight`

- VUID-VkFramebufferCreateInfo-layers-00889
  `layers` must be greater than `0`

- VUID-VkFramebufferCreateInfo-layers-00890
  `layers` must be less than or equal to `maxFramebufferLayers`

- VUID-VkFramebufferCreateInfo-renderPass-02531
  If `renderPass` was specified with non-zero view masks, `layers` must be `1`

- VUID-VkFramebufferCreateInfo-pAttachments-00891
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` that is a 2D or 2D array image view taken from a 3D image must not be a depth/stencil format

- VUID-VkFramebufferCreateInfo-flags-03189
  If the `imagelessFramebuffer` feature is not enabled, `flags` must not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`

- VUID-VkFramebufferCreateInfo-flags-03190
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `pNext` chain must include a VkFramebufferAttachmentsCreateInfo structure

- VUID-VkFramebufferCreateInfo-flags-03191
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `attachmentImageInfoCount` member of a VkFramebufferAttachmentsCreateInfo structure in the `pNext` chain must be equal to either zero or `attachmentCount`

- VUID-VkFramebufferCreateInfo-flags-04541
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `width` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure in the `pNext` chain that is used as an input, color, resolve or depth/stencil attachment in `renderPass` must be greater than or equal to `width`

- VUID-VkFramebufferCreateInfo-flags-04542
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `height` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure in the `pNext` chain that is used as an input, color, resolve or depth/stencil attachment in `renderPass` must be greater than or equal to `height`

- VUID-VkFramebufferCreateInfo-flags-03196
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `width` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure in the `pNext` chain that is referenced by VkRenderPassFragmentDensityMapCreateInfoEXT::`fragmentDensityMapAttachment` in `renderPass` must be greater than or equal to ⌈ma x F r a g m e n t De n s i t y T e x e lS i z e w i d t h​w i d t h​⌉

- VUID-VkFramebufferCreateInfo-flags-03197
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `height` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure included in the `pNext` chain that is referenced by VkRenderPassFragmentDensityMapCreateInfoEXT::`fragmentDensityMapAttachment` in `renderPass` must be greater than or equal to ⌈ma x F r a g m e n t De n s i t y T e x e lS i z e h e i g h t​h e i g h t​⌉

- VUID-VkFramebufferCreateInfo-flags-04543
  If the `maintenance7` feature is not enabled or the `robustFragmentShadingRateAttachmentAccess` limit is `VK_FALSE` or the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure was created with VkImageSubresourceRange::`baseMipLevel` greater than 0, and `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `width` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure in the `pNext` chain that is used as a fragment shading rate attachment must be greater than or equal to ⌈`width` / `texelWidth`⌉, where `texelWidth` is the largest value of `shadingRateAttachmentTexelSize.width` in a VkFragmentShadingRateAttachmentInfoKHR which references that attachment

- VUID-VkFramebufferCreateInfo-flags-04544
  If the `maintenance7` feature is not enabled or the `robustFragmentShadingRateAttachmentAccess` limit is `VK_FALSE` or the `imageView` member of a VkRenderingFragmentShadingRateAttachmentInfoKHR structure was created with VkImageSubresourceRange::`baseMipLevel` greater than 0, and `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `height` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure in the `pNext` chain that is used as a fragment shading rate attachment must be greater than or equal to ⌈`height` / `texelHeight`⌉, where `texelHeight` is the largest value of `shadingRateAttachmentTexelSize.height` in a VkFragmentShadingRateAttachmentInfoKHR which references that attachment

- VUID-VkFramebufferCreateInfo-flags-04545
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `layerCount` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure in the `pNext` chain that is used as a fragment shading rate attachment must be either `1`, or greater than or equal to `layers`

- VUID-VkFramebufferCreateInfo-flags-04587
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT` and `renderPass` was specified with non-zero view masks, the `layerCount` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure in the `pNext` chain that is used as a fragment shading rate attachment must be either `1`, or greater than the index of the most significant bit set in any of those view masks

- VUID-VkFramebufferCreateInfo-renderPass-03198
  If multiview is enabled for `renderPass` and `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `layerCount` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure included in the `pNext` chain used as an input, color, resolve, or depth/stencil attachment in `renderPass` must be greater than the maximum bit index set in the view mask in the subpasses in which it is used in `renderPass`

- VUID-VkFramebufferCreateInfo-renderPass-04546
  If multiview is not enabled for `renderPass` and `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `layerCount` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure included in the `pNext` chain used as an input, color, resolve, or depth/stencil attachment in `renderPass` must be greater than or equal to `layers`

- VUID-VkFramebufferCreateInfo-flags-03201
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `usage` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure included in the `pNext` chain that refers to an attachment used as a color attachment or resolve attachment by `renderPass` must include `VK_IMAGE_USAGE_COLOR_ATTACHMENT_BIT`

- VUID-VkFramebufferCreateInfo-flags-03202
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `usage` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure included in the `pNext` chain that refers to an attachment used as a depth/stencil attachment by `renderPass` must include `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkFramebufferCreateInfo-flags-03203
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `usage` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure included in the `pNext` chain that refers to an attachment used as a depth/stencil resolve attachment by `renderPass` must include `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-VkFramebufferCreateInfo-flags-03204
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `usage` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure included in the `pNext` chain that refers to an attachment used as an input attachment by `renderPass` must include `VK_IMAGE_USAGE_INPUT_ATTACHMENT_BIT`

- VUID-VkFramebufferCreateInfo-flags-03205
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, at least one element of the `pViewFormats` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure included in the `pNext` chain must be equal to the corresponding value of VkAttachmentDescription::`format` used to create `renderPass`

- VUID-VkFramebufferCreateInfo-flags-04113
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` must have been created with VkImageViewCreateInfo::`viewType` not equal to `VK_IMAGE_VIEW_TYPE_3D`

- VUID-VkFramebufferCreateInfo-flags-04548
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of `pAttachments` that is used as a fragment shading rate attachment by `renderPass` must have been created with a `usage` value including `VK_IMAGE_USAGE_FRAGMENT_SHADING_RATE_ATTACHMENT_BIT_KHR`

- VUID-VkFramebufferCreateInfo-flags-04549
  If `flags` includes `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `usage` member of any element of the `pAttachmentImageInfos` member of a VkFramebufferAttachmentsCreateInfo structure included in the `pNext` chain that refers to an attachment used as a fragment shading rate attachment by `renderPass` must include `VK_IMAGE_USAGE_FRAGMENT_SHADING_RATE_ATTACHMENT_BIT_KHR`

- VUID-VkFramebufferCreateInfo-samples-06881
  If multisampled-render-to-single-sampled is enabled for any subpass, all color, depth/stencil and input attachments used in that subpass which have `VkAttachmentDescription`::`samples` or `VkAttachmentDescription2`::`samples` equal to `VK_SAMPLE_COUNT_1_BIT` must have been created with `VK_IMAGE_CREATE_MULTISAMPLED_RENDER_TO_SINGLE_SAMPLED_BIT_EXT` in their VkImageCreateInfo::`flags`

- VUID-VkFramebufferCreateInfo-samples-07009
  If multisampled-render-to-single-sampled is enabled for any subpass, all color, depth/stencil and input attachments used in that subpass which have `VkAttachmentDescription`::`samples` or `VkAttachmentDescription2`::`samples` equal to `VK_SAMPLE_COUNT_1_BIT` must have a format that supports the sample count specified in VkMultisampledRenderToSingleSampledInfoEXT::`rasterizationSamples`

- VUID-VkFramebufferCreateInfo-nullColorAttachmentWithExternalFormatResolve-09349
  If the `nullColorAttachmentWithExternalFormatResolve` is `VK_FALSE`, and `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the format of the color attachment for each subpass in `renderPass` that includes an external format image as a resolve attachment must have a format equal to the value of VkAndroidHardwareBufferFormatResolvePropertiesANDROID::`colorAttachmentFormat` as returned by a call to vkGetAndroidHardwareBufferPropertiesANDROID for the Android hardware buffer that was used to create the image view use as its resolve attachment

- VUID-VkFramebufferCreateInfo-pAttachments-09350
  If `flags` does not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, then if an element of `pAttachments` has a format of `VK_FORMAT_UNDEFINED`, it must have been created with a VkExternalFormatANDROID::`externalFormat` value identical to that provided in the VkExternalFormatANDROID::`externalFormat` specified by the corresponding VkAttachmentDescription2 in `renderPass`

Valid Usage (Implicit)

- VUID-VkFramebufferCreateInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_FRAMEBUFFER_CREATE_INFO`

- VUID-VkFramebufferCreateInfo-pNext-pNext
  `pNext` must be `NULL` or a pointer to a valid instance of VkFramebufferAttachmentsCreateInfo

- VUID-VkFramebufferCreateInfo-sType-unique
  The `sType` value of each struct in the `pNext` chain must be unique

- VUID-VkFramebufferCreateInfo-flags-parameter
  `flags` must be a valid combination of VkFramebufferCreateFlagBits values

- VUID-VkFramebufferCreateInfo-renderPass-parameter
  `renderPass` must be a valid VkRenderPass handle

- VUID-VkFramebufferCreateInfo-commonparent
  Both of `renderPass`, and the elements of `pAttachments` that are valid handles of non-ignored parameters must have been created, allocated, or retrieved from the same VkDevice

The `VkFramebufferAttachmentsCreateInfo` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkFramebufferAttachmentsCreateInfo {
        VkStructureType                            sType;
        const void*                                pNext;
        uint32_t                                   attachmentImageInfoCount;
        const VkFramebufferAttachmentImageInfo*    pAttachmentImageInfos;
    } VkFramebufferAttachmentsCreateInfo;

or the equivalent

    // Provided by VK_KHR_imageless_framebuffer
    typedef VkFramebufferAttachmentsCreateInfo VkFramebufferAttachmentsCreateInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `attachmentImageInfoCount` is the number of attachments being described.

- `pAttachmentImageInfos` is a pointer to an array of VkFramebufferAttachmentImageInfo structures, each structure describing a number of parameters of the corresponding attachment in a render pass instance.

Valid Usage (Implicit)

- VUID-VkFramebufferAttachmentsCreateInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_FRAMEBUFFER_ATTACHMENTS_CREATE_INFO`

- VUID-VkFramebufferAttachmentsCreateInfo-pAttachmentImageInfos-parameter
  If `attachmentImageInfoCount` is not `0`, `pAttachmentImageInfos` must be a valid pointer to an array of `attachmentImageInfoCount` valid VkFramebufferAttachmentImageInfo structures

The `VkFramebufferAttachmentImageInfo` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkFramebufferAttachmentImageInfo {
        VkStructureType       sType;
        const void*           pNext;
        VkImageCreateFlags    flags;
        VkImageUsageFlags     usage;
        uint32_t              width;
        uint32_t              height;
        uint32_t              layerCount;
        uint32_t              viewFormatCount;
        const VkFormat*       pViewFormats;
    } VkFramebufferAttachmentImageInfo;

or the equivalent

    // Provided by VK_KHR_imageless_framebuffer
    typedef VkFramebufferAttachmentImageInfo VkFramebufferAttachmentImageInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `flags` is a bitmask of VkImageCreateFlagBits, matching the value of VkImageCreateInfo::`flags` used to create an image that will be used with this framebuffer.

- `usage` is a bitmask of VkImageUsageFlagBits, matching the value of VkImageCreateInfo::`usage` used to create an image used with this framebuffer.

- `width` is the width of the image view used for rendering.

- `height` is the height of the image view used for rendering.

- `layerCount` is the number of array layers of the image view used for rendering.

- `viewFormatCount` is the number of entries in the `pViewFormats` array, matching the value of VkImageFormatListCreateInfo::`viewFormatCount` used to create an image used with this framebuffer.

- `pViewFormats` is a pointer to an array of VkFormat values specifying all of the formats which can be used when creating views of the image, matching the value of VkImageFormatListCreateInfo::`pViewFormats` used to create an image used with this framebuffer.

Images that can be used with the framebuffer when beginning a render pass, as specified by VkRenderPassAttachmentBeginInfo, must be created with parameters that are identical to those specified here.

Valid Usage

- VUID-VkFramebufferAttachmentImageInfo-viewFormatCount-09536
  If `viewFormatCount` is not 0, and the render pass is not being used with an external format resolve attachment, each element of `pViewFormats` must not be `VK_FORMAT_UNDEFINED`

Valid Usage (Implicit)

- VUID-VkFramebufferAttachmentImageInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_FRAMEBUFFER_ATTACHMENT_IMAGE_INFO`

- VUID-VkFramebufferAttachmentImageInfo-pNext-pNext
  `pNext` must be `NULL`

- VUID-VkFramebufferAttachmentImageInfo-flags-parameter
  `flags` must be a valid combination of VkImageCreateFlagBits values

- VUID-VkFramebufferAttachmentImageInfo-usage-parameter
  `usage` must be a valid combination of VkImageUsageFlagBits values

- VUID-VkFramebufferAttachmentImageInfo-usage-requiredbitmask
  `usage` must not be `0`

- VUID-VkFramebufferAttachmentImageInfo-pViewFormats-parameter
  If `viewFormatCount` is not `0`, `pViewFormats` must be a valid pointer to an array of `viewFormatCount` valid VkFormat values

Bits which can be set in VkFramebufferCreateInfo::`flags`, specifying options for framebuffers, are:

    // Provided by VK_VERSION_1_0
    typedef enum VkFramebufferCreateFlagBits {
      // Provided by VK_VERSION_1_2
        VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT = 0x00000001,
      // Provided by VK_KHR_imageless_framebuffer
        VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT_KHR = VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT,
    } VkFramebufferCreateFlagBits;

- `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT` specifies that image views are not specified, and only attachment compatibility information will be provided via a VkFramebufferAttachmentImageInfo structure.

    // Provided by VK_VERSION_1_0
    typedef VkFlags VkFramebufferCreateFlags;

`VkFramebufferCreateFlags` is a bitmask type for setting a mask of zero or more VkFramebufferCreateFlagBits.

To destroy a framebuffer, call:

    // Provided by VK_VERSION_1_0
    void vkDestroyFramebuffer(
        VkDevice                                    device,
        VkFramebuffer                               framebuffer,
        const VkAllocationCallbacks*                pAllocator);

- `device` is the logical device that destroys the framebuffer.

- `framebuffer` is the handle of the framebuffer to destroy.

- `pAllocator` controls host memory allocation as described in the Memory Allocation chapter.

Valid Usage

- VUID-vkDestroyFramebuffer-framebuffer-00892
  All submitted commands that refer to `framebuffer` must have completed execution

- VUID-vkDestroyFramebuffer-framebuffer-00893
  If `VkAllocationCallbacks` were provided when `framebuffer` was created, a compatible set of callbacks must be provided here

- VUID-vkDestroyFramebuffer-framebuffer-00894
  If no `VkAllocationCallbacks` were provided when `framebuffer` was created, `pAllocator` must be `NULL`

Valid Usage (Implicit)

- VUID-vkDestroyFramebuffer-device-parameter
  `device` must be a valid VkDevice handle

- VUID-vkDestroyFramebuffer-framebuffer-parameter
  If `framebuffer` is not VK_NULL_HANDLE, `framebuffer` must be a valid VkFramebuffer handle

- VUID-vkDestroyFramebuffer-pAllocator-parameter
  If `pAllocator` is not `NULL`, `pAllocator` must be a valid pointer to a valid VkAllocationCallbacks structure

- VUID-vkDestroyFramebuffer-framebuffer-parent
  If `framebuffer` is a valid handle, it must have been created, allocated, or retrieved from `device`

Host Synchronization

- Host access to `framebuffer` must be externally synchronized

### 8.5. Render Pass Load Operations

Render pass load operations define the initial values of an attachment during a render pass instance.

Load operations for attachments with a depth/stencil format execute in the `VK_PIPELINE_STAGE_EARLY_FRAGMENT_TESTS_BIT` pipeline stage. Load operations for attachments with a color format execute in the `VK_PIPELINE_STAGE_COLOR_ATTACHMENT_OUTPUT_BIT` pipeline stage. The load operation for each sample in an attachment happens-before any recorded command which accesses the sample in that render pass instance via that attachment or an alias.

Note | Because load operations always happen first, external synchronization with attachment access only needs to synchronize the load operations with previous commands; not the operations within the render pass instance. This does not apply when using `VK_ATTACHMENT_LOAD_OP_NONE`.

Load operations only update values within the defined render area for the render pass instance. However, any writes performed by a load operation (as defined by its access masks) to a given attachment may read and write back any memory locations within the image subresource bound for that attachment. For depth/stencil images, if the maintenance7 feature is not enabled or `separateDepthStencilAttachmentAccess` is `VK_FALSE`, writes to one aspect may also result in read-modify-write operations for the other aspect. If the subresource is in the `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT` layout, implementations must not access pixels outside of the render area.

Note | As entire subresources could be accessed by load operations, applications cannot safely access values outside of the render area during a render pass instance when a load operation that modifies values is used.

Load operations that can be used for a render pass are:

    // Provided by VK_VERSION_1_0
    typedef enum VkAttachmentLoadOp {
        VK_ATTACHMENT_LOAD_OP_LOAD = 0,
        VK_ATTACHMENT_LOAD_OP_CLEAR = 1,
        VK_ATTACHMENT_LOAD_OP_DONT_CARE = 2,
      // Provided by VK_VERSION_1_4
        VK_ATTACHMENT_LOAD_OP_NONE = 1000400000,
      // Provided by VK_EXT_load_store_op_none
        VK_ATTACHMENT_LOAD_OP_NONE_EXT = VK_ATTACHMENT_LOAD_OP_NONE,
      // Provided by VK_KHR_load_store_op_none
        VK_ATTACHMENT_LOAD_OP_NONE_KHR = VK_ATTACHMENT_LOAD_OP_NONE,
    } VkAttachmentLoadOp;

- `VK_ATTACHMENT_LOAD_OP_LOAD` specifies that the previous contents of the image within the render area will be preserved as the initial values. For attachments with a depth/stencil format, this uses the access type `VK_ACCESS_DEPTH_STENCIL_ATTACHMENT_READ_BIT`. For attachments with a color format, this uses the access type `VK_ACCESS_COLOR_ATTACHMENT_READ_BIT`.

- `VK_ATTACHMENT_LOAD_OP_CLEAR` specifies that the contents within the render area will be cleared to a uniform value, which is specified when a render pass instance is begun. For attachments with a depth/stencil format, this uses the access type `VK_ACCESS_DEPTH_STENCIL_ATTACHMENT_WRITE_BIT`. For attachments with a color format, this uses the access type `VK_ACCESS_COLOR_ATTACHMENT_WRITE_BIT`.

- `VK_ATTACHMENT_LOAD_OP_DONT_CARE` specifies that the previous contents within the area need not be preserved; the contents of the attachment will be undefined inside the render area. For attachments with a depth/stencil format, this uses the access type `VK_ACCESS_DEPTH_STENCIL_ATTACHMENT_WRITE_BIT`. For attachments with a color format, this uses the access type `VK_ACCESS_COLOR_ATTACHMENT_WRITE_BIT`.

- `VK_ATTACHMENT_LOAD_OP_NONE` specifies that the previous contents of the image will be undefined inside the render pass. No access type is used as the image is not accessed.

During a render pass instance, input and color attachments with color formats that have a component size of 8, 16, or 32 bits must be represented in the attachment’s format throughout the instance. Attachments with other floating- or fixed-point color formats, or with depth components may be represented in a format with a precision higher than the attachment format, but must be represented with the same range. When such a component is loaded via the `loadOp`, it will be converted into an implementation-dependent format used by the render pass. Such components must be converted from the render pass format, to the format of the attachment, before they are resolved or stored at the end of a render pass instance via `storeOp`. Conversions occur as described in Numeric Representation and Computation and Fixed-Point Data Conversions.

### 8.6. Render Pass Store Operations

Render pass store operations define how values written to an attachment during a render pass instance are stored to memory.

Store operations for attachments with a depth/stencil format execute in the `VK_PIPELINE_STAGE_LATE_FRAGMENT_TESTS_BIT` pipeline stage. Store operations for attachments with a color format execute in the `VK_PIPELINE_STAGE_COLOR_ATTACHMENT_OUTPUT_BIT` pipeline stage. The store operation for each sample in an attachment happens-after any recorded command which accesses the sample via that attachment or an alias.

Note | Because store operations always happen after other accesses in a render pass instance, external synchronization with attachment access in an earlier render pass only needs to synchronize with the store operations; not the operations within the render pass instance. This does not apply when using `VK_ATTACHMENT_STORE_OP_NONE`.

Store operations only update values within the defined render area for the render pass instance. However, any writes performed by a store operation (as defined by its access masks) to a given attachment may read and write back any memory locations within the image subresource bound for that attachment. For depth/stencil images, if `separateDepthStencilAttachmentAccess` is `VK_FALSE`, writes to one aspect may also result in read-modify-write operations for the other aspect. If the subresource is in the `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT` layout, implementations must not access pixels outside of the render area.

Note | As entire subresources could be accessed by store operations, applications cannot safely access values outside of the render area via aliased resources during a render pass instance when a store operation that modifies values is used.

Possible values of VkAttachmentDescription::`storeOp` and `stencilStoreOp`, specifying how the contents of the attachment are treated, are:

    // Provided by VK_VERSION_1_0
    typedef enum VkAttachmentStoreOp {
        VK_ATTACHMENT_STORE_OP_STORE = 0,
        VK_ATTACHMENT_STORE_OP_DONT_CARE = 1,
      // Provided by VK_VERSION_1_3
        VK_ATTACHMENT_STORE_OP_NONE = 1000301000,
      // Provided by VK_KHR_dynamic_rendering, VK_KHR_load_store_op_none
        VK_ATTACHMENT_STORE_OP_NONE_KHR = VK_ATTACHMENT_STORE_OP_NONE,
      // Provided by VK_QCOM_render_pass_store_ops
        VK_ATTACHMENT_STORE_OP_NONE_QCOM = VK_ATTACHMENT_STORE_OP_NONE,
      // Provided by VK_EXT_load_store_op_none
        VK_ATTACHMENT_STORE_OP_NONE_EXT = VK_ATTACHMENT_STORE_OP_NONE,
    } VkAttachmentStoreOp;

- `VK_ATTACHMENT_STORE_OP_STORE` specifies the contents generated during the render pass and within the render area are written to memory. For attachments with a depth/stencil format, this uses the access type `VK_ACCESS_DEPTH_STENCIL_ATTACHMENT_WRITE_BIT`. For attachments with a color format, this uses the access type `VK_ACCESS_COLOR_ATTACHMENT_WRITE_BIT`.

- `VK_ATTACHMENT_STORE_OP_DONT_CARE` specifies the contents within the render area are not needed after rendering, and may be discarded; the contents of the attachment will be undefined inside the render area. For attachments with a depth/stencil format, this uses the access type `VK_ACCESS_DEPTH_STENCIL_ATTACHMENT_WRITE_BIT`. For attachments with a color format, this uses the access type `VK_ACCESS_COLOR_ATTACHMENT_WRITE_BIT`.

- `VK_ATTACHMENT_STORE_OP_NONE` specifies the contents within the render area are not accessed by the store operation as long as no values are written to the attachment during the render pass. If values are written during the render pass, this behaves identically to `VK_ATTACHMENT_STORE_OP_DONT_CARE` and with matching access semantics.

Note | `VK_ATTACHMENT_STORE_OP_DONT_CARE` can cause contents generated during previous render passes to be discarded before reaching memory, even if no write to the attachment occurs during the current render pass.

### 8.7. Render Pass Multisample Resolve Operations

Render pass multisample resolve operations combine sample values from a single pixel in a multisample attachment and store the result to the corresponding pixel in a single sample attachment.

Multisample resolve operations for attachments execute in the `VK_PIPELINE_STAGE_COLOR_ATTACHMENT_OUTPUT_BIT` pipeline stage. A final resolve operation for all pixels in the render area happens-after any recorded command which writes a pixel via the multisample attachment to be resolved or an explicit alias of it in the subpass that it is specified. Any single sample attachment specified for use in a multisample resolve operation may have its contents modified at any point once rendering begins for the render pass instance. Reads from the multisample attachment can be synchronized with `VK_ACCESS_COLOR_ATTACHMENT_READ_BIT`. Access to the single sample attachment can be synchronized with `VK_ACCESS_COLOR_ATTACHMENT_READ_BIT` and `VK_ACCESS_COLOR_ATTACHMENT_WRITE_BIT`. These pipeline stage and access types are used whether the attachments are color or depth/stencil attachments.

When using render pass objects, a subpass dependency specified with the above pipeline stages and access flags will ensure synchronization with multisample resolve operations for any attachments that were last accessed by that subpass. This allows later subpasses to read resolved values as input attachments.

Resolve operations only update values within the defined render area for the render pass instance. However, any writes performed by a resolve operation (as defined by its access masks) to a given attachment may read and write back any memory locations within the image subresource bound for that attachment. For depth/stencil images, if `separateDepthStencilAttachmentAccess` is `VK_FALSE`, writes to one aspect may also result in read-modify-write operations for the other aspect. If the subresource is in the `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT` layout, implementations must not access pixels outside of the render area.

Note | As entire subresources could be accessed by multisample resolve operations, applications cannot safely access values outside of the render area via aliased resources during a render pass instance when a multisample resolve operation is performed.

Multisample values in a multisample attachment are combined according to the resolve mode used:

    // Provided by VK_VERSION_1_2
    typedef enum VkResolveModeFlagBits {
        VK_RESOLVE_MODE_NONE = 0,
        VK_RESOLVE_MODE_SAMPLE_ZERO_BIT = 0x00000001,
        VK_RESOLVE_MODE_AVERAGE_BIT = 0x00000002,
        VK_RESOLVE_MODE_MIN_BIT = 0x00000004,
        VK_RESOLVE_MODE_MAX_BIT = 0x00000008,
      // Provided by VK_ANDROID_external_format_resolve with VK_KHR_dynamic_rendering or VK_VERSION_1_3
        VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID = 0x00000010,
      // Provided by VK_KHR_depth_stencil_resolve
        VK_RESOLVE_MODE_NONE_KHR = VK_RESOLVE_MODE_NONE,
      // Provided by VK_KHR_depth_stencil_resolve
        VK_RESOLVE_MODE_SAMPLE_ZERO_BIT_KHR = VK_RESOLVE_MODE_SAMPLE_ZERO_BIT,
      // Provided by VK_KHR_depth_stencil_resolve
        VK_RESOLVE_MODE_AVERAGE_BIT_KHR = VK_RESOLVE_MODE_AVERAGE_BIT,
      // Provided by VK_KHR_depth_stencil_resolve
        VK_RESOLVE_MODE_MIN_BIT_KHR = VK_RESOLVE_MODE_MIN_BIT,
      // Provided by VK_KHR_depth_stencil_resolve
        VK_RESOLVE_MODE_MAX_BIT_KHR = VK_RESOLVE_MODE_MAX_BIT,
    } VkResolveModeFlagBits;

or the equivalent

    // Provided by VK_KHR_depth_stencil_resolve
    typedef VkResolveModeFlagBits VkResolveModeFlagBitsKHR;

- `VK_RESOLVE_MODE_NONE` specifies that no resolve operation is done.

- `VK_RESOLVE_MODE_SAMPLE_ZERO_BIT` specifies that result of the resolve operation is equal to the value of sample 0.

- `VK_RESOLVE_MODE_AVERAGE_BIT` specifies that result of the resolve operation is the average of the sample values.

- `VK_RESOLVE_MODE_MIN_BIT` specifies that result of the resolve operation is the minimum of the sample values.

- `VK_RESOLVE_MODE_MAX_BIT` specifies that result of the resolve operation is the maximum of the sample values.

- `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID` specifies that rather than a multisample resolve, a single sampled color attachment will be downsampled into a Y′CBCR format image specified by an external Android format. Unlike other resolve modes, implementations can resolve multiple times during rendering, or even bypass writing to the color attachment altogether, as long as the final value is resolved to the resolve attachment. Values in the G, B, and R channels of the color attachment will be written to the Y, CB, and CR channels of the external format image, respectively. Chroma values are calculated as if sampling with a linear filter from the color attachment at full rate, at the location the chroma values sit according to VkPhysicalDeviceExternalFormatResolvePropertiesANDROID::`chromaOffsetX`, VkPhysicalDeviceExternalFormatResolvePropertiesANDROID::`chromaOffsetY`, and the chroma sample rate of the resolved image.

If no resolve mode is otherwise specified, `VK_RESOLVE_MODE_AVERAGE_BIT` is used.

Note | No range compression or Y′CBCR model conversion is performed by `VK_RESOLVE_MODE_EXTERNAL_FORMAT_DOWNSAMPLE_ANDROID`; applications have to do these conversions themselves. Value outputs are expected to match those that would be read through a Y′CBCR sampler using `VK_SAMPLER_YCBCR_MODEL_CONVERSION_RGB_IDENTITY`. The color space that the values should be in is defined by the platform and is not exposed via Vulkan.

    // Provided by VK_VERSION_1_2
    typedef VkFlags VkResolveModeFlags;

or the equivalent

    // Provided by VK_KHR_depth_stencil_resolve
    typedef VkResolveModeFlags VkResolveModeFlagsKHR;

`VkResolveModeFlags` is a bitmask type for setting a mask of zero or more VkResolveModeFlagBits.

### 8.8. Render Pass Commands

An application records the commands for a render pass instance one subpass at a time, by beginning a render pass instance, iterating over the subpasses to record commands for that subpass, and then ending the render pass instance.

To begin a render pass instance, call:

    // Provided by VK_VERSION_1_0
    void vkCmdBeginRenderPass(
        VkCommandBuffer                             commandBuffer,
        const VkRenderPassBeginInfo*                pRenderPassBegin,
        VkSubpassContents                           contents);

- `commandBuffer` is the command buffer in which to record the command.

- `pRenderPassBegin` is a pointer to a VkRenderPassBeginInfo structure specifying the render pass to begin an instance of, and the framebuffer the instance uses.

- `contents` is a VkSubpassContents value specifying how the commands in the first subpass will be provided.

After beginning a render pass instance, the command buffer is ready to record the commands for the first subpass of that render pass.

Valid Usage

- VUID-vkCmdBeginRenderPass-initialLayout-00895
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_COLOR_ATTACHMENT_BIT`

- VUID-vkCmdBeginRenderPass-initialLayout-01758
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-vkCmdBeginRenderPass-initialLayout-02842
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-vkCmdBeginRenderPass-stencilInitialLayout-02843
  If any of the `stencilInitialLayout` or `stencilFinalLayout` member of the `VkAttachmentDescriptionStencilLayout` structures or the `stencilLayout` member of the `VkAttachmentReferenceStencilLayout` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-vkCmdBeginRenderPass-initialLayout-00897
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_SAMPLED_BIT` or `VK_IMAGE_USAGE_INPUT_ATTACHMENT_BIT`

- VUID-vkCmdBeginRenderPass-initialLayout-00898
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_TRANSFER_SRC_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_TRANSFER_SRC_BIT`

- VUID-vkCmdBeginRenderPass-initialLayout-00899
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_TRANSFER_DST_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_TRANSFER_DST_BIT`

- VUID-vkCmdBeginRenderPass-initialLayout-00900
  If the `initialLayout` member of any of the `VkAttachmentDescription` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is not `VK_IMAGE_LAYOUT_UNDEFINED`, then each such `initialLayout` must be equal to the current layout of the corresponding attachment image subresource of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin`

- VUID-vkCmdBeginRenderPass-srcStageMask-06451
  The `srcStageMask` members of any element of the `pDependencies` member of VkRenderPassCreateInfo used to create `renderPass` must be supported by the capabilities of the queue family identified by the `queueFamilyIndex` member of the VkCommandPoolCreateInfo used to create the command pool which `commandBuffer` was allocated from

- VUID-vkCmdBeginRenderPass-dstStageMask-06452
  The `dstStageMask` members of any element of the `pDependencies` member of VkRenderPassCreateInfo used to create `renderPass` must be supported by the capabilities of the queue family identified by the `queueFamilyIndex` member of the VkCommandPoolCreateInfo used to create the command pool which `commandBuffer` was allocated from

- VUID-vkCmdBeginRenderPass-framebuffer-02532
  For any attachment in `framebuffer` that is used by `renderPass` and is bound to memory locations that are also bound to another attachment used by `renderPass`, and if at least one of those uses causes either attachment to be written to, both attachments must have had the `VK_ATTACHMENT_DESCRIPTION_MAY_ALIAS_BIT` set

- VUID-vkCmdBeginRenderPass-framebuffer-09045
  If any attachments specified in `framebuffer` are used by `renderPass` and are bound to overlapping memory locations, there must be only one that is used as a color attachment, depth/stencil, or resolve attachment in any subpass

- VUID-vkCmdBeginRenderPass-initialLayout-07000
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including either the `VK_IMAGE_USAGE_COLOR_ATTACHMENT_BIT` or `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT` and either the `VK_IMAGE_USAGE_INPUT_ATTACHMENT_BIT` or `VK_IMAGE_USAGE_SAMPLED_BIT` usage bits

- VUID-vkCmdBeginRenderPass-initialLayout-07001
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value the `VK_IMAGE_USAGE_ATTACHMENT_FEEDBACK_LOOP_BIT_EXT` usage bit

- VUID-vkCmdBeginRenderPass-initialLayout-09537
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_RENDERING_LOCAL_READ` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including either `VK_IMAGE_USAGE_STORAGE_BIT`, or both `VK_IMAGE_USAGE_INPUT_ATTACHMENT_BIT` and either of `VK_IMAGE_USAGE_COLOR_ATTACHMENT_BIT` or `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-vkCmdBeginRenderPass-contents-09640
  If `contents` is `VK_SUBPASS_CONTENTS_INLINE_AND_SECONDARY_COMMAND_BUFFERS_KHR`, then at least one of the following features must be enabled:

  - `maintenance7`

  - `nestedCommandBuffer`

Valid Usage (Implicit)

- VUID-vkCmdBeginRenderPass-commandBuffer-parameter
  `commandBuffer` must be a valid VkCommandBuffer handle

- VUID-vkCmdBeginRenderPass-pRenderPassBegin-parameter
  `pRenderPassBegin` must be a valid pointer to a valid VkRenderPassBeginInfo structure

- VUID-vkCmdBeginRenderPass-contents-parameter
  `contents` must be a valid VkSubpassContents value

- VUID-vkCmdBeginRenderPass-commandBuffer-recording
  `commandBuffer` must be in the recording state

- VUID-vkCmdBeginRenderPass-commandBuffer-cmdpool
  The `VkCommandPool` that `commandBuffer` was allocated from must support graphics operations

- VUID-vkCmdBeginRenderPass-renderpass
  This command must only be called outside of a render pass instance

- VUID-vkCmdBeginRenderPass-videocoding
  This command must only be called outside of a video coding scope

- VUID-vkCmdBeginRenderPass-bufferlevel
  `commandBuffer` must be a primary `VkCommandBuffer`

Host Synchronization

- Host access to `commandBuffer` must be externally synchronized

- Host access to the `VkCommandPool` that `commandBuffer` was allocated from must be externally synchronized

Command Properties

Command Buffer Levels | Render Pass Scope | Video Coding Scope | Supported Queue Types | Command Type
--- | --- | --- | --- | ---
Primary | Outside | Outside | Graphics | Action State Synchronization

Alternatively to begin a render pass, call:

    // Provided by VK_VERSION_1_2
    void vkCmdBeginRenderPass2(
        VkCommandBuffer                             commandBuffer,
        const VkRenderPassBeginInfo*                pRenderPassBegin,
        const VkSubpassBeginInfo*                   pSubpassBeginInfo);

or the equivalent command

    // Provided by VK_KHR_create_renderpass2
    void vkCmdBeginRenderPass2KHR(
        VkCommandBuffer                             commandBuffer,
        const VkRenderPassBeginInfo*                pRenderPassBegin,
        const VkSubpassBeginInfo*                   pSubpassBeginInfo);

- `commandBuffer` is the command buffer in which to record the command.

- `pRenderPassBegin` is a pointer to a VkRenderPassBeginInfo structure specifying the render pass to begin an instance of, and the framebuffer the instance uses.

- `pSubpassBeginInfo` is a pointer to a VkSubpassBeginInfo structure containing information about the subpass which is about to begin rendering.

After beginning a render pass instance, the command buffer is ready to record the commands for the first subpass of that render pass.

Valid Usage

- VUID-vkCmdBeginRenderPass2-framebuffer-02779
  Both the `framebuffer` and `renderPass` members of `pRenderPassBegin` must have been created on the same VkDevice that `commandBuffer` was allocated on

- VUID-vkCmdBeginRenderPass2-initialLayout-03094
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_COLOR_ATTACHMENT_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_COLOR_ATTACHMENT_BIT`

- VUID-vkCmdBeginRenderPass2-initialLayout-03096
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_DEPTH_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_DEPTH_STENCIL_READ_ONLY_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-vkCmdBeginRenderPass2-initialLayout-02844
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_OPTIMAL`, `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-vkCmdBeginRenderPass2-stencilInitialLayout-02845
  If any of the `stencilInitialLayout` or `stencilFinalLayout` member of the `VkAttachmentDescriptionStencilLayout` structures or the `stencilLayout` member of the `VkAttachmentReferenceStencilLayout` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_STENCIL_ATTACHMENT_OPTIMAL`, or `VK_IMAGE_LAYOUT_STENCIL_READ_ONLY_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

- VUID-vkCmdBeginRenderPass2-initialLayout-03097
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_SHADER_READ_ONLY_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_SAMPLED_BIT` or `VK_IMAGE_USAGE_INPUT_ATTACHMENT_BIT`

- VUID-vkCmdBeginRenderPass2-initialLayout-03098
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_TRANSFER_SRC_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_TRANSFER_SRC_BIT`

- VUID-vkCmdBeginRenderPass2-initialLayout-03099
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_TRANSFER_DST_OPTIMAL` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including `VK_IMAGE_USAGE_TRANSFER_DST_BIT`

- VUID-vkCmdBeginRenderPass2-initialLayout-03100
  If the `initialLayout` member of any of the `VkAttachmentDescription` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is not `VK_IMAGE_LAYOUT_UNDEFINED`, then each such `initialLayout` must be equal to the current layout of the corresponding attachment image subresource of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin`

- VUID-vkCmdBeginRenderPass2-srcStageMask-06453
  The `srcStageMask` members of any element of the `pDependencies` member of VkRenderPassCreateInfo used to create `renderPass` must be supported by the capabilities of the queue family identified by the `queueFamilyIndex` member of the VkCommandPoolCreateInfo used to create the command pool which `commandBuffer` was allocated from

- VUID-vkCmdBeginRenderPass2-dstStageMask-06454
  The `dstStageMask` members of any element of the `pDependencies` member of VkRenderPassCreateInfo used to create `renderPass` must be supported by the capabilities of the queue family identified by the `queueFamilyIndex` member of the VkCommandPoolCreateInfo used to create the command pool which `commandBuffer` was allocated from

- VUID-vkCmdBeginRenderPass2-framebuffer-02533
  For any attachment in `framebuffer` that is used by `renderPass` and is bound to memory locations that are also bound to another attachment used by `renderPass`, and if at least one of those uses causes either attachment to be written to, both attachments must have had the `VK_ATTACHMENT_DESCRIPTION_MAY_ALIAS_BIT` set

- VUID-vkCmdBeginRenderPass2-framebuffer-09046
  If any attachments specified in `framebuffer` are used by `renderPass` and are bound to overlapping memory locations, there must be only one that is used as a color attachment, depth/stencil, or resolve attachment in any subpass

- VUID-vkCmdBeginRenderPass2-initialLayout-07002
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including either the `VK_IMAGE_USAGE_COLOR_ATTACHMENT_BIT` or `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT` and either the `VK_IMAGE_USAGE_INPUT_ATTACHMENT_BIT` or `VK_IMAGE_USAGE_SAMPLED_BIT` usage bits

- VUID-vkCmdBeginRenderPass2-initialLayout-07003
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value the `VK_IMAGE_USAGE_ATTACHMENT_FEEDBACK_LOOP_BIT_EXT` usage bit

- VUID-vkCmdBeginRenderPass2-initialLayout-09538
  If any of the `initialLayout` or `finalLayout` member of the `VkAttachmentDescription` structures or the `layout` member of the `VkAttachmentReference` structures specified when creating the render pass specified in the `renderPass` member of `pRenderPassBegin` is `VK_IMAGE_LAYOUT_RENDERING_LOCAL_READ` then the corresponding attachment image view of the framebuffer specified in the `framebuffer` member of `pRenderPassBegin` must have been created with a `usage` value including either `VK_IMAGE_USAGE_STORAGE_BIT`, or both `VK_IMAGE_USAGE_INPUT_ATTACHMENT_BIT` and either of `VK_IMAGE_USAGE_COLOR_ATTACHMENT_BIT` or `VK_IMAGE_USAGE_DEPTH_STENCIL_ATTACHMENT_BIT`

Valid Usage (Implicit)

- VUID-vkCmdBeginRenderPass2-commandBuffer-parameter
  `commandBuffer` must be a valid VkCommandBuffer handle

- VUID-vkCmdBeginRenderPass2-pRenderPassBegin-parameter
  `pRenderPassBegin` must be a valid pointer to a valid VkRenderPassBeginInfo structure

- VUID-vkCmdBeginRenderPass2-pSubpassBeginInfo-parameter
  `pSubpassBeginInfo` must be a valid pointer to a valid VkSubpassBeginInfo structure

- VUID-vkCmdBeginRenderPass2-commandBuffer-recording
  `commandBuffer` must be in the recording state

- VUID-vkCmdBeginRenderPass2-commandBuffer-cmdpool
  The `VkCommandPool` that `commandBuffer` was allocated from must support graphics operations

- VUID-vkCmdBeginRenderPass2-renderpass
  This command must only be called outside of a render pass instance

- VUID-vkCmdBeginRenderPass2-videocoding
  This command must only be called outside of a video coding scope

- VUID-vkCmdBeginRenderPass2-bufferlevel
  `commandBuffer` must be a primary `VkCommandBuffer`

Host Synchronization

- Host access to `commandBuffer` must be externally synchronized

- Host access to the `VkCommandPool` that `commandBuffer` was allocated from must be externally synchronized

Command Properties

Command Buffer Levels | Render Pass Scope | Video Coding Scope | Supported Queue Types | Command Type
--- | --- | --- | --- | ---
Primary | Outside | Outside | Graphics | Action State Synchronization

The `VkRenderPassBeginInfo` structure is defined as:

    // Provided by VK_VERSION_1_0
    typedef struct VkRenderPassBeginInfo {
        VkStructureType        sType;
        const void*            pNext;
        VkRenderPass           renderPass;
        VkFramebuffer          framebuffer;
        VkRect2D               renderArea;
        uint32_t               clearValueCount;
        const VkClearValue*    pClearValues;
    } VkRenderPassBeginInfo;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `renderPass` is the render pass to begin an instance of.

- `framebuffer` is the framebuffer containing the attachments that are used with the render pass.

- `renderArea` is the render area that is affected by the render pass instance, and is described in more detail below.

- `clearValueCount` is the number of elements in `pClearValues`.

- `pClearValues` is a pointer to an array of `clearValueCount` VkClearValue structures containing clear values for each attachment, if the attachment uses a `loadOp` value of `VK_ATTACHMENT_LOAD_OP_CLEAR` or if the attachment has a depth/stencil format and uses a `stencilLoadOp` value of `VK_ATTACHMENT_LOAD_OP_CLEAR`. The array is indexed by attachment number. Only elements corresponding to cleared attachments are used. Other elements of `pClearValues` are ignored.

`renderArea` is the render area that is affected by the render pass instance. The effects of attachment load, store and multisample resolve operations are restricted to the pixels whose x and y coordinates fall within the render area on all attachments. The render area extends to all layers of `framebuffer`. The application must ensure (using scissor if necessary) that all rendering is contained within the render area. The render area, after any transform specified by VkRenderPassTransformBeginInfoQCOM::`transform` is applied, must be contained within the framebuffer dimensions.

If render pass transform is enabled, then `renderArea` must equal the framebuffer pre-transformed dimensions. After `renderArea` has been transformed by VkRenderPassTransformBeginInfoQCOM::`transform`, the resulting render area must be equal to the framebuffer dimensions.

If multiview is enabled in `renderPass`, and `multiviewPerViewRenderAreas` feature is enabled, and there is an instance of VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM included in the `pNext` chain with `perViewRenderAreaCount` not equal to `0`, then the elements of VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM::`pPerViewRenderAreas` override `renderArea` and define a render area for each view. In this case, `renderArea` must be an area at least as large as the union of all the per-view render areas.

If the `subpassShading` feature is enabled, then `renderArea` must equal the framebuffer dimensions.

Note | There may be a performance cost for using a render area smaller than the framebuffer, unless it matches the render area granularity for the render pass.

Valid Usage

- VUID-VkRenderPassBeginInfo-clearValueCount-00902
  `clearValueCount` must be greater than the largest attachment index in `renderPass` specifying a `loadOp` (or `stencilLoadOp`, if the attachment has a depth/stencil format) of `VK_ATTACHMENT_LOAD_OP_CLEAR`

- VUID-VkRenderPassBeginInfo-clearValueCount-04962
  If `clearValueCount` is not `0`, `pClearValues` must be a valid pointer to an array of `clearValueCount` VkClearValue unions

- VUID-VkRenderPassBeginInfo-renderPass-00904
  `renderPass` must be compatible with the `renderPass` member of the VkFramebufferCreateInfo structure specified when creating `framebuffer`

- VUID-VkRenderPassBeginInfo-None-08996
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, `renderArea.extent.width` must be greater than 0

- VUID-VkRenderPassBeginInfo-None-08997
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, `renderArea.extent.height` must be greater than 0

- VUID-VkRenderPassBeginInfo-pNext-02850
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, `renderArea.offset.x` must be greater than or equal to 0

- VUID-VkRenderPassBeginInfo-pNext-02851
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, `renderArea.offset.y` must be greater than or equal to 0

- VUID-VkRenderPassBeginInfo-pNext-02852
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, `renderArea.offset.x` + `renderArea.extent.width` must be less than or equal to VkFramebufferCreateInfo::`width` the `framebuffer` was created with

- VUID-VkRenderPassBeginInfo-pNext-02853
  If the `pNext` chain does not contain VkDeviceGroupRenderPassBeginInfo or its `deviceRenderAreaCount` member is equal to 0, `renderArea.offset.y` + `renderArea.extent.height` must be less than or equal to VkFramebufferCreateInfo::`height` the `framebuffer` was created with

- VUID-VkRenderPassBeginInfo-pNext-02856
  If the `pNext` chain contains VkDeviceGroupRenderPassBeginInfo, `offset.x` + `extent.width` of each element of `pDeviceRenderAreas` must be less than or equal to VkFramebufferCreateInfo::`width` the `framebuffer` was created with

- VUID-VkRenderPassBeginInfo-pNext-02857
  If the `pNext` chain contains VkDeviceGroupRenderPassBeginInfo, `offset.y` + `extent.height` of each element of `pDeviceRenderAreas` must be less than or equal to VkFramebufferCreateInfo::`height` the `framebuffer` was created with

- VUID-VkRenderPassBeginInfo-framebuffer-03207
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that did not include `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, and the `pNext` chain includes a VkRenderPassAttachmentBeginInfo structure, its `attachmentCount` must be zero

- VUID-VkRenderPassBeginInfo-framebuffer-03208
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, the `attachmentCount` of a VkRenderPassAttachmentBeginInfo structure included in the `pNext` chain must be equal to the value of VkFramebufferAttachmentsCreateInfo::`attachmentImageInfoCount` used to create `framebuffer`

- VUID-VkRenderPassBeginInfo-framebuffer-02780
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of the `pAttachments` member of a VkRenderPassAttachmentBeginInfo structure included in the `pNext` chain must have been created on the same VkDevice as `framebuffer` and `renderPass`

- VUID-VkRenderPassBeginInfo-framebuffer-03209
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of the `pAttachments` member of a VkRenderPassAttachmentBeginInfo structure included in the `pNext` chain must be a VkImageView of an image created with a value of VkImageCreateInfo::`flags` equal to the `flags` member of the corresponding element of VkFramebufferAttachmentsCreateInfo::`pAttachmentImageInfos` used to create `framebuffer`

- VUID-VkRenderPassBeginInfo-framebuffer-04627
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of the `pAttachments` member of a VkRenderPassAttachmentBeginInfo structure included in the `pNext` chain must be a VkImageView with an inherited usage equal to the `usage` member of the corresponding element of VkFramebufferAttachmentsCreateInfo::`pAttachmentImageInfos` used to create `framebuffer`

- VUID-VkRenderPassBeginInfo-framebuffer-03211
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of the `pAttachments` member of a VkRenderPassAttachmentBeginInfo structure included in the `pNext` chain must be a VkImageView with a width equal to the `width` member of the corresponding element of VkFramebufferAttachmentsCreateInfo::`pAttachmentImageInfos` used to create `framebuffer`

- VUID-VkRenderPassBeginInfo-framebuffer-03212
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of the `pAttachments` member of a VkRenderPassAttachmentBeginInfo structure included in the `pNext` chain must be a VkImageView with a height equal to the `height` member of the corresponding element of VkFramebufferAttachmentsCreateInfo::`pAttachmentImageInfos` used to create `framebuffer`

- VUID-VkRenderPassBeginInfo-framebuffer-03213
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of the `pAttachments` member of a VkRenderPassAttachmentBeginInfo structure included in the `pNext` chain must be a VkImageView of an image created with a value of VkImageViewCreateInfo::`subresourceRange.layerCount` equal to the `layerCount` member of the corresponding element of VkFramebufferAttachmentsCreateInfo::`pAttachmentImageInfos` used to create `framebuffer`

- VUID-VkRenderPassBeginInfo-framebuffer-03214
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of the `pAttachments` member of a VkRenderPassAttachmentBeginInfo structure included in the `pNext` chain must be a VkImageView of an image created with a value of VkImageFormatListCreateInfo::`viewFormatCount` equal to the `viewFormatCount` member of the corresponding element of VkFramebufferAttachmentsCreateInfo::`pAttachmentImageInfos` used to create `framebuffer`

- VUID-VkRenderPassBeginInfo-framebuffer-03215
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of the `pAttachments` member of a VkRenderPassAttachmentBeginInfo structure included in the `pNext` chain must be a VkImageView of an image created with a set of elements in VkImageFormatListCreateInfo::`pViewFormats` equal to the set of elements in the `pViewFormats` member of the corresponding element of VkFramebufferAttachmentsCreateInfo::`pAttachmentImageInfos` used to create `framebuffer`

- VUID-VkRenderPassBeginInfo-framebuffer-03216
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of the `pAttachments` member of a VkRenderPassAttachmentBeginInfo structure included in the `pNext` chain must be a VkImageView of an image created with a value of VkImageViewCreateInfo::`format` equal to the corresponding value of VkAttachmentDescription::`format` in `renderPass`

- VUID-VkRenderPassBeginInfo-framebuffer-09353
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, and the `nullColorAttachmentWithExternalFormatResolve` is `VK_FALSE`, the format of the color attachment for each subpass that includes an external format image as a resolve attachment must have a format equal to the value of VkAndroidHardwareBufferFormatResolvePropertiesANDROID::`colorAttachmentFormat` as returned by a call to vkGetAndroidHardwareBufferPropertiesANDROID for the Android hardware buffer that was used to create the image view use as its resolve attachment

- VUID-VkRenderPassBeginInfo-framebuffer-09354
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of the `pAttachments` member of a VkRenderPassAttachmentBeginInfo structure included in the `pNext` chain must be a VkImageView of an image created with a value of VkExternalFormatANDROID::`externalFormat` equal to VkExternalFormatANDROID::`externalFormat` in the `pNext` chain of the corresponding VkAttachmentDescription2 structure used to create `renderPass`

- VUID-VkRenderPassBeginInfo-framebuffer-09047
  If `framebuffer` was created with a VkFramebufferCreateInfo::`flags` value that included `VK_FRAMEBUFFER_CREATE_IMAGELESS_BIT`, each element of the `pAttachments` member of a VkRenderPassAttachmentBeginInfo structure included in the `pNext` chain must be a VkImageView of an image created with a value of VkImageCreateInfo::`samples` equal to the corresponding value of VkAttachmentDescription::`samples` in `renderPass` , or `VK_SAMPLE_COUNT_1_BIT` if `renderPass` was created with VkMultisampledRenderToSingleSampledInfoEXT structure in the `pNext` chain with `multisampledRenderToSingleSampledEnable` equal to `VK_TRUE`

- VUID-VkRenderPassBeginInfo-pNext-02869
  If the `pNext` chain includes VkRenderPassTransformBeginInfoQCOM, `renderArea.offset` must equal (0,0)

- VUID-VkRenderPassBeginInfo-pNext-02870
  If the `pNext` chain includes VkRenderPassTransformBeginInfoQCOM, `renderArea.extent` transformed by VkRenderPassTransformBeginInfoQCOM::`transform` must equal the `framebuffer` dimensions

- VUID-VkRenderPassBeginInfo-perViewRenderAreaCount-07859
  If the `perViewRenderAreaCount` member of a VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM structure included in the `pNext` chain is not `0`, then the `multiviewPerViewRenderAreas` feature must be enabled

- VUID-VkRenderPassBeginInfo-perViewRenderAreaCount-07860
  If the `perViewRenderAreaCount` member of a VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM structure included in the `pNext` chain is not `0`, then `renderArea` must specify a render area that includes the union of all per view render areas

- VUID-VkRenderPassBeginInfo-pNext-09539
  If the `pNext` chain contains a VkRenderPassStripeBeginInfoARM structure, the union of stripe areas defined by the elements of VkRenderPassStripeInfoARM::`pStripeInfos` must cover the `renderArea`

Valid Usage (Implicit)

- VUID-VkRenderPassBeginInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_BEGIN_INFO`

- VUID-VkRenderPassBeginInfo-pNext-pNext
  Each `pNext` member of any structure (including this one) in the `pNext` chain must be either `NULL` or a pointer to a valid instance of VkDeviceGroupRenderPassBeginInfo, VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM, VkRenderPassAttachmentBeginInfo, VkRenderPassSampleLocationsBeginInfoEXT, VkRenderPassStripeBeginInfoARM, or VkRenderPassTransformBeginInfoQCOM

- VUID-VkRenderPassBeginInfo-sType-unique
  The `sType` value of each struct in the `pNext` chain must be unique

- VUID-VkRenderPassBeginInfo-renderPass-parameter
  `renderPass` must be a valid VkRenderPass handle

- VUID-VkRenderPassBeginInfo-framebuffer-parameter
  `framebuffer` must be a valid VkFramebuffer handle

- VUID-VkRenderPassBeginInfo-commonparent
  Both of `framebuffer`, and `renderPass` must have been created, allocated, or retrieved from the same VkDevice

The image layout of the depth aspect of a depth/stencil attachment referring to an image created with `VK_IMAGE_CREATE_SAMPLE_LOCATIONS_COMPATIBLE_DEPTH_BIT_EXT` is dependent on the last sample locations used to render to the image subresource, thus preserving the contents of such depth/stencil attachments across subpass boundaries requires the application to specify these sample locations whenever a layout transition of the attachment may occur. This information can be provided by adding a `VkRenderPassSampleLocationsBeginInfoEXT` structure to the `pNext` chain of `VkRenderPassBeginInfo`.

The `VkRenderPassSampleLocationsBeginInfoEXT` structure is defined as:

    // Provided by VK_EXT_sample_locations
    typedef struct VkRenderPassSampleLocationsBeginInfoEXT {
        VkStructureType                          sType;
        const void*                              pNext;
        uint32_t                                 attachmentInitialSampleLocationsCount;
        const VkAttachmentSampleLocationsEXT*    pAttachmentInitialSampleLocations;
        uint32_t                                 postSubpassSampleLocationsCount;
        const VkSubpassSampleLocationsEXT*       pPostSubpassSampleLocations;
    } VkRenderPassSampleLocationsBeginInfoEXT;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `attachmentInitialSampleLocationsCount` is the number of elements in the `pAttachmentInitialSampleLocations` array.

- `pAttachmentInitialSampleLocations` is a pointer to an array of `attachmentInitialSampleLocationsCount` VkAttachmentSampleLocationsEXT structures specifying the attachment indices and their corresponding sample location state. Each element of `pAttachmentInitialSampleLocations` can specify the sample location state to use in the automatic layout transition performed to transition a depth/stencil attachment from the initial layout of the attachment to the image layout specified for the attachment in the first subpass using it.

- `postSubpassSampleLocationsCount` is the number of elements in the `pPostSubpassSampleLocations` array.

- `pPostSubpassSampleLocations` is a pointer to an array of `postSubpassSampleLocationsCount` VkSubpassSampleLocationsEXT structures specifying the subpass indices and their corresponding sample location state. Each element of `pPostSubpassSampleLocations` can specify the sample location state to use in the automatic layout transition performed to transition the depth/stencil attachment used by the specified subpass to the image layout specified in a dependent subpass or to the final layout of the attachment in case the specified subpass is the last subpass using that attachment. In addition, if VkPhysicalDeviceSampleLocationsPropertiesEXT::`variableSampleLocations` is `VK_FALSE`, each element of `pPostSubpassSampleLocations` must specify the sample location state that matches the sample locations used by all pipelines that will be bound to a command buffer during the specified subpass. If `variableSampleLocations` is `VK_TRUE`, the sample locations used for rasterization do not depend on `pPostSubpassSampleLocations`.

Valid Usage (Implicit)

- VUID-VkRenderPassSampleLocationsBeginInfoEXT-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_SAMPLE_LOCATIONS_BEGIN_INFO_EXT`

- VUID-VkRenderPassSampleLocationsBeginInfoEXT-pAttachmentInitialSampleLocations-parameter
  If `attachmentInitialSampleLocationsCount` is not `0`, `pAttachmentInitialSampleLocations` must be a valid pointer to an array of `attachmentInitialSampleLocationsCount` valid VkAttachmentSampleLocationsEXT structures

- VUID-VkRenderPassSampleLocationsBeginInfoEXT-pPostSubpassSampleLocations-parameter
  If `postSubpassSampleLocationsCount` is not `0`, `pPostSubpassSampleLocations` must be a valid pointer to an array of `postSubpassSampleLocationsCount` valid VkSubpassSampleLocationsEXT structures

The `VkAttachmentSampleLocationsEXT` structure is defined as:

    // Provided by VK_EXT_sample_locations
    typedef struct VkAttachmentSampleLocationsEXT {
        uint32_t                    attachmentIndex;
        VkSampleLocationsInfoEXT    sampleLocationsInfo;
    } VkAttachmentSampleLocationsEXT;

- `attachmentIndex` is the index of the attachment for which the sample locations state is provided.

- `sampleLocationsInfo` is the sample locations state to use for the layout transition of the given attachment from the initial layout of the attachment to the image layout specified for the attachment in the first subpass using it.

If the image referenced by the framebuffer attachment at index `attachmentIndex` was not created with `VK_IMAGE_CREATE_SAMPLE_LOCATIONS_COMPATIBLE_DEPTH_BIT_EXT` then the values specified in `sampleLocationsInfo` are ignored.

Valid Usage

- VUID-VkAttachmentSampleLocationsEXT-attachmentIndex-01531
  `attachmentIndex` must be less than the `attachmentCount` specified in VkRenderPassCreateInfo the render pass specified by VkRenderPassBeginInfo::`renderPass` was created with

Valid Usage (Implicit)

- VUID-VkAttachmentSampleLocationsEXT-sampleLocationsInfo-parameter
  `sampleLocationsInfo` must be a valid VkSampleLocationsInfoEXT structure

The `VkSubpassSampleLocationsEXT` structure is defined as:

    // Provided by VK_EXT_sample_locations
    typedef struct VkSubpassSampleLocationsEXT {
        uint32_t                    subpassIndex;
        VkSampleLocationsInfoEXT    sampleLocationsInfo;
    } VkSubpassSampleLocationsEXT;

- `subpassIndex` is the index of the subpass for which the sample locations state is provided.

- `sampleLocationsInfo` is the sample locations state to use for the layout transition of the depth/stencil attachment away from the image layout the attachment is used with in the subpass specified in `subpassIndex`.

If the image referenced by the depth/stencil attachment used in the subpass identified by `subpassIndex` was not created with `VK_IMAGE_CREATE_SAMPLE_LOCATIONS_COMPATIBLE_DEPTH_BIT_EXT` or if the subpass does not use a depth/stencil attachment, and VkPhysicalDeviceSampleLocationsPropertiesEXT::`variableSampleLocations` is `VK_TRUE` then the values specified in `sampleLocationsInfo` are ignored.

Valid Usage

- VUID-VkSubpassSampleLocationsEXT-subpassIndex-01532
  `subpassIndex` must be less than the `subpassCount` specified in VkRenderPassCreateInfo the render pass specified by VkRenderPassBeginInfo::`renderPass` was created with

Valid Usage (Implicit)

- VUID-VkSubpassSampleLocationsEXT-sampleLocationsInfo-parameter
  `sampleLocationsInfo` must be a valid VkSampleLocationsInfoEXT structure

To begin a render pass instance with render pass transform enabled, add the VkRenderPassTransformBeginInfoQCOM to the `pNext` chain of VkRenderPassBeginInfo structure passed to the vkCmdBeginRenderPass command specifying the render pass transform.

The `VkRenderPassTransformBeginInfoQCOM` structure is defined as:

    // Provided by VK_QCOM_render_pass_transform
    typedef struct VkRenderPassTransformBeginInfoQCOM {
        VkStructureType                  sType;
        void*                            pNext;
        VkSurfaceTransformFlagBitsKHR    transform;
    } VkRenderPassTransformBeginInfoQCOM;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `transform` is a VkSurfaceTransformFlagBitsKHR value describing the transform to be applied to rasterization.

Valid Usage

- VUID-VkRenderPassTransformBeginInfoQCOM-transform-02871
  `transform` must be `VK_SURFACE_TRANSFORM_IDENTITY_BIT_KHR`, `VK_SURFACE_TRANSFORM_ROTATE_90_BIT_KHR`, `VK_SURFACE_TRANSFORM_ROTATE_180_BIT_KHR`, or `VK_SURFACE_TRANSFORM_ROTATE_270_BIT_KHR`

- VUID-VkRenderPassTransformBeginInfoQCOM-flags-02872
  The `renderpass` must have been created with VkRenderPassCreateInfo::`flags` containing `VK_RENDER_PASS_CREATE_TRANSFORM_BIT_QCOM`

Valid Usage (Implicit)

- VUID-VkRenderPassTransformBeginInfoQCOM-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_TRANSFORM_BEGIN_INFO_QCOM`

The `VkSubpassBeginInfo` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkSubpassBeginInfo {
        VkStructureType      sType;
        const void*          pNext;
        VkSubpassContents    contents;
    } VkSubpassBeginInfo;

or the equivalent

    // Provided by VK_KHR_create_renderpass2
    typedef VkSubpassBeginInfo VkSubpassBeginInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `contents` is a VkSubpassContents value specifying how the commands in the next subpass will be provided.

Valid Usage

- VUID-VkSubpassBeginInfo-contents-09382
  If `contents` is `VK_SUBPASS_CONTENTS_INLINE_AND_SECONDARY_COMMAND_BUFFERS_KHR`, then at least one of the following features must be enabled:

  - `maintenance7`

  - `nestedCommandBuffer`

Valid Usage (Implicit)

- VUID-VkSubpassBeginInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_SUBPASS_BEGIN_INFO`

- VUID-VkSubpassBeginInfo-pNext-pNext
  `pNext` must be `NULL`

- VUID-VkSubpassBeginInfo-contents-parameter
  `contents` must be a valid VkSubpassContents value

Possible values of vkCmdBeginRenderPass::`contents`, specifying how the commands in the first subpass will be provided, are:

    // Provided by VK_VERSION_1_0
    typedef enum VkSubpassContents {
        VK_SUBPASS_CONTENTS_INLINE = 0,
        VK_SUBPASS_CONTENTS_SECONDARY_COMMAND_BUFFERS = 1,
      // Provided by VK_KHR_maintenance7
        VK_SUBPASS_CONTENTS_INLINE_AND_SECONDARY_COMMAND_BUFFERS_KHR = 1000451000,
      // Provided by VK_EXT_nested_command_buffer
        VK_SUBPASS_CONTENTS_INLINE_AND_SECONDARY_COMMAND_BUFFERS_EXT = VK_SUBPASS_CONTENTS_INLINE_AND_SECONDARY_COMMAND_BUFFERS_KHR,
    } VkSubpassContents;

- `VK_SUBPASS_CONTENTS_INLINE` specifies that the contents of the subpass will be recorded inline in the primary command buffer, and secondary command buffers must not be executed within the subpass.

- `VK_SUBPASS_CONTENTS_SECONDARY_COMMAND_BUFFERS` specifies that the contents are recorded in secondary command buffers that will be called from the primary command buffer, and vkCmdExecuteCommands is the only valid command in the command buffer until vkCmdNextSubpass or vkCmdEndRenderPass.

- `VK_SUBPASS_CONTENTS_INLINE_AND_SECONDARY_COMMAND_BUFFERS_KHR` specifies that the contents of the subpass can be recorded both inline and in secondary command buffers executed from this command buffer with vkCmdExecuteCommands.

If the `pNext` chain of VkRenderPassBeginInfo or VkRenderingInfo includes a `VkDeviceGroupRenderPassBeginInfo` structure, then that structure includes a device mask and set of render areas for the render pass instance.

The `VkDeviceGroupRenderPassBeginInfo` structure is defined as:

    // Provided by VK_VERSION_1_1
    typedef struct VkDeviceGroupRenderPassBeginInfo {
        VkStructureType    sType;
        const void*        pNext;
        uint32_t           deviceMask;
        uint32_t           deviceRenderAreaCount;
        const VkRect2D*    pDeviceRenderAreas;
    } VkDeviceGroupRenderPassBeginInfo;

or the equivalent

    // Provided by VK_KHR_device_group
    typedef VkDeviceGroupRenderPassBeginInfo VkDeviceGroupRenderPassBeginInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `deviceMask` is the device mask for the render pass instance.

- `deviceRenderAreaCount` is the number of elements in the `pDeviceRenderAreas` array.

- `pDeviceRenderAreas` is a pointer to an array of VkRect2D structures defining the render area for each physical device.

The `deviceMask` serves several purposes. It is an upper bound on the set of physical devices that can be used during the render pass instance, and the initial device mask when the render pass instance begins. In addition, commands transitioning to the next subpass in a render pass instance and commands ending the render pass instance, and, accordingly render pass load, store, and multisample resolve operations and subpass dependencies corresponding to the render pass instance, are executed on the physical devices included in the device mask provided here.

If `deviceRenderAreaCount` is not zero, then the elements of `pDeviceRenderAreas` override the value of VkRenderPassBeginInfo::`renderArea`, and provide a render area specific to each physical device. These render areas serve the same purpose as VkRenderPassBeginInfo::`renderArea`, including controlling the region of attachments that are cleared by `VK_ATTACHMENT_LOAD_OP_CLEAR` and that are resolved into resolve attachments.

If this structure is not present, the render pass instance’s device mask is the value of VkDeviceGroupCommandBufferBeginInfo::`deviceMask`. If this structure is not present or if `deviceRenderAreaCount` is zero, VkRenderPassBeginInfo::`renderArea` is used for all physical devices.

Valid Usage

- VUID-VkDeviceGroupRenderPassBeginInfo-deviceMask-00905
  `deviceMask` must be a valid device mask value

- VUID-VkDeviceGroupRenderPassBeginInfo-deviceMask-00906
  `deviceMask` must not be zero

- VUID-VkDeviceGroupRenderPassBeginInfo-deviceMask-00907
  `deviceMask` must be a subset of the command buffer’s initial device mask

- VUID-VkDeviceGroupRenderPassBeginInfo-deviceRenderAreaCount-00908
  `deviceRenderAreaCount` must either be zero or equal to the number of physical devices in the logical device

- VUID-VkDeviceGroupRenderPassBeginInfo-offset-06166
  The `offset.x` member of any element of `pDeviceRenderAreas` must be greater than or equal to 0

- VUID-VkDeviceGroupRenderPassBeginInfo-offset-06167
  The `offset.y` member of any element of `pDeviceRenderAreas` must be greater than or equal to 0

- VUID-VkDeviceGroupRenderPassBeginInfo-offset-06168
  The sum of the `offset.x` and `extent.width` members of any element of `pDeviceRenderAreas` must be less than or equal to `maxFramebufferWidth`

- VUID-VkDeviceGroupRenderPassBeginInfo-offset-06169
  The sum of the `offset.y` and `extent.height` members of any element of `pDeviceRenderAreas` must be less than or equal to `maxFramebufferHeight`

- VUID-VkDeviceGroupRenderPassBeginInfo-extent-08998
  The `extent.width` member of any element of `pDeviceRenderAreas` must be greater than 0

- VUID-VkDeviceGroupRenderPassBeginInfo-extent-08999
  The `extent.height` member of any element of `pDeviceRenderAreas` must be greater than 0

Valid Usage (Implicit)

- VUID-VkDeviceGroupRenderPassBeginInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_DEVICE_GROUP_RENDER_PASS_BEGIN_INFO`

- VUID-VkDeviceGroupRenderPassBeginInfo-pDeviceRenderAreas-parameter
  If `deviceRenderAreaCount` is not `0`, `pDeviceRenderAreas` must be a valid pointer to an array of `deviceRenderAreaCount` VkRect2D structures

The `VkRenderPassAttachmentBeginInfo` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkRenderPassAttachmentBeginInfo {
        VkStructureType       sType;
        const void*           pNext;
        uint32_t              attachmentCount;
        const VkImageView*    pAttachments;
    } VkRenderPassAttachmentBeginInfo;

or the equivalent

    // Provided by VK_KHR_imageless_framebuffer
    typedef VkRenderPassAttachmentBeginInfo VkRenderPassAttachmentBeginInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `attachmentCount` is the number of attachments.

- `pAttachments` is a pointer to an array of `VkImageView` handles, each of which will be used as the corresponding attachment in the render pass instance.

Valid Usage

- VUID-VkRenderPassAttachmentBeginInfo-pAttachments-03218
  Each element of `pAttachments` must only specify a single mip level

- VUID-VkRenderPassAttachmentBeginInfo-pAttachments-03219
  Each element of `pAttachments` must have been created with the identity swizzle

- VUID-VkRenderPassAttachmentBeginInfo-pAttachments-04114
  Each element of `pAttachments` must have been created with VkImageViewCreateInfo::`viewType` not equal to `VK_IMAGE_VIEW_TYPE_3D`

- VUID-VkRenderPassAttachmentBeginInfo-pAttachments-07010
  If multisampled-render-to-single-sampled is enabled for any subpass, all element of `pAttachments` which have a sample count equal to `VK_SAMPLE_COUNT_1_BIT` must have a format that supports the sample count specified in VkMultisampledRenderToSingleSampledInfoEXT::`rasterizationSamples`

Valid Usage (Implicit)

- VUID-VkRenderPassAttachmentBeginInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_ATTACHMENT_BEGIN_INFO`

- VUID-VkRenderPassAttachmentBeginInfo-pAttachments-parameter
  If `attachmentCount` is not `0`, `pAttachments` must be a valid pointer to an array of `attachmentCount` valid VkImageView handles

If a render pass instance enables multiview and if the `multiviewPerViewRenderAreas` feature is enabled, the `VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM` structure can be included in the `pNext` chain of VkRenderPassBeginInfo or VkRenderingInfo

The `VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM` structure is defined as:

    // Provided by VK_QCOM_multiview_per_view_render_areas
    typedef struct VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM {
        VkStructureType    sType;
        const void*        pNext;
        uint32_t           perViewRenderAreaCount;
        const VkRect2D*    pPerViewRenderAreas;
    } VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `perViewRenderAreaCount` is the number of elements in the `pPerViewRenderAreas` array.

- `pPerViewRenderAreas` is a pointer to an array of VkRect2D structures defining the render area for each view.

If `perViewRenderAreaCount` is not zero, then the elements of `pPerViewRenderAreas` override the value of VkRenderPassBeginInfo::`renderArea` or VkRenderingInfo::`renderArea` and define per-view render areas for the individual views of a multiview render pass. The render area for the view with view index `i` is specified by `pPerViewRenderAreas`[i].

The per-view render areas define per-view regions of attachments that are loaded, stored, and resolved according to the `loadOp`, `storeOp`, and `resolveMode` values of the render pass instance. When per-view render areas are defined, the value of VkRenderPassBeginInfo::`renderArea` or VkRenderingInfo::`renderArea` must be a render area that includes the union of all per-view render areas, may be used by the implementation for optimizations, but does not affect loads, stores, or resolves.

If this structure is present and if `perViewRenderAreaCount` is not zero, then `perViewRenderAreaCount` must be at least one greater than the most significant bit set in any element of VkRenderPassMultiviewCreateInfo::`pViewMasks`. or VkRenderingInfo::`viewMask`

If this structure is not present or if `perViewRenderAreaCount` is zero, VkRenderPassBeginInfo::`renderArea` or VkRenderingInfo::`renderArea` is used for all views.

Valid Usage

- VUID-VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM-offset-07861
  The `offset.x` member of any element of `pPerViewRenderAreas` must be greater than or equal to 0

- VUID-VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM-offset-07862
  The `offset.y` member of any element of `pPerViewRenderAreas` must be greater than or equal to 0

- VUID-VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM-offset-07863
  The sum of the `offset.x` and `extent.width` members of any element of `pPerViewRenderAreas` must be less than or equal to `maxFramebufferWidth`

- VUID-VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM-offset-07864
  The sum of the `offset.y` and `extent.height` members of any element of `pPerViewRenderAreas` must be less than or equal to `maxFramebufferHeight`

- VUID-VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM-pNext-07865
  If this structure is in the `pNext` chain of VkRenderPassBeginInfo and if the render pass object included an element in VkRenderPassMultiviewCreateInfo::`pViewMasks` that set bit `n`, then `perViewRenderAreaCount` must be at least equal to `n+1`

- VUID-VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM-pNext-07866
  If this structure is in the `pNext` chain of VkRenderingInfo and if VkRenderingInfo::`viewMask` set bit `n`, then `perViewRenderAreaCount` must be at least equal to `n+1`

Valid Usage (Implicit)

- VUID-VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_MULTIVIEW_PER_VIEW_RENDER_AREAS_RENDER_PASS_BEGIN_INFO_QCOM`

- VUID-VkMultiviewPerViewRenderAreasRenderPassBeginInfoQCOM-pPerViewRenderAreas-parameter
  If `perViewRenderAreaCount` is not `0`, `pPerViewRenderAreas` must be a valid pointer to an array of `perViewRenderAreaCount` VkRect2D structures

To query the render area granularity, call:

    // Provided by VK_VERSION_1_0
    void vkGetRenderAreaGranularity(
        VkDevice                                    device,
        VkRenderPass                                renderPass,
        VkExtent2D*                                 pGranularity);

- `device` is the logical device that owns the render pass.

- `renderPass` is a handle to a render pass.

- `pGranularity` is a pointer to a VkExtent2D structure in which the granularity is returned.

The conditions leading to an optimal `renderArea` are:

- the `offset.x` member in `renderArea` is a multiple of the `width` member of the returned VkExtent2D (the horizontal granularity).

- the `offset.y` member in `renderArea` is a multiple of the `height` member of the returned VkExtent2D (the vertical granularity).

- either the `extent.width` member in `renderArea` is a multiple of the horizontal granularity or `offset.x`+`extent.width` is equal to the `width` of the `framebuffer` in the VkRenderPassBeginInfo.

- either the `extent.height` member in `renderArea` is a multiple of the vertical granularity or `offset.y`+`extent.height` is equal to the `height` of the `framebuffer` in the VkRenderPassBeginInfo.

Subpass dependencies are not affected by the render area, and apply to the entire image subresources attached to the framebuffer as specified in the description of automatic layout transitions. Similarly, pipeline barriers are valid even if their effect extends outside the render area.

Valid Usage (Implicit)

- VUID-vkGetRenderAreaGranularity-device-parameter
  `device` must be a valid VkDevice handle

- VUID-vkGetRenderAreaGranularity-renderPass-parameter
  `renderPass` must be a valid VkRenderPass handle

- VUID-vkGetRenderAreaGranularity-pGranularity-parameter
  `pGranularity` must be a valid pointer to a VkExtent2D structure

- VUID-vkGetRenderAreaGranularity-renderPass-parent
  `renderPass` must have been created, allocated, or retrieved from `device`

To transition to the next subpass in the render pass instance after recording the commands for a subpass, call:

    // Provided by VK_VERSION_1_0
    void vkCmdNextSubpass(
        VkCommandBuffer                             commandBuffer,
        VkSubpassContents                           contents);

- `commandBuffer` is the command buffer in which to record the command.

- `contents` specifies how the commands in the next subpass will be provided, in the same fashion as the corresponding parameter of vkCmdBeginRenderPass.

The subpass index for a render pass begins at zero when `vkCmdBeginRenderPass` is recorded, and increments each time `vkCmdNextSubpass` is recorded.

After transitioning to the next subpass, the application can record the commands for that subpass.

Valid Usage

- VUID-vkCmdNextSubpass-None-00909
  The current subpass index must be less than the number of subpasses in the render pass minus one

- VUID-vkCmdNextSubpass-None-02349
  This command must not be recorded when transform feedback is active

Valid Usage (Implicit)

- VUID-vkCmdNextSubpass-commandBuffer-parameter
  `commandBuffer` must be a valid VkCommandBuffer handle

- VUID-vkCmdNextSubpass-contents-parameter
  `contents` must be a valid VkSubpassContents value

- VUID-vkCmdNextSubpass-commandBuffer-recording
  `commandBuffer` must be in the recording state

- VUID-vkCmdNextSubpass-commandBuffer-cmdpool
  The `VkCommandPool` that `commandBuffer` was allocated from must support graphics operations

- VUID-vkCmdNextSubpass-renderpass
  This command must only be called inside of a render pass instance

- VUID-vkCmdNextSubpass-videocoding
  This command must only be called outside of a video coding scope

- VUID-vkCmdNextSubpass-bufferlevel
  `commandBuffer` must be a primary `VkCommandBuffer`

Host Synchronization

- Host access to `commandBuffer` must be externally synchronized

- Host access to the `VkCommandPool` that `commandBuffer` was allocated from must be externally synchronized

Command Properties

Command Buffer Levels | Render Pass Scope | Video Coding Scope | Supported Queue Types | Command Type
--- | --- | --- | --- | ---
Primary | Inside | Outside | Graphics | Action State Synchronization

To transition to the next subpass in the render pass instance after recording the commands for a subpass, call:

    // Provided by VK_VERSION_1_2
    void vkCmdNextSubpass2(
        VkCommandBuffer                             commandBuffer,
        const VkSubpassBeginInfo*                   pSubpassBeginInfo,
        const VkSubpassEndInfo*                     pSubpassEndInfo);

or the equivalent command

    // Provided by VK_KHR_create_renderpass2
    void vkCmdNextSubpass2KHR(
        VkCommandBuffer                             commandBuffer,
        const VkSubpassBeginInfo*                   pSubpassBeginInfo,
        const VkSubpassEndInfo*                     pSubpassEndInfo);

- `commandBuffer` is the command buffer in which to record the command.

- `pSubpassBeginInfo` is a pointer to a VkSubpassBeginInfo structure containing information about the subpass which is about to begin rendering.

- `pSubpassEndInfo` is a pointer to a VkSubpassEndInfo structure containing information about how the previous subpass will be ended.

`vkCmdNextSubpass2` is semantically identical to vkCmdNextSubpass, except that it is extensible, and that `contents` is provided as part of an extensible structure instead of as a flat parameter.

Valid Usage

- VUID-vkCmdNextSubpass2-None-03102
  The current subpass index must be less than the number of subpasses in the render pass minus one

- VUID-vkCmdNextSubpass2-None-02350
  This command must not be recorded when transform feedback is active

Valid Usage (Implicit)

- VUID-vkCmdNextSubpass2-commandBuffer-parameter
  `commandBuffer` must be a valid VkCommandBuffer handle

- VUID-vkCmdNextSubpass2-pSubpassBeginInfo-parameter
  `pSubpassBeginInfo` must be a valid pointer to a valid VkSubpassBeginInfo structure

- VUID-vkCmdNextSubpass2-pSubpassEndInfo-parameter
  `pSubpassEndInfo` must be a valid pointer to a valid VkSubpassEndInfo structure

- VUID-vkCmdNextSubpass2-commandBuffer-recording
  `commandBuffer` must be in the recording state

- VUID-vkCmdNextSubpass2-commandBuffer-cmdpool
  The `VkCommandPool` that `commandBuffer` was allocated from must support graphics operations

- VUID-vkCmdNextSubpass2-renderpass
  This command must only be called inside of a render pass instance

- VUID-vkCmdNextSubpass2-videocoding
  This command must only be called outside of a video coding scope

- VUID-vkCmdNextSubpass2-bufferlevel
  `commandBuffer` must be a primary `VkCommandBuffer`

Host Synchronization

- Host access to `commandBuffer` must be externally synchronized

- Host access to the `VkCommandPool` that `commandBuffer` was allocated from must be externally synchronized

Command Properties

Command Buffer Levels | Render Pass Scope | Video Coding Scope | Supported Queue Types | Command Type
--- | --- | --- | --- | ---
Primary | Inside | Outside | Graphics | Action State Synchronization

To record a command to end a render pass instance after recording the commands for the last subpass, call:

    // Provided by VK_VERSION_1_0
    void vkCmdEndRenderPass(
        VkCommandBuffer                             commandBuffer);

- `commandBuffer` is the command buffer in which to end the current render pass instance.

Ending a render pass instance performs any multisample resolve operations on the final subpass.

Valid Usage

- VUID-vkCmdEndRenderPass-None-00910
  The current subpass index must be equal to the number of subpasses in the render pass minus one

- VUID-vkCmdEndRenderPass-None-02351
  This command must not be recorded when transform feedback is active

- VUID-vkCmdEndRenderPass-None-06170
  The current render pass instance must not have been begun with vkCmdBeginRendering

- VUID-vkCmdEndRenderPass-None-07004
  If `vkCmdBeginQuery`* was called within a subpass of the render pass, the corresponding `vkCmdEndQuery`* must have been called subsequently within the same subpass

Valid Usage (Implicit)

- VUID-vkCmdEndRenderPass-commandBuffer-parameter
  `commandBuffer` must be a valid VkCommandBuffer handle

- VUID-vkCmdEndRenderPass-commandBuffer-recording
  `commandBuffer` must be in the recording state

- VUID-vkCmdEndRenderPass-commandBuffer-cmdpool
  The `VkCommandPool` that `commandBuffer` was allocated from must support graphics operations

- VUID-vkCmdEndRenderPass-renderpass
  This command must only be called inside of a render pass instance

- VUID-vkCmdEndRenderPass-videocoding
  This command must only be called outside of a video coding scope

- VUID-vkCmdEndRenderPass-bufferlevel
  `commandBuffer` must be a primary `VkCommandBuffer`

Host Synchronization

- Host access to `commandBuffer` must be externally synchronized

- Host access to the `VkCommandPool` that `commandBuffer` was allocated from must be externally synchronized

Command Properties

Command Buffer Levels | Render Pass Scope | Video Coding Scope | Supported Queue Types | Command Type
--- | --- | --- | --- | ---
Primary | Inside | Outside | Graphics | Action State Synchronization

To record a command to end a render pass instance after recording the commands for the last subpass, call:

    // Provided by VK_VERSION_1_2
    void vkCmdEndRenderPass2(
        VkCommandBuffer                             commandBuffer,
        const VkSubpassEndInfo*                     pSubpassEndInfo);

or the equivalent command

    // Provided by VK_KHR_create_renderpass2
    void vkCmdEndRenderPass2KHR(
        VkCommandBuffer                             commandBuffer,
        const VkSubpassEndInfo*                     pSubpassEndInfo);

- `commandBuffer` is the command buffer in which to end the current render pass instance.

- `pSubpassEndInfo` is a pointer to a VkSubpassEndInfo structure containing information about how the last subpass will be ended.

`vkCmdEndRenderPass2` is semantically identical to vkCmdEndRenderPass, except that it is extensible.

Valid Usage

- VUID-vkCmdEndRenderPass2-None-03103
  The current subpass index must be equal to the number of subpasses in the render pass minus one

- VUID-vkCmdEndRenderPass2-None-02352
  This command must not be recorded when transform feedback is active

- VUID-vkCmdEndRenderPass2-None-06171
  The current render pass instance must not have been begun with vkCmdBeginRendering

- VUID-vkCmdEndRenderPass2-None-07005
  If `vkCmdBeginQuery`* was called within a subpass of the render pass, the corresponding `vkCmdEndQuery`* must have been called subsequently within the same subpass

Valid Usage (Implicit)

- VUID-vkCmdEndRenderPass2-commandBuffer-parameter
  `commandBuffer` must be a valid VkCommandBuffer handle

- VUID-vkCmdEndRenderPass2-pSubpassEndInfo-parameter
  `pSubpassEndInfo` must be a valid pointer to a valid VkSubpassEndInfo structure

- VUID-vkCmdEndRenderPass2-commandBuffer-recording
  `commandBuffer` must be in the recording state

- VUID-vkCmdEndRenderPass2-commandBuffer-cmdpool
  The `VkCommandPool` that `commandBuffer` was allocated from must support graphics operations

- VUID-vkCmdEndRenderPass2-renderpass
  This command must only be called inside of a render pass instance

- VUID-vkCmdEndRenderPass2-videocoding
  This command must only be called outside of a video coding scope

- VUID-vkCmdEndRenderPass2-bufferlevel
  `commandBuffer` must be a primary `VkCommandBuffer`

Host Synchronization

- Host access to `commandBuffer` must be externally synchronized

- Host access to the `VkCommandPool` that `commandBuffer` was allocated from must be externally synchronized

Command Properties

Command Buffer Levels | Render Pass Scope | Video Coding Scope | Supported Queue Types | Command Type
--- | --- | --- | --- | ---
Primary | Inside | Outside | Graphics | Action State Synchronization

The `VkSubpassEndInfo` structure is defined as:

    // Provided by VK_VERSION_1_2
    typedef struct VkSubpassEndInfo {
        VkStructureType    sType;
        const void*        pNext;
    } VkSubpassEndInfo;

or the equivalent

    // Provided by VK_KHR_create_renderpass2
    typedef VkSubpassEndInfo VkSubpassEndInfoKHR;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

Valid Usage (Implicit)

- VUID-VkSubpassEndInfo-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_SUBPASS_END_INFO`

- VUID-VkSubpassEndInfo-pNext-pNext
  `pNext` must be `NULL` or a pointer to a valid instance of VkSubpassFragmentDensityMapOffsetEndInfoQCOM

- VUID-VkSubpassEndInfo-sType-unique
  The `sType` value of each struct in the `pNext` chain must be unique

If the VkSubpassEndInfo::`pNext` chain includes a `VkSubpassFragmentDensityMapOffsetEndInfoQCOM` structure, then that structure includes an array of fragment density map offsets per layer for the render pass.

The `VkSubpassFragmentDensityMapOffsetEndInfoQCOM` structure is defined as:

    // Provided by VK_QCOM_fragment_density_map_offset
    typedef struct VkSubpassFragmentDensityMapOffsetEndInfoQCOM {
        VkStructureType      sType;
        const void*          pNext;
        uint32_t             fragmentDensityOffsetCount;
        const VkOffset2D*    pFragmentDensityOffsets;
    } VkSubpassFragmentDensityMapOffsetEndInfoQCOM;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `fragmentDensityOffsetCount` is the number of offsets being specified.

- `pFragmentDensityOffsets` is a pointer to an array of VkOffset2D structs, each of which describes the offset per layer.

The array elements are given per `layer` as defined by Fetch Density Value, where index = layer. Each (x,y) offset is in framebuffer pixels and shifts the fetch of the fragment density map by that amount. Offsets can be positive or negative.

Offset values specified for any subpass that is not the last subpass in the render pass are ignored. If the VkSubpassEndInfo::`pNext` chain for the last subpass of a render pass does not include `VkSubpassFragmentDensityMapOffsetEndInfoQCOM`, or if `fragmentDensityOffsetCount` is zero, then the offset (0,0) is used for Fetch Density Value.

Valid Usage

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-fragmentDensityMapOffsets-06503
  If the `fragmentDensityMapOffset` feature is not enabled or fragment density map is not enabled in the render pass, `fragmentDensityOffsetCount` must equal `0`

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-fragmentDensityMapAttachment-06504
  If `VkSubpassDescription`::`fragmentDensityMapAttachment` is not is not `VK_ATTACHMENT_UNUSED` and was not created with `VK_IMAGE_CREATE_FRAGMENT_DENSITY_MAP_OFFSET_BIT_QCOM`, `fragmentDensityOffsetCount` must equal `0`

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-pDepthStencilAttachment-06505
  If `VkSubpassDescription`::`pDepthStencilAttachment` is not is not `VK_ATTACHMENT_UNUSED` and was not created with `VK_IMAGE_CREATE_FRAGMENT_DENSITY_MAP_OFFSET_BIT_QCOM`, `fragmentDensityOffsetCount` must equal `0`

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-pInputAttachments-06506
  If any element of `VkSubpassDescription`::`pInputAttachments` is not is not `VK_ATTACHMENT_UNUSED` and was not created with `VK_IMAGE_CREATE_FRAGMENT_DENSITY_MAP_OFFSET_BIT_QCOM`, `fragmentDensityOffsetCount` must equal `0`

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-pColorAttachments-06507
  If any element of `VkSubpassDescription`::`pColorAttachments` is not is not `VK_ATTACHMENT_UNUSED` and was not created with `VK_IMAGE_CREATE_FRAGMENT_DENSITY_MAP_OFFSET_BIT_QCOM`, `fragmentDensityOffsetCount` must equal `0`

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-pResolveAttachments-06508
  If any element of `VkSubpassDescription`::`pResolveAttachments` is not is not `VK_ATTACHMENT_UNUSED` and was not created with `VK_IMAGE_CREATE_FRAGMENT_DENSITY_MAP_OFFSET_BIT_QCOM`, `fragmentDensityOffsetCount` must equal `0`

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-pPreserveAttachments-06509
  If any element of `VkSubpassDescription`::`pPreserveAttachments` is not is not `VK_ATTACHMENT_UNUSED` and was not created with `VK_IMAGE_CREATE_FRAGMENT_DENSITY_MAP_OFFSET_BIT_QCOM`, `fragmentDensityOffsetCount` must equal `0`

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-fragmentDensityOffsetCount-06510
  If `fragmentDensityOffsetCount` is not `0` and multiview is enabled for the render pass, `fragmentDensityOffsetCount` must equal the `layerCount` that was specified in creating the fragment density map attachment view

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-fragmentDensityOffsetCount-06511
  If `fragmentDensityOffsetCount` is not `0` and multiview is not enabled for the render pass, `fragmentDensityOffsetCount` must equal `1`

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-x-06512
  The `x` component of each element of `pFragmentDensityOffsets` must be an integer multiple of `fragmentDensityOffsetGranularity.width`

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-y-06513
  The `y` component of each element of `pFragmentDensityOffsets` must be an integer multiple of `fragmentDensityOffsetGranularity.height`

Valid Usage (Implicit)

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_SUBPASS_FRAGMENT_DENSITY_MAP_OFFSET_END_INFO_QCOM`

- VUID-VkSubpassFragmentDensityMapOffsetEndInfoQCOM-pFragmentDensityOffsets-parameter
  If `fragmentDensityOffsetCount` is not `0`, `pFragmentDensityOffsets` must be a valid pointer to an array of `fragmentDensityOffsetCount` VkOffset2D structures

### 8.9. Render Pass Creation Feedback

A `VkRenderPassCreationControlEXT` structure can be included in the `pNext` chain of `VkRenderPassCreateInfo2` or `pNext` chain of VkSubpassDescription2. The `VkRenderPassCreationControlEXT` structure is defined as:

    // Provided by VK_EXT_subpass_merge_feedback
    typedef struct VkRenderPassCreationControlEXT {
        VkStructureType    sType;
        const void*        pNext;
        VkBool32           disallowMerging;
    } VkRenderPassCreationControlEXT;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `disallowMerging` is a boolean value indicating whether subpass merging will be disabled.

If a `VkRenderPassCreationControlEXT` structure is included in the `pNext` chain of VkRenderPassCreateInfo2 and its value of `disallowMerging` is `VK_TRUE`, the implementation will disable subpass merging for the entire render pass. If a `VkRenderPassCreationControlEXT` structure is included in the `pNext` chain of VkSubpassDescription2 and its value of `disallowMerging` is `VK_TRUE`, the implementation will disable merging the described subpass with previous subpasses in the render pass.

Valid Usage (Implicit)

- VUID-VkRenderPassCreationControlEXT-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_CREATION_CONTROL_EXT`

To obtain feedback about the creation of a render pass, include a `VkRenderPassCreationFeedbackCreateInfoEXT` structure in the `pNext` chain of VkRenderPassCreateInfo2. The `VkRenderPassCreationFeedbackCreateInfoEXT` structure is defined as:

    // Provided by VK_EXT_subpass_merge_feedback
    typedef struct VkRenderPassCreationFeedbackCreateInfoEXT {
        VkStructureType                         sType;
        const void*                             pNext;
        VkRenderPassCreationFeedbackInfoEXT*    pRenderPassFeedback;
    } VkRenderPassCreationFeedbackCreateInfoEXT;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `pRenderPassFeedback` is a pointer to a VkRenderPassCreationFeedbackInfoEXT structure in which feedback is returned.

Valid Usage (Implicit)

- VUID-VkRenderPassCreationFeedbackCreateInfoEXT-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_CREATION_FEEDBACK_CREATE_INFO_EXT`

- VUID-VkRenderPassCreationFeedbackCreateInfoEXT-pRenderPassFeedback-parameter
  `pRenderPassFeedback` must be a valid pointer to a VkRenderPassCreationFeedbackInfoEXT structure

The `VkRenderPassCreationFeedbackInfoEXT` structure is defined as:

    // Provided by VK_EXT_subpass_merge_feedback
    typedef struct VkRenderPassCreationFeedbackInfoEXT {
        uint32_t    postMergeSubpassCount;
    } VkRenderPassCreationFeedbackInfoEXT;

- `postMergeSubpassCount` is the subpass count after merge.

Feedback about the creation of a subpass can be obtained by including a `VkRenderPassSubpassFeedbackCreateInfoEXT` structure in the `pNext` chain of VkSubpassDescription2. `VkRenderPassSubpassFeedbackCreateInfoEXT` structure is defined as:

    // Provided by VK_EXT_subpass_merge_feedback
    typedef struct VkRenderPassSubpassFeedbackCreateInfoEXT {
        VkStructureType                        sType;
        const void*                            pNext;
        VkRenderPassSubpassFeedbackInfoEXT*    pSubpassFeedback;
    } VkRenderPassSubpassFeedbackCreateInfoEXT;

- `sType` is a VkStructureType value identifying this structure.

- `pNext` is `NULL` or a pointer to a structure extending this structure.

- `pSubpassFeedback` is a pointer to a VkRenderPassSubpassFeedbackInfoEXT structure in which feedback is returned.

Valid Usage (Implicit)

- VUID-VkRenderPassSubpassFeedbackCreateInfoEXT-sType-sType
  `sType` must be `VK_STRUCTURE_TYPE_RENDER_PASS_SUBPASS_FEEDBACK_CREATE_INFO_EXT`

- VUID-VkRenderPassSubpassFeedbackCreateInfoEXT-pSubpassFeedback-parameter
  `pSubpassFeedback` must be a valid pointer to a VkRenderPassSubpassFeedbackInfoEXT structure

The `VkRenderPassSubpassFeedbackInfoEXT` structure is defined as:

    // Provided by VK_EXT_subpass_merge_feedback
    typedef struct VkRenderPassSubpassFeedbackInfoEXT {
        VkSubpassMergeStatusEXT    subpassMergeStatus;
        char                       description[VK_MAX_DESCRIPTION_SIZE];
        uint32_t                   postMergeIndex;
    } VkRenderPassSubpassFeedbackInfoEXT;

- `subpassMergeStatus` is a `VkSubpassMergeStatusEXT` value specifying information about whether the subpass is merged with the previous subpass and the reason why it is not merged.

- `description` is an array of `VK_MAX_DESCRIPTION_SIZE` `char` containing a null-terminated UTF-8 string which provides additional details.

- `postMergeIndex` is the subpass index after the subpass merging.

Possible values of `VkRenderPassSubpassFeedbackInfoEXT`:subpassMergeStatus are:

    // Provided by VK_EXT_subpass_merge_feedback
    typedef enum VkSubpassMergeStatusEXT {
        VK_SUBPASS_MERGE_STATUS_MERGED_EXT = 0,
        VK_SUBPASS_MERGE_STATUS_DISALLOWED_EXT = 1,
        VK_SUBPASS_MERGE_STATUS_NOT_MERGED_SIDE_EFFECTS_EXT = 2,
        VK_SUBPASS_MERGE_STATUS_NOT_MERGED_SAMPLES_MISMATCH_EXT = 3,
        VK_SUBPASS_MERGE_STATUS_NOT_MERGED_VIEWS_MISMATCH_EXT = 4,
        VK_SUBPASS_MERGE_STATUS_NOT_MERGED_ALIASING_EXT = 5,
        VK_SUBPASS_MERGE_STATUS_NOT_MERGED_DEPENDENCIES_EXT = 6,
        VK_SUBPASS_MERGE_STATUS_NOT_MERGED_INCOMPATIBLE_INPUT_ATTACHMENT_EXT = 7,
        VK_SUBPASS_MERGE_STATUS_NOT_MERGED_TOO_MANY_ATTACHMENTS_EXT = 8,
        VK_SUBPASS_MERGE_STATUS_NOT_MERGED_INSUFFICIENT_STORAGE_EXT = 9,
        VK_SUBPASS_MERGE_STATUS_NOT_MERGED_DEPTH_STENCIL_COUNT_EXT = 10,
        VK_SUBPASS_MERGE_STATUS_NOT_MERGED_RESOLVE_ATTACHMENT_REUSE_EXT = 11,
        VK_SUBPASS_MERGE_STATUS_NOT_MERGED_SINGLE_SUBPASS_EXT = 12,
        VK_SUBPASS_MERGE_STATUS_NOT_MERGED_UNSPECIFIED_EXT = 13,
    } VkSubpassMergeStatusEXT;

- `VK_SUBPASS_MERGE_STATUS_MERGED_EXT` specifies that the subpass is merged with a previous subpass.

- `VK_SUBPASS_MERGE_STATUS_DISALLOWED_EXT` specifies that the subpass is not merged because merging was disabled using VkRenderPassCreationControlEXT. If the render pass does not allow subpass merging, then all subpass statuses are set to this value. If a subpass description does not allow subpass merging, then only that subpass’s status is set to this value.

- `VK_SUBPASS_MERGE_STATUS_NOT_MERGED_SIDE_EFFECTS_EXT` specifies that the subpass is not merged because it contains side effects.

- `VK_SUBPASS_MERGE_STATUS_NOT_MERGED_SAMPLES_MISMATCH_EXT` specifies that the subpass is not merged because sample count is not compatible with the previous subpass.

- `VK_SUBPASS_MERGE_STATUS_NOT_MERGED_VIEWS_MISMATCH_EXT` specifies that the subpass is not merged because view masks do not match with previous subpass.

- `VK_SUBPASS_MERGE_STATUS_NOT_MERGED_ALIASING_EXT` specifies that the subpass is not merged because of attachments aliasing between them.

- `VK_SUBPASS_MERGE_STATUS_NOT_MERGED_DEPENDENCIES_EXT` specifies that the subpass is not merged because subpass dependencies do not allow merging.

- `VK_SUBPASS_MERGE_STATUS_NOT_MERGED_INCOMPATIBLE_INPUT_ATTACHMENT_EXT` specifies that the subpass is not merged because input attachment is not a color attachment from previous subpass or the formats are incompatible.

- `VK_SUBPASS_MERGE_STATUS_NOT_MERGED_TOO_MANY_ATTACHMENTS_EXT` specifies that the subpass is not merged because of too many attachments.

- `VK_SUBPASS_MERGE_STATUS_NOT_MERGED_INSUFFICIENT_STORAGE_EXT` specifies that the subpass is not merged because of insufficient memory.

- `VK_SUBPASS_MERGE_STATUS_NOT_MERGED_DEPTH_STENCIL_COUNT_EXT` specifies that the subpass is not merged because of too many depth/stencil attachments.

- `VK_SUBPASS_MERGE_STATUS_NOT_MERGED_RESOLVE_ATTACHMENT_REUSE_EXT` specifies that the subpass is not merged because a resolve attachment is reused as an input attachment in a subsequent subpass.

- `VK_SUBPASS_MERGE_STATUS_NOT_MERGED_SINGLE_SUBPASS_EXT` specifies that the subpass is not merged because the render pass has only one subpass.

- `VK_SUBPASS_MERGE_STATUS_NOT_MERGED_UNSPECIFIED_EXT` specifies that the subpass is not merged for unspecified reasons. Implementations should return this value when no other `VkSubpassMergeStatusEXT` value is appropriate.

### 8.10. Common Render Pass Data Races (Informative)

Due to the complexity of how rendering is performed, there are several ways an application can accidentally introduce a data race, usually by doing something that may seem benign but actually cannot be supported. This section indicates a number of the more common cases as guidelines to help avoid them.

#### 8.10.1. Sampling From a Read-Only Attachment

Vulkan includes read-only layouts for depth/stencil images, that allow the images to be both read during a render pass for the purposes of depth/stencil tests, and read as a non-attachment.

However, because `VK_ATTACHMENT_STORE_OP_STORE` and `VK_ATTACHMENT_STORE_OP_DONT_CARE` may perform write operations, even if no recorded command writes to an attachment, reading from an image while also using it as an attachment with these store operations can result in a data race. If the reads from the non-attachment are performed in a fragment shader where the accessed samples match those covered by the fragment shader, no data race will occur as store operations are guaranteed to operate after fragment shader execution for the set of samples the fragment covers. Notably, input attachments can also be used for this case. Reading other samples or in any other shader stage can result in unexpected behavior due to the potential for a data race, and validation errors should be generated for doing so. In practice, many applications have shipped reading samples outside of the covered fragment without any observable issue, but there is no guarantee that this will always work, and it is not advisable to rely on this in new or re-worked code bases. As `VK_ATTACHMENT_STORE_OP_NONE` is guaranteed to perform no writes, applications wishing to read an image as both an attachment and a non-attachment should make use of this store operation, coupled with a load operation that also performs no writes.

#### 8.10.2. Non-Overlapping Access Between Resources

When relying on non-overlapping accesses between attachments and other resources, it is important to note that load and store operations have fairly wide alignment requirements - potentially affecting entire subresources and adjacent depth/stencil aspects. This makes it invalid to access a non-attachment subresource that is simultaneously being used as an attachment where either access performs a write operation.

The only exception to this is if a subresource is in the `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT` image layout, in which case the overlap is defined to occur at a per-pixel granularity, and applications can read data from pixels outside the render area without introducing a data race.

#### 8.10.3. Depth/Stencil and Input Attachments

When rendering to only the depth OR stencil aspect of an image, an input attachment accessing the other aspect will not cause a data race only under very specific conditions. To avoid a data race, the aspect not being written must be in a read-only layout, and writes to it must be disabled in the draw state. For example, to read from stencil while writing depth, the attachment must be in `VK_IMAGE_LAYOUT_DEPTH_ATTACHMENT_STENCIL_READ_ONLY_OPTIMAL` (or equivalent), and the stencil write mask must be 0. Similarly to read from depth while writing stencil, the attachment must be in `VK_IMAGE_LAYOUT_DEPTH_READ_ONLY_STENCIL_ATTACHMENT_OPTIMAL` (or equivalent), and depth write enable must be `VK_FALSE`.

#### 8.10.4. Synchronization Options

There are several synchronization options available to synchronize between accesses to resources within a render pass. Some of the options are outlined below:

- A VkSubpassDependency in a render pass object can synchronize attachment writes and multisample resolve operations from a prior subpass for subsequent input attachment reads.

- A vkCmdPipelineBarrier inside a subpass can synchronize prior attachment writes in the subpass with subsequent input attachment reads.

- A vkCmdPipelineBarrier inside a subpass can synchronize prior attachment writes in the subpass with subsequent non-attachment reads if the attachment is in the `VK_IMAGE_LAYOUT_ATTACHMENT_FEEDBACK_LOOP_OPTIMAL_EXT` image layout.

- If a subresource is used as a color and input attachment, and the pipeline performing the read was created with `VK_PIPELINE_COLOR_BLEND_STATE_CREATE_RASTERIZATION_ORDER_ATTACHMENT_ACCESS_BIT_EXT`

- If a subresource is used as a depth and input attachment, and the pipeline performing the read was created with `VK_PIPELINE_DEPTH_STENCIL_STATE_CREATE_RASTERIZATION_ORDER_ATTACHMENT_DEPTH_ACCESS_BIT_EXT`

- If a subresource is used as a stencil and input attachment, and the pipeline performing the read was created with `VK_PIPELINE_DEPTH_STENCIL_STATE_CREATE_RASTERIZATION_ORDER_ATTACHMENT_STENCIL_ACCESS_BIT_EXT`

- If a subresource is used as two separate non-attachment resources, writes to a pixel or individual sample in a fragment shader can be synchronized with access to the same pixel or sample in another fragment shader by using one of the fragment interlock execution modes.